;/****************************************************************************
; * Copyright 2009 Atheros Communications Inc., all rights reserved.          *
; *                                                                           *
; * Copyright (c) 2011 Qualcomm Atheros, Inc.                                 *
; * All Rights Reserved.                                                      *
; * Qualcomm Atheros Confidential and Proprietary.                            *
; *                                                                           *
; * INF file for Atheros reference designs                                    *
; ****************************************************************************/

[version]
Signature   = "$Windows NT$"
Class       = Net
ClassGUID   = {4d36e972-e325-11ce-bfc1-08002be10318}
Provider    = %ATHEROS%
CatalogFile = athw10x.cat
DriverVer   = 07/14/2015,10.0.0.324

[Manufacturer]
%ATHEROS%     = Atheros, NTamd64.6.2
%GIGABYTE%    = Gigabyte, NTamd64.6.2

[ControlFlags]
ExcludeFromSelect = *
;
; OS 6.2 Manufacturer section
;
[Atheros.NTamd64.6.2]
; DisplayName               Section                 DeviceID
; -----------               -------                 --------
;legacy HW Entries
%ATHR.DeviceDesc.001B%     = ATHR_DEV_OS61_2062.ndi,     PCI\VEN_168C&DEV_FF19
%ATHR.DeviceDesc.ospsim%   = ATHR_DEV_OS61_OSPEMU.ndi,   PCI\VEN_168C&DEV_FE30
%ATHR.DeviceDesc.938x%     = ATHR_DEV_OS61_938x.ndi,     PCI\VEN_168C&DEV_ABCD
%ATHR.DeviceDesc.osprey%   = ATHR_DEV_OS61_OSPREY.ndi,   PCI\VEN_168C&DEV_0030
%ATHR.DeviceDesc.9580%     = ATHR_DEV_OS61_9580.ndi,     PCI\VEN_168C&DEV_0033
%ATHR.DeviceDesc.9485%     = ATHR_DEV_OS61_9485.ndi,     PCI\VEN_168C&DEV_0032&SUBSYS_3118168C
%ATHR.DeviceDesc.9485%     = ATHR_DEV_OS61_312F168C.ndi, PCI\VEN_168C&DEV_0032&SUBSYS_312F168C
%ATHR.DeviceDesc.1111%     = ATHR_DEV_OS61_1111.ndi,     PCI\VEN_168C&DEV_0037&SUBSYS_3118168C
%ATHR.DeviceDesc.3119%     = ATHR_DEV_OS61_3119.ndi,     PCI\VEN_168C&DEV_0032&SUBSYS_3119168C
%ATHR.DeviceDesc.3119%     = ATHR_DEV_OS61_3119.ndi,     PCI\VEN_168C&DEV_0032&SUBSYS_3122168C
%ATHR.DeviceDesc.938x%     = ATHR_DEV_OS61_938x.ndi,     PCI\VEN_168C&DEV_0030&SUBSYS_3112168C
%ATHR.DeviceDesc.938x%     = ATHR_DEV_OS61_938x.ndi,     PCI\VEN_168C&DEV_0030&SUBSYS_3113168C
%ATHR.DeviceDesc.938x%     = ATHR_DEV_OS61_938x.ndi,     PCI\VEN_168C&DEV_0030&SUBSYS_3114168C
%ATHR.DeviceDesc.938x%     = ATHR_DEV_OS61_938x.ndi,     PCI\VEN_168C&DEV_0030&SUBSYS_3116168C
%ATHR.DeviceDesc.938x%     = ATHR_DEV_OS61_938x.ndi,     PCI\VEN_168C&DEV_ABCD&SUBSYS_00000000
%ATHR.DeviceDesc.946x%     = ATHR_DEV_OS61_946x.ndi,     PCI\VEN_168C&DEV_0034&SUBSYS_3117168C
%ATHR.DeviceDesc.956x%     = ATHR_DEV_OS61_956x.ndi,     PCI\VEN_168C&DEV_0036&SUBSYS_3025168C
%ATHR.DeviceDesc.956x%     = ATHR_DEV_OS61_956x.ndi,     PCI\VEN_168C&DEV_0036&SUBSYS_3026168C
%ATHR.DeviceDesc.956x%     = ATHR_DEV_OS61_3027168C.ndi,     PCI\VEN_168C&DEV_0036&SUBSYS_3027168C
%ATHR.DeviceDesc.956x%     = ATHR_DEV_OS61_3028.ndi,     PCI\VEN_168C&DEV_0036&SUBSYS_3028168C
%ATHR.DeviceDesc.956x%     = ATHR_DEV_OS61_956x.ndi,     PCI\VEN_168C&DEV_0036&SUBSYS_302B168C
%ATHR.DeviceDesc.956x%     = ATHR_DEV_OS61_3027168C.ndi,     PCI\VEN_168C&DEV_0036&SUBSYS_302C168C
%ATHR.DeviceDesc.1030%     = ATHR_DEV_OS61_1030.ndi,     PCI\VEN_168C&DEV_0013&SUBSYS_1030168C
%ATHR.DeviceDesc.2030%     = ATHR_DEV_OS61_2030.ndi,     PCI\VEN_168C&DEV_0013&SUBSYS_2030168C
%ATHR.DeviceDesc.1031%     = ATHR_DEV_OS61_1031.ndi,     PCI\VEN_168C&DEV_0013&SUBSYS_1031168C
%ATHR.DeviceDesc.2031%     = ATHR_DEV_OS61_2031.ndi,     PCI\VEN_168C&DEV_0013&SUBSYS_2031168C
%ATHR.DeviceDesc.1041%     = ATHR_DEV_OS61_1041.ndi,     PCI\VEN_168C&DEV_0013&SUBSYS_1041168C
%ATHR.DeviceDesc.2041%     = ATHR_DEV_OS61_2041.ndi,     PCI\VEN_168C&DEV_0013&SUBSYS_2041168C
%ATHR.DeviceDesc.1042%     = ATHR_DEV_OS61_1042.ndi,     PCI\VEN_168C&DEV_0013&SUBSYS_1042168C
%ATHR.DeviceDesc.2042%     = ATHR_DEV_OS61_2042.ndi,     PCI\VEN_168C&DEV_0013&SUBSYS_2042168C
%ATHR.DeviceDesc.1051%     = ATHR_DEV_OS61_1051.ndi,     PCI\VEN_168C&DEV_0013&SUBSYS_1051168C
%ATHR.DeviceDesc.2051%     = ATHR_DEV_OS61_2051.ndi,     PCI\VEN_168C&DEV_0013&SUBSYS_2051168C
%ATHR.DeviceDesc.001A%     = ATHR_DEV_OS61_1052.ndi,     PCI\VEN_168C&DEV_001A&SUBSYS_1052168C
%ATHR.DeviceDesc.001A%     = ATHR_DEV_OS61_2052.ndi,     PCI\VEN_168C&DEV_001A&SUBSYS_2052168C
%ATHR.DeviceDesc.1053%     = ATHR_DEV_OS61_1053.ndi,     PCI\VEN_168C&DEV_0013&SUBSYS_1053168C
%ATHR.DeviceDesc.2053%     = ATHR_DEV_OS61_2053.ndi,     PCI\VEN_168C&DEV_0013&SUBSYS_2053168C
%ATHR.DeviceDesc.001A%     = ATHR_DEV_OS61_1054.ndi,     PCI\VEN_168C&DEV_001A&SUBSYS_1054168C
%ATHR.DeviceDesc.001A%     = ATHR_DEV_OS61_2054.ndi,     PCI\VEN_168C&DEV_001A&SUBSYS_2054168C
%ATHR.DeviceDesc.1062%     = ATHR_DEV_OS61_1062.ndi,     PCI\VEN_168C&DEV_001B&SUBSYS_1062168C
%ATHR.DeviceDesc.2062%     = ATHR_DEV_OS61_2062.ndi,     PCI\VEN_168C&DEV_001B&SUBSYS_2062168C
%ATHR.DeviceDesc.001B%     = ATHR_DEV_OS61_1063.ndi,     PCI\VEN_168C&DEV_001B&SUBSYS_1063168C
%ATHR.DeviceDesc.001B%     = ATHR_DEV_OS61_2063.ndi,     PCI\VEN_168C&DEV_001B&SUBSYS_2063168C
%ATHR.DeviceDesc.3062%     = ATHR_DEV_OS61_2062.ndi,     PCI\VEN_168C&DEV_001C&SUBSYS_3062168C
%ATHR.DeviceDesc.3063%     = ATHR_DEV_OS61_2063.ndi,     PCI\VEN_168C&DEV_001C&SUBSYS_3063168C
%ATHR.DeviceDesc.3061%     = ATHR_DEV_OS61_2051.ndi,     PCI\VEN_168C&DEV_001C&SUBSYS_3061168C
%ATHR.DeviceDesc.3065%     = ATHR_DEV_OS61_2052.ndi,     PCI\VEN_168C&DEV_001C&SUBSYS_3065168C
%ATHR.DeviceDesc.2061%     = ATHR_DEV_OS61_2051.ndi,     PCI\VEN_168C&DEV_001B&SUBSYS_2061168C
%ATHR.DeviceDesc.1061%     = ATHR_DEV_OS61_1051.ndi,     PCI\VEN_168C&DEV_001B&SUBSYS_1061168C
%ATHR.DeviceDesc.2065%     = ATHR_DEV_OS61_2052.ndi,     PCI\VEN_168C&DEV_001B&SUBSYS_2065168C
%ATHR.DeviceDesc.1065%     = ATHR_DEV_OS61_1052.ndi,     PCI\VEN_168C&DEV_001B&SUBSYS_1065168C
%ATHR.DeviceDesc.3067%     = ATHR_DEV_OS61_001C.ndi,     PCI\VEN_168C&DEV_001C&SUBSYS_3067168C
%ATHR.DeviceDesc.3067%     = ATHR_DEV_OS61_3064.ndi,     PCI\VEN_168C&DEV_001C&SUBSYS_3064168C
%ATHR.DeviceDesc.2055%     = ATHR_DEV_OS61_2055.ndi,     PCI\VEN_168C&DEV_001D&SUBSYS_2055168C
%ATHR.DeviceDesc.2055%     = ATHR_DEV_OS61_1055.ndi,     PCI\VEN_168C&DEV_001D&SUBSYS_1055168C
%ATHR.DeviceDesc.0013%     = ATHR_DEV_OS61_0013.ndi,     PCI\VEN_168C&DEV_0013&SUBSYS_1025168C
%ATHR.DeviceDesc.0013%     = ATHR_DEV_OS61_0013.ndi,     PCI\VEN_168C&DEV_0013&SUBSYS_1026168C
%ATHR.DeviceDesc.0013%     = ATHR_DEV_OS61_0013.ndi,     PCI\VEN_168C&DEV_0013&SUBSYS_2026168C
%ATHR.DeviceDesc.1071%     = ATHR_DEV_OS61_1071.ndi,     PCI\VEN_168C&DEV_0023&SUBSYS_1071168C
%ATHR.DeviceDesc.1071%     = ATHR_DEV_OS61_1071.ndi,     PCI\VEN_168C&DEV_0023&SUBSYS_2071168C
%ATHR.DeviceDesc.3072%     = ATHR_DEV_OS61_3072.ndi,     PCI\VEN_168C&DEV_0023&SUBSYS_1072168C
%ATHR.DeviceDesc.3072%     = ATHR_DEV_OS61_3072.ndi,     PCI\VEN_168C&DEV_0023&SUBSYS_2072168C
%ATHR.DeviceDesc.3072%     = ATHR_DEV_OS61_3072.ndi,     PCI\VEN_168C&DEV_0024&SUBSYS_3072168C
%ATHR.DeviceDesc.3091%     = ATHR_DEV_OS61_3091.ndi,     PCI\VEN_168C&DEV_002A&SUBSYS_3091168C
%ATHR.DeviceDesc.3091%     = ATHR_DEV_OS61_3091.ndi,     PCI\VEN_168C&DEV_002A&SUBSYS_3092168C
%ATHR.DeviceDesc.3091%     = ATHR_DEV_OS61_3091.ndi,     PCI\VEN_168C&DEV_002A&SUBSYS_3093168C
%ATHR.DeviceDesc.3091%     = ATHR_DEV_OS61_3091.ndi,     PCI\VEN_168C&DEV_002A&SUBSYS_3094168C
%ATHR.DeviceDesc.3091%     = ATHR_DEV_OS61_3091.ndi,     PCI\VEN_168C&DEV_002A&SUBSYS_3095168C
%ATHR.DeviceDesc.3091%     = ATHR_DEV_OS61_3091.ndi,     PCI\VEN_168C&DEV_002A&SUBSYS_3096168C
%ATHR.DeviceDesc.3091%     = ATHR_DEV_OS61_3091.ndi,     PCI\VEN_168C&DEV_002A&SUBSYS_3097168C
%ATHR.DeviceDesc.3091%     = ATHR_DEV_OS61_3091.ndi,     PCI\VEN_168C&DEV_002A&SUBSYS_3098168C
%ATHR.DeviceDesc.3091%     = ATHR_DEV_OS61_3091.ndi,     PCI\VEN_168C&DEV_002A&SUBSYS_3099168C
%ATHR.DeviceDesc.3091%     = ATHR_DEV_OS61_3091.ndi,     PCI\VEN_168C&DEV_002A&SUBSYS_309A168C
%ATHR.DeviceDesc.3091%     = ATHR_DEV_OS61_3091.ndi,     PCI\VEN_168C&DEV_002A&SUBSYS_309B168C
%ATHR.DeviceDesc.3091%     = ATHR_DEV_OS61_3091.ndi,     PCI\VEN_168C&DEV_002A&SUBSYS_309C168C
%ATHR.DeviceDesc.3091%     = ATHR_DEV_OS61_309D168C.ndi, PCI\VEN_168C&DEV_002A&SUBSYS_309D168C
%ATHR.DeviceDesc.3091%     = ATHR_DEV_OS61_3091.ndi,     PCI\VEN_168C&DEV_002A&SUBSYS_309F168C
%ATHR.DeviceDesc.2091%     = ATHR_DEV_OS61_3091.ndi,     PCI\VEN_168C&DEV_0029&SUBSYS_2091168C
%ATHR.DeviceDesc.2091%     = ATHR_DEV_OS61_3091.ndi,     PCI\VEN_168C&DEV_0029&SUBSYS_2092168C
%ATHR.DeviceDesc.2091%     = ATHR_DEV_OS61_3091PB.ndi,   PCI\VEN_168C&DEV_0029&SUBSYS_2093168C
%ATHR.DeviceDesc.2091%     = ATHR_DEV_OS61_3091.ndi,     PCI\VEN_168C&DEV_0029&SUBSYS_2094168C
%ATHR.DeviceDesc.2091%     = ATHR_DEV_OS61_3091.ndi,     PCI\VEN_168C&DEV_0029&SUBSYS_2096168C
%ATHR.DeviceDesc.2091%     = ATHR_DEV_OS61_3091.ndi,     PCI\VEN_168C&DEV_0029&SUBSYS_2098168C
%ATHR.DeviceDesc.30A1%     = ATHR_DEV_OS61_30A1.ndi,     PCI\VEN_168C&DEV_002B&SUBSYS_30A1168C
%ATHR.DeviceDesc.30A1%     = ATHR_DEV_OS61_30A1.ndi,     PCI\VEN_168C&DEV_002B&SUBSYS_30A2168C
%ATHR.DeviceDesc.30AB%     = ATHR_DEV_OS61_30AB.ndi,     PCI\VEN_168C&DEV_002B&SUBSYS_30AB168C
%ATHR.DeviceDesc.30AD%     = ATHR_DEV_OS61_30AB.ndi,     PCI\VEN_168C&DEV_002B&SUBSYS_30AD168C
%ATHR.DeviceDesc.30AE%     = ATHR_DEV_OS61_30AA.ndi,     PCI\VEN_168C&DEV_002B&SUBSYS_30AE168C
%ATHR.DeviceDesc.30AF%     = ATHR_DEV_OS61_30AB.ndi,     PCI\VEN_168C&DEV_002B&SUBSYS_30AF168C
%ATHR.DeviceDesc.30B0%     = ATHR_DEV_OS61_30B0.ndi,     PCI\VEN_168C&DEV_002E&SUBSYS_30B0168C
%ATHR.DeviceDesc.3091%     = ATHR_DEV_OS61_3091.ndi,     PCI\VEN_168C&DEV_002A&SUBSYS_30A3168C
%ATHR.DeviceDesc.30A7%     = ATHR_DEV_OS61_001C.ndi,     PCI\VEN_168C&DEV_002C&SUBSYS_30A7168C
%ATHR.DeviceDesc.2099%     = ATHR_DEV_OS61_30A1.ndi,     PCI\VEN_168C&DEV_002D&SUBSYS_2099168C
%ATHR.DeviceDesc.30A4%     = ATHR_DEV_OS61_30A4.ndi,     PCI\VEN_168C&DEV_002E&SUBSYS_30A4168C
; Customer X
%ATHR.DeviceDesc.0013%     = ATHR_DEV_OS61_0013.ndi,     PCI\VEN_168C&DEV_0013&SUBSYS_A527167D
%ATHR.DeviceDesc.3072%     = ATHR_DEV_OS61_7125144F.ndi, PCI\VEN_168C&DEV_0024&SUBSYS_04291468
%ATHR.DeviceDesc.3072%     = ATHR_DEV_OS61_3072.ndi,     PCI\VEN_168C&DEV_0024&SUBSYS_04301468
%ATHR.DeviceDesc.2055%     = ATHR_DEV_OS61_2055.ndi,     PCI\VEN_168C&DEV_001D&SUBSYS_720B1799
%ATHR.DeviceDesc.2055%     = ATHR_DEV_OS61_2055.ndi,     PCI\VEN_168C&DEV_001D&SUBSYS_B2031113
; Foxconn
%ATHR.DeviceDesc.3062%     = ATHR_DEV_OS61_04221468.ndi, PCI\VEN_168C&DEV_001C&SUBSYS_04221468
%ATHR.DeviceDesc.001A%     = ATHR_DEV_OS61_04221468.ndi, PCI\VEN_168C&DEV_0013&SUBSYS_04171468
%ATHR.DeviceDesc.001A%     = ATHR_DEV_OS61_04221468.ndi, PCI\VEN_168C&DEV_001A&SUBSYS_04181468
%ATHR.DeviceDesc.001A%     = ATHR_DEV_OS61_04221468.ndi, PCI\VEN_168C&DEV_001A&SUBSYS_04201468
%ATHR.DeviceDesc.30A1%     = ATHR_DEV_OS61_E023105B.ndi, PCI\VEN_168C&DEV_002B&SUBSYS_E023105B
%ATHR.DeviceDesc.30A1%     = ATHR_DEV_OS61_E036105B.ndi, PCI\VEN_168C&DEV_002B&SUBSYS_E036105B
%ATHR.DeviceDesc.30A7%     = ATHR_DEV_OS61_E029105B.ndi, PCI\VEN_168C&DEV_002C&SUBSYS_E029105B
%ATHR.DeviceDesc.30A7%     = ATHR_DEV_OS61_E029105B.ndi, PCI\VEN_168C&DEV_002C&SUBSYS_1029105B
%ATHR.DeviceDesc.30AB%     = ATHR_DEV_OS61_E033105Bw.ndi,PCI\VEN_168C&DEV_002B&SUBSYS_E033105B
%ATHR.DeviceDesc.946x%     = ATHR_DEV_OS61_311711AD.ndi, PCI\VEN_168C&DEV_0034&SUBSYS_E064105B
%ATHR.DeviceDesc.9485%     = ATHR_DEV_OS61_661711AD.ndi, PCI\VEN_168C&DEV_0032&SUBSYS_E062105B
%ATHR.DeviceDesc.3119%     = ATHR_DEV_OS61_661811AD.ndi, PCI\VEN_168C&DEV_0032&SUBSYS_E063105B
%ATHR.DeviceDesc.30A1%     = ATHR_DEV_OS61_S30A1.ndi,    PCI\VEN_168C&DEV_002B&SUBSYS_E070105B
%ATHR.DeviceDesc.311711AD% = ATHR_DEV_OS61_1186788.ndi,  PCI\VEN_168C&DEV_0034&SUBSYS_E07D105B
; Apple
%ATHR.DeviceDesc.3091%     = ATHR_DEV_OS61_008F106B.ndi, PCI\VEN_168C&DEV_002A&SUBSYS_008F106B
%ATHR.DeviceDesc.938x%     = ATHR_DEV_OS61_938x.ndi,     PCI\VEN_168C&DEV_0030&SUBSYS_009A106B
; Linksys
%ATHR.DeviceDesc.1737_g%   = ATHR_DEV_OS61_001A.ndi,     PCI\VEN_168C&DEV_001A&SUBSYS_00531737
%ATHR.DeviceDesc.1737_bg%  = ATHR_DEV_OS61_001B.ndi,     PCI\VEN_168C&DEV_001B&SUBSYS_00431737
%ATHR.DeviceDesc.0044%     = ATHR_DEV_OS61_001B.ndi,     PCI\VEN_168C&DEV_001B&SUBSYS_00441737
%ATHR.DeviceDesc.1737_bg%  = ATHR_DEV_OS61_0013.ndi,     PCI\VEN_168C&DEV_0013&SUBSYS_00351731
%ATHR.DeviceDesc.1737_bg%  = ATHR_DEV_OS61_0013.ndi,     PCI\VEN_168C&DEV_0013&SUBSYS_00351737
%ATHR.DeviceDesc.1737_bg%  = ATHR_DEV_OS61_0013.ndi,     PCI\VEN_168C&DEV_0013&SUBSYS_00171737
%ATHR.DeviceDesc.1737_bg%  = ATHR_DEV_OS61_0013.ndi,     PCI\VEN_168C&DEV_0013&SUBSYS_00251737
%ATHR.DeviceDesc.1737_bg%  = ATHR_DEV_OS61_0013.ndi,     PCI\VEN_168C&DEV_0013&SUBSYS_1026168C
%ATHR.DeviceDesc.1737_abg% = ATHR_DEV_OS61_0013.ndi,     PCI\VEN_168C&DEV_0013&SUBSYS_00361737
; Siemens
%ATHR.DeviceDesc.800118CB% = ATHR_DEV_OS61_3072.ndi,     PCI\VEN_168C&DEV_0023&SUBSYS_800118CB
%ATHR.DeviceDesc.3070%     = ATHR_DEV_OS61_1042.ndi,     PCI\VEN_168C&DEV_0013&SUBSYS_307002FA
%ATHR.DeviceDesc.3071%     = ATHR_DEV_OS61_1042.ndi,     PCI\VEN_168C&DEV_001A&SUBSYS_307102FA
%ATHR.DeviceDesc.30A1%     = ATHR_DEV_OS61_662111AD.ndi, PCI\VEN_168C&DEV_002B&SUBSYS_662111AD
%ATHR.DeviceDesc.3091%     = ATHR_DEV_OS61_662211AD.ndi, PCI\VEN_168C&DEV_002A&SUBSYS_662211AD
;Accton
%ATHR.DeviceDesc.3062%     = ATHR_DEV_OS61_2062.ndi,     PCI\VEN_168C&DEV_001C&SUBSYS_75191113
; AMD
%ATHR.DeviceDesc.3091%     = ATHR_DEV_OS61_3091amd.ndi,  PCI\VEN_168C&DEV_002A&SUBSYS_1130168C
; Netgear
%ATHR.DeviceDesc.90001385% = ATHR_DEV_OS61_90001385.ndi, PCI\VEN_168C&DEV_0024&SUBSYS_90001385
%ATHR.DeviceDesc.4B001385% = ATHR_DEV_OS61_0013.ndi,     PCI\VEN_168C&DEV_0013&SUBSYS_4B001385
%ATHR.DeviceDesc.4B001385% = ATHR_DEV_OS61_0013.ndi,     PCI\VEN_168C&DEV_0013&SUBSYS_5B001385
%ATHR.DeviceDesc.5D001385% = ATHR_DEV_OS61_0013.ndi,     PCI\VEN_168C&DEV_0013&SUBSYS_5D001385
%ATHR.DeviceDesc.4D001385% = ATHR_DEV_OS61_0013.ndi,     PCI\VEN_168C&DEV_0013&SUBSYS_4D001385
%ATHR.DeviceDesc.4F001385% = ATHR_DEV_OS61_0013.ndi,     PCI\VEN_168C&DEV_0013&SUBSYS_4F001385
%ATHR.DeviceDesc.5E001385% = ATHR_DEV_OS61_0013.ndi,     PCI\VEN_168C&DEV_0013&SUBSYS_5E001385
%ATHR.DeviceDesc.4D001385% = ATHR_DEV_OS61_0013.ndi,     PCI\VEN_168C&DEV_0013&SUBSYS_5A001385
%ATHR.DeviceDesc.0013%     = ATHR_DEV_OS61_0013.ndi,     PCI\VEN_168C&DEV_0013&SUBSYS_46101385
; OQO
%ATHR.DeviceDesc.2062%     = ATHR_DEV_OS61_2062.ndi,     PCI\VEN_168C&DEV_001B&SUBSYS_1602196f
%ATHR.DeviceDesc.2062%     = ATHR_DEV_OS61_2062.ndi,     PCI\VEN_168C&DEV_001B&SUBSYS_1603196f
%ATHR.DeviceDesc.3062%     = ATHR_DEV_OS61_2062.ndi,     PCI\VEN_168C&DEV_001C&SUBSYS_1604196f
;Lenovo Japan
%ATHR.DeviceDesc.5013%     = ATHR_DEV_OS61_5013.ndi,     PCI\VEN_168C&DEV_001C&SUBSYS_0034168c
%ATHR.DeviceDesc.6013%     = ATHR_DEV_OS61_6013.ndi,     PCI\VEN_168C&DEV_001C&SUBSYS_0035168c
%ATHR.DeviceDesc.3013%     = ATHR_DEV_OS61_3013.ndi,     PCI\VEN_168C&DEV_1014&SUBSYS_05891014
%ATHR.DeviceDesc.4013%     = ATHR_DEV_OS61_4013.ndi,     PCI\VEN_168C&DEV_1014&SUBSYS_058A1014
%ATHR.DeviceDesc.2013%     = ATHR_DEV_OS61_2013.ndi,     PCI\VEN_168C&DEV_1014&SUBSYS_057E1014
%ATHR.DeviceDesc.1013%     = ATHR_DEV_OS61_1013.ndi,     PCI\VEN_168C&DEV_0013&SUBSYS_04081468
%ATHR.DeviceDesc.0032168c% = ATHR_DEV_OS61_0032168c.ndi, PCI\VEN_168C&DEV_0024&SUBSYS_0032168c
%ATHR.DeviceDesc.0033168c% = ATHR_DEV_OS61_0033168c.ndi, PCI\VEN_168C&DEV_0024&SUBSYS_0033168c
%ATHR.DeviceDesc.0036%     = ATHR_DEV_OS61_0036.ndi,     PCI\VEN_168C&DEV_002A&SUBSYS_0036168c
%ATHR.DeviceDesc.0037%     = ATHR_DEV_OS61_0037.ndi,     PCI\VEN_168C&DEV_002B&SUBSYS_0037168c
%ATHR.DeviceDesc.946x%     = ATHR_DEV_OS61_946x.ndi,     PCI\VEN_168C&DEV_0034&SUBSYS_008814CD
%ATHR.DeviceDesc.946x%     = ATHR_DEV_OS61_946x.ndi,     PCI\VEN_168C&DEV_0034&SUBSYS_008114CD
; Lenovo China
%ATHR.DeviceDesc.309917AA% = ATHR_DEV_OS61_309917AA.ndi, PCI\VEN_168C&DEV_002A&SUBSYS_309917AA
%ATHR.DeviceDesc.3067%     = ATHR_DEV_OS61_316417AA.ndi, PCI\VEN_168C&DEV_001C&SUBSYS_316417AA
%ATHR.DeviceDesc.3091%     = ATHR_DEV_OS61_309D17AA.ndi, PCI\VEN_168C&DEV_002A&SUBSYS_309D17AA
%ATHR.DeviceDesc.30A1%     = ATHR_DEV_OS61_30A117AA.ndi, PCI\VEN_168C&DEV_002B&SUBSYS_30A117AA
%ATHR.DeviceDesc.30A1%     = ATHR_DEV_OS61_30A117AAw.ndi,PCI\VEN_168C&DEV_002B&SUBSYS_31A117AA
%ATHR.DeviceDesc.30A4%     = ATHR_DEV_OS61_30A417AA.ndi, PCI\VEN_168C&DEV_002E&SUBSYS_30A417AA
%ATHR.DeviceDesc.30A4%     = ATHR_DEV_OS61_30A417AAw.ndi,PCI\VEN_168C&DEV_002E&SUBSYS_31A417AA
%ATHR.DeviceDesc.30ABLT%   = ATHR_DEV_OS61_30A117AAw.ndi,PCI\VEN_168C&DEV_002B&SUBSYS_30AB185F
%ATHR.DeviceDesc.9485%     = ATHR_DEV_OS61_311817AA.ndi, PCI\VEN_168C&DEV_0032&SUBSYS_311817AA
%ATHR.DeviceDesc.3119%     = ATHR_DEV_OS61_321817AA.ndi, PCI\VEN_168C&DEV_0032&SUBSYS_321817AA
%ATHR.DeviceDesc.3119%     = ATHR_DEV_OS61_321917AA.ndi, PCI\VEN_168C&DEV_0032&SUBSYS_321917AA
%ATHR.DeviceDesc.946x%     = ATHR_DEV_OS61_311417AA.ndi, PCI\VEN_168C&DEV_0034&SUBSYS_311417AA
%ATHR.DeviceDesc.946x%     = ATHR_DEV_OS61_321417AA.ndi, PCI\VEN_168C&DEV_0034&SUBSYS_321417AA
%ATHR.DeviceDesc.946x%     = ATHR_DEV_OS61_00911969.ndi, PCI\VEN_168C&DEV_0034&SUBSYS_00911969
%ATHR.DeviceDesc.302617AA% = ATHR_DEV_OS61_302617AA.ndi, PCI\VEN_168C&DEV_0036&SUBSYS_302617AA
%ATHR.DeviceDesc.302617AA% = ATHR_DEV_OS61_402617AA.ndi, PCI\VEN_168C&DEV_0036&SUBSYS_402617AA
; QCA Killer
%ATHR.DeviceDesc.k1202%    = ATHR_DEV_OS61_K1202.ndi,    PCI\VEN_168C&DEV_0034&SUBSYS_20031A56
%ATHR.DeviceDesc.k1103%    = ATHR_DEV_OS61_K110x.ndi,    PCI\VEN_168C&DEV_0030&SUBSYS_20011A56
%ATHR.DeviceDesc.k1102%    = ATHR_DEV_OS61_K110x.ndi,    PCI\VEN_168C&DEV_0030&SUBSYS_20001A56
; IBM
%ATHR.DeviceDesc.0033168c% = ATHR_DEV_OS61_03841014.ndi, PCI\VEN_168C&DEV_0024&SUBSYS_03841014
; Samsung
%ATHR.DeviceDesc.001A%     = ATHR_DEV_OS61_S001A.ndi,    PCI\VEN_168C&DEV_001A&SUBSYS_7101144F
%ATHR.DeviceDesc.001A%     = ATHR_DEV_OS61_S001A.ndi,    PCI\VEN_168C&DEV_001A&SUBSYS_7114144F
%ATHR.DeviceDesc.001A%     = ATHR_DEV_OS61_S001A.ndi,    PCI\VEN_168C&DEV_001A&SUBSYS_7115144F
%ATHR.DeviceDesc.3067%     = ATHR_DEV_OS61_S3067b.ndi,   PCI\VEN_168C&DEV_001C&SUBSYS_7131144F
%ATHR.DeviceDesc.3067%     = ATHR_DEV_OS61_S3067b.ndi,   PCI\VEN_168C&DEV_001C&SUBSYS_7130144F
%ATHR.DeviceDesc.001B%     = ATHR_DEV_OS61_S001B.ndi,    PCI\VEN_168C&DEV_001C&SUBSYS_7108144F
%ATHR.DeviceDesc.001B%     = ATHR_DEV_OS61_S001B.ndi,    PCI\VEN_168C&DEV_001C&SUBSYS_7116144F
%ATHR.DeviceDesc.3067%     = ATHR_DEV_OS61_S3067b.ndi,   PCI\VEN_168C&DEV_001C&SUBSYS_E00B105B
%ATHR.DeviceDesc.3067%     = ATHR_DEV_OS61_S3067b.ndi,   PCI\VEN_168C&DEV_001C&SUBSYS_E00C105B
%ATHR.DeviceDesc.001B%     = ATHR_DEV_OS61_S3067.ndi,    PCI\VEN_168C&DEV_001C&SUBSYS_E00E105B
%ATHR.DeviceDesc.3091%     = ATHR_DEV_OS61_3091SF.ndi,   PCI\VEN_168C&DEV_002A&SUBSYS_E00F105B
%ATHR.DeviceDesc.3091%     = ATHR_DEV_OS61_3091SF.ndi,   PCI\VEN_168C&DEV_002A&SUBSYS_E010105B
%ATHR.DeviceDesc.3091%     = ATHR_DEV_OS61_3091SF.ndi,   PCI\VEN_168C&DEV_002A&SUBSYS_7161144F
%ATHR.DeviceDesc.30A1%     = ATHR_DEV_OS61_30A1a.ndi,    PCI\VEN_168C&DEV_002B&SUBSYS_7167144F
%ATHR.DeviceDesc.30A1%     = ATHR_DEV_OS61_30A1a.ndi,    PCI\VEN_168C&DEV_002B&SUBSYS_E025105B
%ATHR.DeviceDesc.30AB%     = ATHR_DEV_OS61_30A1w.ndi,    PCI\VEN_168C&DEV_002B&SUBSYS_E032105B
%ATHR.DeviceDesc.30ABLT%   = ATHR_DEV_OS61_30A1w.ndi,    PCI\VEN_168C&DEV_002B&SUBSYS_7178144F
%ATHR.DeviceDesc.30ABLT%   = ATHR_DEV_OS61_30A1w.ndi,    PCI\VEN_168C&DEV_002B&SUBSYS_30B2185F
%ATHR.DeviceDesc.30A1%     = ATHR_DEV_OS61_30A1a.ndi,    PCI\VEN_168C&DEV_002B&SUBSYS_7187144F
%ATHR.DeviceDesc.30B0%     = ATHR_DEV_OS61_30B07189.ndi, PCI\VEN_168C&DEV_002E&SUBSYS_7189144F
%ATHR.DeviceDesc.30A1%     = ATHR_DEV_OS61_30A1a.ndi,    PCI\VEN_168C&DEV_002B&SUBSYS_4101144D
%ATHR.DeviceDesc.30A1%     = ATHR_DEV_OS61_30A1a.ndi,    PCI\VEN_168C&DEV_002B&SUBSYS_4114144D
%ATHR.DeviceDesc.30ABLT%   = ATHR_DEV_OS61_30A1w.ndi,    PCI\VEN_168C&DEV_002B&SUBSYS_4102144D
%ATHR.DeviceDesc.30ABLT%   = ATHR_DEV_OS61_30A1w.ndi,    PCI\VEN_168C&DEV_002B&SUBSYS_4103144D
%ATHR.DeviceDesc.30ABLT%   = ATHR_DEV_OS61_30A1w.ndi,    PCI\VEN_168C&DEV_002B&SUBSYS_4104144D
%ATHR.DeviceDesc.3119%     = ATHR_DEV_OS61_3119s.ndi,    PCI\VEN_168C&DEV_0032&SUBSYS_4105144D
%ATHR.DeviceDesc.3119%     = ATHR_DEV_OS61_3119s.ndi,    PCI\VEN_168C&DEV_0032&SUBSYS_4106144D
%ATHR.DeviceDesc.3119%     = ATHR_DEV_OS61_3119s.ndi,    PCI\VEN_168C&DEV_0032&SUBSYS_410D144D
%ATHR.DeviceDesc.3119%     = ATHR_DEV_OS61_3119s.ndi,    PCI\VEN_168C&DEV_0032&SUBSYS_410E144D
%ATHR.DeviceDesc.3119%     = ATHR_DEV_OS61_3119s.ndi,    PCI\VEN_168C&DEV_0032&SUBSYS_410F144D
%ATHR.DeviceDesc.938x%     = ATHR_DEV_OS61_4107144D.ndi, PCI\VEN_168C&DEV_0030&SUBSYS_4107144D
%ATHR.DeviceDesc.938x%     = ATHR_DEV_OS61_4107144D.ndi, PCI\VEN_168C&DEV_0030&SUBSYS_4108144D
%ATHR.DeviceDesc.938x%     = ATHR_DEV_OS61_4107144D.ndi, PCI\VEN_168C&DEV_0030&SUBSYS_4109144D
%ATHR.DeviceDesc.938x%     = ATHR_DEV_OS61_4107144D.ndi, PCI\VEN_168C&DEV_0030&SUBSYS_410A144D
%ATHR.DeviceDesc.938x%     = ATHR_DEV_OS61_4107144D.ndi, PCI\VEN_168C&DEV_0030&SUBSYS_410B144D
%ATHR.DeviceDesc.938x%     = ATHR_DEV_OS61_4107144D.ndi, PCI\VEN_168C&DEV_0030&SUBSYS_410C144D
%ATHR.DeviceDesc.9485%     = ATHR_DEV_OS61_9485s.ndi,    PCI\VEN_168C&DEV_0032&SUBSYS_4115144D
%ATHR.DeviceDesc.9485%     = ATHR_DEV_OS61_9485s.ndi,    PCI\VEN_168C&DEV_0032&SUBSYS_4116144D
%ATHR.DeviceDesc.9485%     = ATHR_DEV_OS61_9485s.ndi,    PCI\VEN_168C&DEV_0032&SUBSYS_4117144D
%ATHR.DeviceDesc.946x%     = ATHR_DEV_OS61_946xs.ndi,    PCI\VEN_168C&DEV_0034&SUBSYS_4110144D
%ATHR.DeviceDesc.946x%     = ATHR_DEV_OS61_946xs.ndi,    PCI\VEN_168C&DEV_0034&SUBSYS_4111144D
%ATHR.DeviceDesc.946x%     = ATHR_DEV_OS61_946xs.ndi,    PCI\VEN_168C&DEV_0034&SUBSYS_4112144D
%ATHR.DeviceDesc.946x%     = ATHR_DEV_OS61_946xs.ndi,    PCI\VEN_168C&DEV_0034&SUBSYS_4113144D
%ATHR.DeviceDesc.946x%     = ATHR_DEV_OS61_946xs.ndi,    PCI\VEN_168C&DEV_0034&SUBSYS_C0F9144D
%ATHR.DeviceDesc.946x%     = ATHR_DEV_OS61_946xs.ndi,    PCI\VEN_168C&DEV_0034&SUBSYS_C0E8144D
%ATHR.DeviceDesc.946x%     = ATHR_DEV_OS61_946xs.ndi,    PCI\VEN_168C&DEV_0034&SUBSYS_C0E6144D
%ATHR.DeviceDesc.946x%     = ATHR_DEV_OS61_946xs.ndi,    PCI\VEN_168C&DEV_0034&SUBSYS_411F144D
%ATHR.DeviceDesc.946x%     = ATHR_DEV_OS61_946xs.ndi,    PCI\VEN_168C&DEV_0034&SUBSYS_4120144D
%ATHR.DeviceDesc.3119%     = ATHR_DEV_OS61_3119s.ndi,    PCI\VEN_168C&DEV_0032&SUBSYS_C706144D
%ATHR.DeviceDesc.3119%     = ATHR_DEV_OS61_3119s.ndi,    PCI\VEN_168C&DEV_0032&SUBSYS_C680144D
%ATHR.DeviceDesc.3119%     = ATHR_DEV_OS61_3119s.ndi,    PCI\VEN_168C&DEV_0032&SUBSYS_C708144D
%ATHR.DeviceDesc.956x%     = ATHR_DEV_OS61_956xs.ndi,    PCI\VEN_168C&DEV_0036&SUBSYS_411A144D
%ATHR.DeviceDesc.956x%     = ATHR_DEV_OS61_956xs.ndi,    PCI\VEN_168C&DEV_0036&SUBSYS_411B144D
%ATHR.DeviceDesc.956x%     = ATHR_DEV_OS61_956xs.ndi,    PCI\VEN_168C&DEV_0036&SUBSYS_411C144D
%ATHR.DeviceDesc.956x%     = ATHR_DEV_OS61_956xs.ndi,    PCI\VEN_168C&DEV_0036&SUBSYS_411D144D
%ATHR.DeviceDesc.956x%     = ATHR_DEV_OS61_956xs.ndi,    PCI\VEN_168C&DEV_0036&SUBSYS_411E144D
%ATHR.DeviceDesc.956x%     = ATHR_DEV_OS61_SS335.ndi,    PCI\VEN_168C&DEV_0036&SUBSYS_4129144D
%ATHR.DeviceDesc.956x%     = ATHR_DEV_OS61_SS335.ndi,    PCI\VEN_168C&DEV_0036&SUBSYS_412A144D
; Option
%ATHR.DeviceDesc.00231931% = ATHR_DEV_OS61_30A1op.ndi,   PCI\VEN_168C&DEV_002B&SUBSYS_00231931
; D-Link
%ATHR.DeviceDesc.DWA642%   = ATHR_DEV_OS61_1186.ndi,     PCI\VEN_168C&DEV_0023&SUBSYS_3A6A1186
%ATHR.DeviceDesc.DWA645%   = ATHR_DEV_OS61_1186.ndi,     PCI\VEN_168C&DEV_0023&SUBSYS_3A0907D1
%ATHR.DeviceDesc.DWA645%   = ATHR_DEV_OS61_1186.ndi,     PCI\VEN_168C&DEV_0023&SUBSYS_3A761186
%ATHR.DeviceDesc.DWA645%   = ATHR_DEV_OS61_3A7B1186.ndi, PCI\VEN_168C&DEV_0029&SUBSYS_3A791186
%ATHR.DeviceDesc.DWA542%   = ATHR_DEV_OS61_3A691186.ndi, PCI\VEN_168C&DEV_0023&SUBSYS_3A691186
%ATHR.DeviceDesc.DWA547%   = ATHR_DEV_OS61_3A6D1186.ndi, PCI\VEN_168C&DEV_0023&SUBSYS_3A6B1186
%ATHR.DeviceDesc.DWA547%   = ATHR_DEV_OS61_3A7A1186.ndi, PCI\VEN_168C&DEV_0029&SUBSYS_3A781186
%ATHR.DeviceDesc.DWA652%   = ATHR_DEV_OS61_1186.ndi,     PCI\VEN_168C&DEV_0023&SUBSYS_3A6E1186
%ATHR.DeviceDesc.DWA652%   = ATHR_DEV_OS61_3A7B1186.ndi, PCI\VEN_168C&DEV_0029&SUBSYS_3A7B1186
%ATHR.DeviceDesc.DWA552%   = ATHR_DEV_OS61_3A6D1186.ndi, PCI\VEN_168C&DEV_0023&SUBSYS_3A6D1186
%ATHR.DeviceDesc.DWA552%   = ATHR_DEV_OS61_3A7A1186.ndi, PCI\VEN_168C&DEV_0029&SUBSYS_3A7A1186
%ATHR.DeviceDesc.DWA643%   = ATHR_DEV_OS61_3A6F1186.ndi, PCI\VEN_168C&DEV_0024&SUBSYS_3A6F1186
%ATHR.DeviceDesc.DWA556%   = ATHR_DEV_OS61_3A701186.ndi, PCI\VEN_168C&DEV_0024&SUBSYS_3A701186
%ATHR.DeviceDesc.G650%     = ATHR_DEV_OS61_0013.ndi,     PCI\VEN_168C&DEV_0013&SUBSYS_3A121186
%ATHR.DeviceDesc.G520X%    = ATHR_DEV_OS61_0013.ndi,     PCI\VEN_168C&DEV_0013&SUBSYS_32031186
%ATHR.DeviceDesc.G520%     = ATHR_DEV_OS61_0013.ndi,     PCI\VEN_168C&DEV_0013&SUBSYS_3A131186
%ATHR.DeviceDesc.AG520%    = ATHR_DEV_OS61_0013.ndi,     PCI\VEN_168C&DEV_0013&SUBSYS_3A081186
%ATHR.DeviceDesc.AG530%    = ATHR_DEV_OS61_0013.ndi,     PCI\VEN_168C&DEV_0013&SUBSYS_3A141186
%ATHR.DeviceDesc.G630%     = ATHR_DEV_OS61_0013.ndi,     PCI\VEN_168C&DEV_001A&SUBSYS_3A151186
%ATHR.DeviceDesc.G510%     = ATHR_DEV_OS61_0013.ndi,     PCI\VEN_168C&DEV_001A&SUBSYS_3A161186
%ATHR.DeviceDesc.AG650%    = ATHR_DEV_OS61_0013.ndi,     PCI\VEN_168C&DEV_0013&SUBSYS_3A071186
%ATHR.DeviceDesc.AG660%    = ATHR_DEV_OS61_0013.ndi,     PCI\VEN_168C&DEV_0013&SUBSYS_3A631186
%ATHR.DeviceDesc.G680%     = ATHR_DEV_OS61_3A171186.ndi, PCI\VEN_168C&DEV_0013&SUBSYS_3A171186
%ATHR.DeviceDesc.G550%     = ATHR_DEV_OS61_0013.ndi,     PCI\VEN_168C&DEV_0013&SUBSYS_3A181186
%ATHR.DeviceDesc.AG660B%   = ATHR_DEV_OS61_3A171186.ndi, PCI\VEN_168C&DEV_001B&SUBSYS_3A191186
%ATHR.DeviceDesc.AG530B%   = ATHR_DEV_OS61_0013.ndi,     PCI\VEN_168C&DEV_001B&SUBSYS_3A221186
%ATHR.DeviceDesc.G650P%    = ATHR_DEV_OS61_0013.ndi,     PCI\VEN_168C&DEV_001A&SUBSYS_3A241186
%ATHR.DeviceDesc.G520P%    = ATHR_DEV_OS61_0013.ndi,     PCI\VEN_168C&DEV_001A&SUBSYS_3A231186
%ATHR.DeviceDesc.WDA1320%  = ATHR_DEV_OS61_0013.ndi,     PCI\VEN_168C&DEV_001A&SUBSYS_3A1D1186
%ATHR.DeviceDesc.WDA2320%  = ATHR_DEV_OS61_0013.ndi,     PCI\VEN_168C&DEV_0013&SUBSYS_3A1B1186
%ATHR.DeviceDesc.DWA520%   = ATHR_DEV_OS61_0013.ndi,     PCI\VEN_168C&DEV_0013&SUBSYS_3A731186
%ATHR.DeviceDesc.DWA620%   = ATHR_DEV_OS61_0013.ndi,     PCI\VEN_168C&DEV_0013&SUBSYS_3A741186
%ATHR.DeviceDesc.CWNA2330% = ATHR_DEV_OS61_3A171186.ndi, PCI\VEN_168C&DEV_0013&SUBSYS_3A1A1186
%ATHR.DeviceDesc.CWNA1330% = ATHR_DEV_OS61_0013.ndi,     PCI\VEN_168C&DEV_0013&SUBSYS_3A1C1186
%ATHR.DeviceDesc.CWNA1330% = ATHR_DEV_OS61_3A171186.ndi, PCI\VEN_168C&DEV_001A&SUBSYS_3A1C1186
%ATHR.DeviceDesc.CG650%    = ATHR_DEV_OS61_0013.ndi,     PCI\VEN_168C&DEV_0013&SUBSYS_32021186
%ATHR.DeviceDesc.CG630%    = ATHR_DEV_OS61_0013.ndi,     PCI\VEN_168C&DEV_001A&SUBSYS_3B081186
%ATHR.DeviceDesc.CG630%    = ATHR_DEV_OS61_0013.ndi,     PCI\VEN_168C&DEV_0013&SUBSYS_3B081186
; Alpha/ATKK
%ATIWC.DeviceDesc.ATICB%   = ATHR_DEV_OS61_0013.ndi,     PCI\VEN_168C&DEV_0013&SUBSYS_12041259
%ATIWC.DeviceDesc.ATIPC%   = ATHR_DEV_OS61_0013.ndi,     PCI\VEN_168C&DEV_0013&SUBSYS_12031259
%ATHR.DeviceDesc.DWA566%   = ATHR_DEV_OS61_938x.ndi,     PCI\VEN_168C&DEV_0030&SUBSYS_3A7E1186
%ATHR.DeviceDesc.TEW726%   = ATHR_DEV_OS61_938x.ndi,     PCI\VEN_168C&DEV_0030&SUBSYS_3ABE1948
; Motion Computing
%ATHR.DeviceDesc.3061%     = ATHR_DEV_OS61_7111144F.ndi, PCI\VEN_168C&DEV_001C&SUBSYS_7111144F
; Azurewave
%ATHR.DeviceDesc.3067%     = ATHR_DEV_OS61_001C.ndi,     PCI\VEN_168C&DEV_001C&SUBSYS_10341A3B
%ATHR.DeviceDesc.3067%     = ATHR_DEV_OS61_10261A3B.ndi, PCI\VEN_168C&DEV_001C&SUBSYS_10261A3B
%ATHR.DeviceDesc.3067%     = ATHR_DEV_OS61_10261A3B.ndi, PCI\VEN_168C&DEV_001C&SUBSYS_10601A3B
%ATHR.DeviceDesc.3072%     = ATHR_DEV_OS61_10241A3B.ndi, PCI\VEN_168C&DEV_0024&SUBSYS_10241A3B
%ATHR.DeviceDesc.3091%     = ATHR_DEV_OS61_10671A3B.ndi, PCI\VEN_168C&DEV_002A&SUBSYS_10671A3B
%ATHR.DeviceDesc.3091%     = ATHR_DEV_OS61_10711A3B.ndi, PCI\VEN_168C&DEV_002A&SUBSYS_10711A3B
%ATHR.DeviceDesc.3091%     = ATHR_DEV_OS61_10711A3B.ndi, PCI\VEN_168C&DEV_002A&SUBSYS_10811A3B
%ATHR.DeviceDesc.30A1%     = ATHR_DEV_OS61_10891A3B.ndi, PCI\VEN_168C&DEV_002B&SUBSYS_10891A3B
%ATHR.DeviceDesc.30ABLT%   = ATHR_DEV_OS61_1D891A3B.ndi, PCI\VEN_168C&DEV_002B&SUBSYS_1D891A3B
%ATHR.DeviceDesc.3091%     = ATHR_DEV_OS61_10671A3B.ndi, PCI\VEN_168C&DEV_002A&SUBSYS_10901A3B
%ATHR.DeviceDesc.30A1%     = ATHR_DEV_OS61_20371A3B.ndi, PCI\VEN_168C&DEV_002B&SUBSYS_11061A3B
%ATHR.DeviceDesc.3091%     = ATHR_DEV_OS61_1A671A3B.ndi, PCI\VEN_168C&DEV_002A&SUBSYS_1A671A3B
%ATHR.DeviceDesc.30A1%     = ATHR_DEV_OS61_1A891A3B.ndi, PCI\VEN_168C&DEV_002B&SUBSYS_1A891A3B
%ATHR.DeviceDesc.30A7%     = ATHR_DEV_OS61_11121A3B.ndi, PCI\VEN_168C&DEV_002C&SUBSYS_11121A3B
%ATHR.DeviceDesc.30A7%     = ATHR_DEV_OS61_11121A3B.ndi, PCI\VEN_168C&DEV_002C&SUBSYS_1A121A3B
%ATHR.DeviceDesc.3067%     = ATHR_DEV_OS61_10261A3B.ndi, PCI\VEN_168C&DEV_001C&SUBSYS_10331A3B
%ATHR.DeviceDesc.30AB%     = ATHR_DEV_OS61_30AB.ndi,     PCI\VEN_168C&DEV_002B&SUBSYS_20361A3B
%ATHR.DeviceDesc.30ABLT%   = ATHR_DEV_OS61_2C371A3B.ndi, PCI\VEN_168C&DEV_002B&SUBSYS_2C371A3B
%ATHR.DeviceDesc.30A4%     = ATHR_DEV_OS61_11211A3B.ndi, PCI\VEN_168C&DEV_002E&SUBSYS_11211A3B
%ATHR.DeviceDesc.30A4%     = ATHR_DEV_OS61_1A211A3B.ndi, PCI\VEN_168C&DEV_002E&SUBSYS_1A211A3B
%ATHR.DeviceDesc.2A371A3B% = ATHR_DEV_OS61_2A371A3B.ndi, PCI\VEN_168C&DEV_002B&SUBSYS_2A371A3B
%ATHR.DeviceDesc.3119%     = ATHR_DEV_OS61_2C971A3B_3.ndi, PCI\VEN_168C&DEV_0032&SUBSYS_2C971A3B
%ATHR.DeviceDesc.9485%     = ATHR_DEV_OS61_11861A3B.ndi, PCI\VEN_168C&DEV_0032&SUBSYS_11861A3B
%ATHR.DeviceDesc.3119%     = ATHR_DEV_OS61_20861A3B.ndi,   PCI\VEN_168C&DEV_0032&SUBSYS_20861A3B
%ATHR.DeviceDesc.9485%     = ATHR_DEV_OS61_11861A3B.ndi, PCI\VEN_168C&DEV_0032&SUBSYS_1F861A3B
%ATHR.DeviceDesc.11951A3B% = ATHR_DEV_OS61_11861A3B.ndi, PCI\VEN_168C&DEV_0032&SUBSYS_11951A3B
%ATHR.DeviceDesc.11951A3B% = ATHR_DEV_OS61_11861A3B.ndi, PCI\VEN_168C&DEV_0032&SUBSYS_1F951A3B
%ATHR.DeviceDesc.21001A3B% = ATHR_DEV_OS61_2C971A3B.ndi, PCI\VEN_168C&DEV_0032&SUBSYS_21001A3B
%ATHR.DeviceDesc.11951A3B% = ATHR_DEV_OS61_11861A3B.ndi, PCI\VEN_168C&DEV_0037&SUBSYS_11951A3B
%ATHR.DeviceDesc.11951A3B% = ATHR_DEV_OS61_11861A3B.ndi, PCI\VEN_168C&DEV_0037&SUBSYS_1F951A3B
%ATHR.DeviceDesc.21001A3B% = ATHR_DEV_OS61_2C971A3B.ndi, PCI\VEN_168C&DEV_0037&SUBSYS_21001A3B
%ATHR.DeviceDesc.938x%     = ATHR_DEV_OS61_651311AD.ndi, PCI\VEN_168C&DEV_0030&SUBSYS_11731A3B
%ATHR.DeviceDesc.9485%     = ATHR_DEV_OS61_118C1A3B1.ndi, PCI\VEN_168C&DEV_0032&SUBSYS_118C1A3B
%ATHR.DeviceDesc.3119%     = ATHR_DEV_OS61_209C1A3B.ndi, PCI\VEN_168C&DEV_0032&SUBSYS_209C1A3B
%ATHR.DeviceDesc.946x%     = ATHR_DEV_OS61_21101A3B.ndi, PCI\VEN_168C&DEV_0034&SUBSYS_21101A3B
%ATHR.DeviceDesc.946x%     = ATHR_DEV_OS61_211C1A3B.ndi, PCI\VEN_168C&DEV_0034&SUBSYS_211C1A3B
%ATHR.DeviceDesc.946x%     = ATHR_DEV_OS61_21101A3B.ndi, PCI\VEN_168C&DEV_0034&SUBSYS_211F1A3B
%ATHR.DeviceDesc.3119%     = ATHR_DEV_OS61_CUS198_1.ndi, PCI\VEN_168C&DEV_0032&SUBSYS_12371A3B
%ATHR.DeviceDesc.3119%     = ATHR_DEV_OS61_21261A3B.ndi, PCI\VEN_168C&DEV_0032&SUBSYS_21261A3B
%ATHR.DeviceDesc.3119%     = ATHR_DEV_OS61_20971A3B.ndi, PCI\VEN_168C&DEV_0032&SUBSYS_20971A3B
; Huawei
%ATHR.DeviceDesc.30A1%     = ATHR_DEV_OS61_10891A3B.ndi, PCI\VEN_168C&DEV_002B&SUBSYS_A5003485
%ATHR.DeviceDesc.30A1%     = ATHR_DEV_OS61_10891A3B.ndi, PCI\VEN_168C&DEV_002B&SUBSYS_A5013485
%ATHR.DeviceDesc.663111AD% = ATHR_DEV_OS61_663111AD.ndi, PCI\VEN_168C&DEV_002B&SUBSYS_A5023485
; Panasonic
%ATHR.DeviceDesc.3091%     = ATHR_DEV_OS61_1C711A3B.ndi, PCI\VEN_168C&DEV_002A&SUBSYS_1C711A3B
; QMI    
%ATHR.DeviceDesc.0013%     = ATHR_DEV_OS61_001C.ndi,     PCI\VEN_168C&DEV_001C&SUBSYS_01121A32                        
%ATHR.DeviceDesc.3065%     = ATHR_DEV_OS61_01001A32.ndi, PCI\VEN_168C&DEV_001C&SUBSYS_01001A32
%ATHR.DeviceDesc.3063%     = ATHR_DEV_OS61_01001A32.ndi, PCI\VEN_168C&DEV_001C&SUBSYS_02001A32
%ATHR.DeviceDesc.3072%     = ATHR_DEV_OS61_03011A32.ndi, PCI\VEN_168C&DEV_0024&SUBSYS_05021A32
%ATHR.DeviceDesc.3091%     = ATHR_DEV_OS61_03011A32.ndi, PCI\VEN_168C&DEV_002A&SUBSYS_03011A32
%ATHR.DeviceDesc.3091%     = ATHR_DEV_OS61_03011A32.ndi, PCI\VEN_168C&DEV_002A&SUBSYS_05041A32
%ATHR.DeviceDesc.3067%     = ATHR_DEV_OS61_01051A32.ndi, PCI\VEN_168C&DEV_001C&SUBSYS_21081A32
%ATHR.DeviceDesc.3067%     = ATHR_DEV_OS61_01051A32.ndi, PCI\VEN_168C&DEV_001C&SUBSYS_01051A32 
%ATHR.DeviceDesc.3067%     = ATHR_DEV_OS61_01051A32.ndi, PCI\VEN_168C&DEV_001C&SUBSYS_2A97103C
%ATHR.DeviceDesc.3067%     = ATHR_DEV_OS61_01121A32.ndi, PCI\VEN_168C&DEV_001C&SUBSYS_01121A32
%ATHR.DeviceDesc.3091%     = ATHR_DEV_OS61_03011A32.ndi, PCI\VEN_168C&DEV_002A&SUBSYS_05071A32
%ATHR.DeviceDesc.30A4%     = ATHR_DEV_OS61_03091A32.ndi, PCI\VEN_168C&DEV_002E&SUBSYS_03091A32
%ATHR.DeviceDesc.30AB%     = ATHR_DEV_OS61_03051A32w.ndi,PCI\VEN_168C&DEV_002B&SUBSYS_23001A32
; Arcadyan
%ATHR.DeviceDesc.3067%     = ATHR_DEV_OS61_01051A32.ndi, PCI\VEN_168C&DEV_001C&SUBSYS_C6011113
%ATHR.DeviceDesc.30A1%     = ATHR_DEV_OS61_D8111113.ndi, PCI\VEN_168C&DEV_002B&SUBSYS_D8111113
%ATHR.DeviceDesc.30A1%     = ATHR_DEV_OS61_03051A32.ndi, PCI\VEN_168C&DEV_002B&SUBSYS_F6111113
%ATHR.DeviceDesc.3091%     = ATHR_DEV_OS61_E006105B.ndi, PCI\VEN_168C&DEV_002A&SUBSYS_C8231113
%ATHR.DeviceDesc.3091%     = ATHR_DEV_OS61_03011A32.ndi, PCI\VEN_168C&DEV_002A&SUBSYS_C8221113
%ATHR.DeviceDesc.3091%     = ATHR_DEV_OS61_03011A32.ndi, PCI\VEN_168C&DEV_002A&SUBSYS_D8221113
%ATHR.DeviceDesc.30A1%     = ATHR_DEV_OS61_03051A32w.ndi,PCI\VEN_168C&DEV_002B&SUBSYS_98111113
%ATHR.DeviceDesc.30A1%     = ATHR_DEV_OS61_10891A3B.ndi, PCI\VEN_168C&DEV_002B&SUBSYS_A0111113
%ATHR.DeviceDesc.9485%     = ATHR_DEV_OS61_9485.ndi,     PCI\VEN_168C&DEV_0032&SUBSYS_F8421113
; Askey/Compal
%ATHR.DeviceDesc.3091%     = ATHR_DEV_OS61_03011A32.ndi, PCI\VEN_168C&DEV_002A&SUBSYS_7168144F
%ATHR.DeviceDesc.3119%     = ATHR_DEV_OS61_2C971A3B_1.ndi, PCI\VEN_168C&DEV_0032&SUBSYS_40011C56
; LiteOn
%ATHR.DeviceDesc.3067%     = ATHR_DEV_OS61_6313.ndi,     PCI\VEN_168C&DEV_001C&SUBSYS_630311AD
%ATHR.DeviceDesc.3067%     = ATHR_DEV_OS61_6313.ndi,     PCI\VEN_168C&DEV_001C&SUBSYS_631311AD
%ATHR.DeviceDesc.3067%     = ATHR_DEV_OS61_6313.ndi,     PCI\VEN_168C&DEV_001C&SUBSYS_633311AD
%ATHR.DeviceDesc.2061%     = ATHR_DEV_OS61_11AD.ndi,     PCI\VEN_168C&DEV_001B&SUBSYS_530111AD
%ATHR.DeviceDesc.2062%     = ATHR_DEV_OS61_11AD.ndi,     PCI\VEN_168C&DEV_001B&SUBSYS_540111AD
%ATHR.DeviceDesc.30A4%     = ATHR_DEV_OS61_660311AD.ndi, PCI\VEN_168C&DEV_002E&SUBSYS_661311AD
%ATHR.DeviceDesc.30AB%     = ATHR_DEV_OS61_30AB.ndi,     PCI\VEN_168C&DEV_002B&SUBSYS_660311AD
%ATHR.DeviceDesc.7136144F% = ATHR_DEV_OS61_03011A32.ndi, PCI\VEN_168C&DEV_002A&SUBSYS_654211AD
%ATHR.DeviceDesc.30A1%     = ATHR_DEV_OS61_10891A3B.ndi, PCI\VEN_168C&DEV_002B&SUBSYS_665111AD
%ATHR.DeviceDesc.938x%     = ATHR_DEV_OS61_651311AD.ndi, PCI\VEN_168C&DEV_0030&SUBSYS_651311AD
%ATHR.DeviceDesc.938x%     = ATHR_DEV_OS61_652311AD.ndi, PCI\VEN_168C&DEV_0030&SUBSYS_652311AD
%ATHR.DeviceDesc.30A4%     = ATHR_DEV_OS61_30A417AAw.ndi,PCI\VEN_168C&DEV_002E&SUBSYS_660711AD
%ATHR.DeviceDesc.9485%     = ATHR_DEV_OS61_11861A3B.ndi, PCI\VEN_168C&DEV_0032&SUBSYS_662711AD
%ATHR.DeviceDesc.3119%     = ATHR_DEV_OS61_662811AD.ndi, PCI\VEN_168C&DEV_0032&SUBSYS_662811AD
%ATHR.DeviceDesc.946x%     = ATHR_DEV_OS61_321417AAA.ndi, PCI\VEN_168C&DEV_0034&SUBSYS_663111AD
%ATHR.DeviceDesc.946x%     = ATHR_DEV_OS61_664111AD.ndi, PCI\VEN_168C&DEV_0034&SUBSYS_664111AD
%ATHR.DeviceDesc.661811AD% = ATHR_DEV_OS61_661811AD.ndi, PCI\VEN_168C&DEV_0037&SUBSYS_661811AD
%ATHR.DeviceDesc.661711AD% = ATHR_DEV_OS61_661711AD.ndi, PCI\VEN_168C&DEV_0037&SUBSYS_661711AD
%ATHR.DeviceDesc.E059105B% = ATHR_DEV_OS61_311711AD.ndi, PCI\VEN_168C&DEV_0034&SUBSYS_665111AD
%ATHR.DeviceDesc.946x%     = ATHR_DEV_OS61_CUS217.ndi,   PCI\VEN_168C&DEV_0034&SUBSYS_666111AD
%ATHR.DeviceDesc.H3119%    = ATHR_DEV_OS61_661711ADPCIE_1_1.ndi, PCI\VEN_168C&DEV_0032&SUBSYS_664711AD
%ATHR.DeviceDesc.956x%     = ATHR_DEV_OS61_956x.ndi,     PCI\VEN_168C&DEV_0036&SUBSYS_062211AD
%ATHR.DeviceDesc.311711AD% = ATHR_DEV_OS61_080211AD.ndi,  PCI\VEN_168C&DEV_0034&SUBSYS_080211AD
%ATHR.DeviceDesc.956x%     = ATHR_DEV_OS61_065211AD.ndi, PCI\VEN_168C&DEV_0036&SUBSYS_065211AD
%ATHR.DeviceDesc.956x%     = ATHR_DEV_OS61_067211AD_PCIE_1_1.ndi, PCI\VEN_168C&DEV_0036&SUBSYS_067211AD
%ATHR.DeviceDesc.946x%     = ATHR_DEV_OS61_081211AD.ndi, PCI\VEN_168C&DEV_0034&SUBSYS_081211AD
%ATHR.DeviceDesc.956x%     = ATHR_DEV_OS61_956x.ndi,     PCI\VEN_168C&DEV_0036&SUBSYS_068211AD
%ATHR.DeviceDesc.946x%     = ATHR_DEV_OS61_664111AD.ndi, PCI\VEN_168C&DEV_0034&SUBSYS_667111AD
%ATHR.DeviceDesc.956x%     = ATHR_DEV_OS61_065211AD.ndi, PCI\VEN_168C&DEV_0036&SUBSYS_069211AD
%ATHR.DeviceDesc.956x%     = ATHR_DEV_OS61_066211AD.ndi, PCI\VEN_168C&DEV_0036&SUBSYS_06A211AD
; Acer
%ATHR.DeviceDesc.E006105B% = ATHR_DEV_OS61_E006105B.ndi, PCI\VEN_168C&DEV_002A&SUBSYS_660011AD 
%ATHR.DeviceDesc.E006105B% = ATHR_DEV_OS61_E006105B.ndi, PCI\VEN_168C&DEV_002A&SUBSYS_E006105B
%ATHR.DeviceDesc.E006105B% = ATHR_DEV_OS61_E006105B.ndi, PCI\VEN_168C&DEV_002A&SUBSYS_03031A32
%ATHR.DeviceDesc.E01F105B% = ATHR_DEV_OS61_E01F105B.ndi, PCI\VEN_168C&DEV_002A&SUBSYS_E01F105B
%ATHR.DeviceDesc.E01F105B% = ATHR_DEV_OS61_E01F105B.ndi, PCI\VEN_168C&DEV_002A&SUBSYS_663211AD
%ATHR.DeviceDesc.E01F105B% = ATHR_DEV_OS61_E01F105B.ndi, PCI\VEN_168C&DEV_002A&SUBSYS_03061A32
%ATHR.DeviceDesc.3067%     = ATHR_DEV_OS61_04281468.ndi, PCI\VEN_168C&DEV_001C&SUBSYS_01081A32   
%ATHR.DeviceDesc.3067%     = ATHR_DEV_OS61_04281468.ndi, PCI\VEN_168C&DEV_001C&SUBSYS_04281468
%ATHR.DeviceDesc.3067%     = ATHR_DEV_OS61_04281468.ndi, PCI\VEN_168C&DEV_001C&SUBSYS_E008105B
%ATHR.DeviceDesc.3067%     = ATHR_DEV_OS61_04281468.ndi, PCI\VEN_168C&DEV_001C&SUBSYS_E00D105B
%ATHR.DeviceDesc.663111AD% = ATHR_DEV_OS61_E016105B.ndi, PCI\VEN_168C&DEV_002B&SUBSYS_663111AD
%ATHR.DeviceDesc.3067%     = ATHR_DEV_OS61_04281468.ndi, PCI\VEN_168C&DEV_001C&SUBSYS_635311AD
%ATHR.DeviceDesc.3067%     = ATHR_DEV_OS61_04281468.ndi, PCI\VEN_168C&DEV_001C&SUBSYS_660311AD
%ATHR.DeviceDesc.663111AD% = ATHR_DEV_OS61_E016105B.ndi, PCI\VEN_168C&DEV_002B&SUBSYS_E016105B
%ATHR.DeviceDesc.663111AD% = ATHR_DEV_OS61_E016105B.ndi, PCI\VEN_168C&DEV_002B&SUBSYS_E022105B
%ATHR.DeviceDesc.E01F105B% = ATHR_DEV_OS61_E01F105B.ndi, PCI\VEN_168C&DEV_002A&SUBSYS_309D185F
%ATHR.DeviceDesc.E031105B% = ATHR_DEV_OS61_E031105Bw.ndi,PCI\VEN_168C&DEV_002B&SUBSYS_E031105B
%ATHR.DeviceDesc.660311AD% = ATHR_DEV_OS61_660311AD.ndi, PCI\VEN_168C&DEV_002E&SUBSYS_660311AD
%ATHR.DeviceDesc.660311AD% = ATHR_DEV_OS61_660311AD.ndi, PCI\VEN_168C&DEV_002E&SUBSYS_23091A32
%ATHR.DeviceDesc.660311AD% = ATHR_DEV_OS61_660311AD.ndi, PCI\VEN_168C&DEV_002E&SUBSYS_E034105B
%ATHR.DeviceDesc.663111AD% = ATHR_DEV_OS61_E016105B.ndi, PCI\VEN_168C&DEV_002B&SUBSYS_23051A32
%ATHR.DeviceDesc.663111AD% = ATHR_DEV_OS61_E035105B.ndi, PCI\VEN_168C&DEV_002B&SUBSYS_E035105B
%ATHR.DeviceDesc.663111AD% = ATHR_DEV_OS61_E035105B.ndi, PCI\VEN_168C&DEV_002B&SUBSYS_664111AD
%ATHR.DeviceDesc.663111AD% = ATHR_DEV_OS61_E035105B.ndi, PCI\VEN_168C&DEV_002B&SUBSYS_63051A32
%ATHR.DeviceDesc.E01F105B% = ATHR_DEV_OS61_664211AD.ndi, PCI\VEN_168C&DEV_002A&SUBSYS_664211AD
%ATHR.DeviceDesc.660311AD% = ATHR_DEV_OS61_660311AD.ndi, PCI\VEN_168C&DEV_002E&SUBSYS_30B4185F
%ATHR.DeviceDesc.655211AD% = ATHR_DEV_OS61_655211AD.ndi, PCI\VEN_168C&DEV_002A&SUBSYS_655211AD
%ATHR.DeviceDesc.661711AD% = ATHR_DEV_OS61_661711AD.ndi, PCI\VEN_168C&DEV_0032&SUBSYS_661711AD
%ATHR.DeviceDesc.661711AD% = ATHR_DEV_OS61_661711AD.ndi, PCI\VEN_168C&DEV_0032&SUBSYS_E047105B
%ATHR.DeviceDesc.E04A105B% = ATHR_DEV_OS61_E04A105B.ndi, PCI\VEN_168C&DEV_0030&SUBSYS_E04A105B
%ATHR.DeviceDesc.661811AD% = ATHR_DEV_OS61_661811AD.ndi, PCI\VEN_168C&DEV_0032&SUBSYS_661811AD
%ATHR.DeviceDesc.661811AD% = ATHR_DEV_OS61_661811AD.ndi, PCI\VEN_168C&DEV_0032&SUBSYS_E04D105B
%ATHR.DeviceDesc.E051105B% = ATHR_DEV_OS61_661811AD.ndi, PCI\VEN_168C&DEV_0032&SUBSYS_E051105B
%ATHR.DeviceDesc.661711AD% = ATHR_DEV_OS61_661711AD.ndi, PCI\VEN_168C&DEV_0032&SUBSYS_A118185F
%ATHR.DeviceDesc.661711AD% = ATHR_DEV_OS61_661711AD.ndi, PCI\VEN_168C&DEV_0032&SUBSYS_663711AD
%ATHR.DeviceDesc.661711AD% = ATHR_DEV_OS61_661711AD.ndi, PCI\VEN_168C&DEV_0037&SUBSYS_663711AD
%ATHR.DeviceDesc.311711AD% = ATHR_DEV_OS61_311711AD.ndi, PCI\VEN_168C&DEV_0034&SUBSYS_662111AD
%ATHR.DeviceDesc.311711AD% = ATHR_DEV_OS61_311711AD.ndi, PCI\VEN_168C&DEV_0034&SUBSYS_E052105B
%ATHR.DeviceDesc.E059105B% = ATHR_DEV_OS61_311711AD.ndi, PCI\VEN_168C&DEV_0034&SUBSYS_E059105B
%ATHR.DeviceDesc.E059105B% = ATHR_DEV_OS61_311711AD.ndi, PCI\VEN_168C&DEV_0034&SUBSYS_E058105B
%ATHR.DeviceDesc.311711AD% = ATHR_DEV_OS61_311711AD.ndi, PCI\VEN_168C&DEV_0034&SUBSYS_211E1A3B
%ATHR.DeviceDesc.311711AD% = ATHR_DEV_OS61_311711AD.ndi, PCI\VEN_168C&DEV_0034&SUBSYS_E085105B
%ATHR.DeviceDesc.E086105B% = ATHR_DEV_OS61_E086105B.ndi, PCI\VEN_168C&DEV_0034&SUBSYS_E086105B
%ATHR.DeviceDesc.E059105B% = ATHR_DEV_OS61_311711AD.ndi, PCI\VEN_168C&DEV_0034&SUBSYS_E087105B
%ATHR.DeviceDesc.E068105B% = ATHR_DEV_OS61_ACER956x.ndi, PCI\VEN_168C&DEV_0036&SUBSYS_E068105B
%ATHR.DeviceDesc.956x%     = ATHR_DEV_OS61_ACER956x.ndi, PCI\VEN_168C&DEV_0036&SUBSYS_06B211AD
%ATHR.DeviceDesc.956x%     = ATHR_DEV_OS61_ACER956x.ndi, PCI\VEN_168C&DEV_0036&SUBSYS_A119185F
%ATHR.DeviceDesc.956x%     = ATHR_DEV_OS61_ACER956x.ndi, PCI\VEN_168C&DEV_0036&SUBSYS_063211AD
%ATHR.DeviceDesc.956x%     = ATHR_DEV_OS61_ACER956x.ndi, PCI\VEN_168C&DEV_0036&SUBSYS_667111AD
%ATHR.DeviceDesc.956x%     = ATHR_DEV_OS61_ACER_956x_CH2.ndi, PCI\VEN_168C&DEV_0036&SUBSYS_064211AD
%ATHR.DeviceDesc.956x%     = ATHR_DEV_OS61_A120185F.ndi, PCI\VEN_168C&DEV_0036&SUBSYS_A120185F
%ATHR.DeviceDesc.956x%     = ATHR_DEV_OS61_ACER_956x_CH2.ndi, PCI\VEN_168C&DEV_0036&SUBSYS_E07F105B
%ATHR.DeviceDesc.956x%     = ATHR_DEV_OS61_ACER_956x_CH2.ndi, PCI\VEN_168C&DEV_0036&SUBSYS_28131B9A
%ATHR.DeviceDesc.E086105B% = ATHR_DEV_OS61_080211AD.ndi, PCI\VEN_168C&DEV_0034&SUBSYS_E08C105B
%ATHR.DeviceDesc.956x%     = ATHR_DEV_OS61_ACER_A11_CH2.ndi, PCI\VEN_168C&DEV_0036&SUBSYS_080311AD
%ATHR.DeviceDesc.956x%     = ATHR_DEV_OS61_ACER_A11_CH2.ndi, PCI\VEN_168C&DEV_0036&SUBSYS_081311AD
%ATHR.DeviceDesc.956x%     = ATHR_DEV_OS61_ACER_A11_CH2.ndi, PCI\VEN_168C&DEV_0036&SUBSYS_E091105B 
%ATHR.DeviceDesc.956x%     = ATHR_DEV_OS61_218B1A3B.ndi, PCI\VEN_168C&DEV_0036&SUBSYS_218B1A3B
%ATHR.DeviceDesc.956x%     = ATHR_DEV_OS61_218B1A3B.ndi, PCI\VEN_168C&DEV_0036&SUBSYS_218C1A3B
; Toshiba
%ATHR.DeviceDesc.2041%     = ATHR_DEV_OS61_2041.ndi,     PCI\VEN_168C&DEV_0013&SUBSYS_7064144F
%ATHR.DeviceDesc.2042%     = ATHR_DEV_OS61_2042.ndi,     PCI\VEN_168C&DEV_0013&SUBSYS_7065144F
%ATHR.DeviceDesc.2051%     = ATHR_DEV_OS61_2051.ndi,     PCI\VEN_168C&DEV_0013&SUBSYS_7084144F
%ATHR.DeviceDesc.2051%     = ATHR_DEV_OS61_2051.ndi,     PCI\VEN_168C&DEV_0013&SUBSYS_7088144F
%ATHR.DeviceDesc.001B%     = ATHR_DEV_OS61_001B.ndi,     PCI\VEN_168C&DEV_001B&SUBSYS_7092144F
%ATHR.DeviceDesc.001A%     = ATHR_DEV_OS61_2054.ndi,     PCI\VEN_168C&DEV_001A&SUBSYS_7094144F
%ATHR.DeviceDesc.3063%     = ATHR_DEV_OS61_2063.ndi,     PCI\VEN_168C&DEV_001C&SUBSYS_7096144F
%ATHR.DeviceDesc.3065%     = ATHR_DEV_OS61_2052.ndi,     PCI\VEN_168C&DEV_001C&SUBSYS_7106144F
%ATHR.DeviceDesc.3067%     = ATHR_DEV_OS61_001C.ndi,     PCI\VEN_168C&DEV_001C&SUBSYS_7128144f
%ATHR.DeviceDesc.001A%     = ATHR_DEV_OS61_001A.ndi,     PCI\VEN_168C&DEV_001C&SUBSYS_04271468
%ATHR.DeviceDesc.001B%     = ATHR_DEV_OS61_001B.ndi,     PCI\VEN_168C&DEV_001C&SUBSYS_04251468
%ATHR.DeviceDesc.001A%     = ATHR_DEV_OS61_001A.ndi,     PCI\VEN_168C&DEV_001A&SUBSYS_04261468
%ATHR.DeviceDesc.3072%     = ATHR_DEV_OS61_7125144F.ndi, PCI\VEN_168C&DEV_0024&SUBSYS_7125144F
%ATHR.DeviceDesc.3067%     = ATHR_DEV_OS61_001C.ndi,     PCI\VEN_168C&DEV_001C&SUBSYS_042A1468
%ATHR.DeviceDesc.7136144F% = ATHR_DEV_OS61_7136144F.ndi, PCI\VEN_168C&DEV_002A&SUBSYS_E004105B
%ATHR.DeviceDesc.7141144F% = ATHR_DEV_OS61_7136144F.ndi, PCI\VEN_168C&DEV_002A&SUBSYS_E009105B
%ATHR.DeviceDesc.7136144F% = ATHR_DEV_OS61_7136144F.ndi, PCI\VEN_168C&DEV_002A&SUBSYS_7136144F
%ATHR.DeviceDesc.7136144F% = ATHR_DEV_OS61_7136144F.ndi, PCI\VEN_168C&DEV_002A&SUBSYS_7154144F
%ATHR.DeviceDesc.7141144F% = ATHR_DEV_OS61_7136144F.ndi, PCI\VEN_168C&DEV_002A&SUBSYS_7141144F
%ATHR.DeviceDesc.3067%     = ATHR_DEV_OS61_001C.ndi,     PCI\VEN_168C&DEV_001C&SUBSYS_41051A32
%ATHR.DeviceDesc.7141144F% = ATHR_DEV_OS61_7136144F.ndi, PCI\VEN_168C&DEV_002A&SUBSYS_43011A32  
%ATHR.DeviceDesc.7141144F% = ATHR_DEV_OS61_7136144F.ndi, PCI\VEN_168C&DEV_002A&SUBSYS_43031A32
%ATHR.DeviceDesc.7141144F% = ATHR_DEV_OS61_7136144F.ndi, PCI\VEN_168C&DEV_002A&SUBSYS_E012105B
%ATHR.DeviceDesc.7136144F% = ATHR_DEV_OS61_7136144F.ndi, PCI\VEN_168C&DEV_002A&SUBSYS_E013105B
%ATHR.DeviceDesc.7136144F% = ATHR_DEV_OS61_7136144F.ndi, PCI\VEN_168C&DEV_002A&SUBSYS_E015105B
%ATHR.DeviceDesc.30A1%     = ATHR_DEV_OS61_T30A1.ndi,    PCI\VEN_168C&DEV_002B&SUBSYS_E014105B
%ATHR.DeviceDesc.7141144F% = ATHR_DEV_OS61_7136144F.ndi, PCI\VEN_168C&DEV_002A&SUBSYS_7158144F
%ATHR.DeviceDesc.7136144F% = ATHR_DEV_OS61_7136144F.ndi, PCI\VEN_168C&DEV_002A&SUBSYS_7156144F
%ATHR.DeviceDesc.7136144F% = ATHR_DEV_OS61_7136144F.ndi, PCI\VEN_168C&DEV_002A&SUBSYS_7157144F
%ATHR.DeviceDesc.30A1%     = ATHR_DEV_OS61_T30A1.ndi,    PCI\VEN_168C&DEV_002B&SUBSYS_7159144F
%ATHR.DeviceDesc.3067%     = ATHR_DEV_OS61_001C.ndi,     PCI\VEN_168C&DEV_001C&SUBSYS_632311AD
%ATHR.DeviceDesc.7141144F% = ATHR_DEV_OS61_7136144F.ndi, PCI\VEN_168C&DEV_002A&SUBSYS_662011AD
%ATHR.DeviceDesc.7136144F% = ATHR_DEV_OS61_7136144F.ndi, PCI\VEN_168C&DEV_002A&SUBSYS_650211AD
%ATHR.DeviceDesc.7136144F% = ATHR_DEV_OS61_7136144F.ndi, PCI\VEN_168C&DEV_002A&SUBSYS_653211AD
%ATHR.DeviceDesc.7141144F% = ATHR_DEV_OS61_7136144F.ndi, PCI\VEN_168C&DEV_002A&SUBSYS_661011AD
%ATHR.DeviceDesc.7136144F% = ATHR_DEV_OS61_7136144F.ndi, PCI\VEN_168C&DEV_002A&SUBSYS_651211AD
%ATHR.DeviceDesc.7136144F% = ATHR_DEV_OS61_7136144F.ndi, PCI\VEN_168C&DEV_002A&SUBSYS_652211AD
%ATHR.DeviceDesc.30A1%     = ATHR_DEV_OS61_T30A1.ndi,    PCI\VEN_168C&DEV_002B&SUBSYS_661111AD
%ATHR.DeviceDesc.7163144F% = ATHR_DEV_OS61_7163144F.ndi, PCI\VEN_168C&DEV_002A&SUBSYS_661211AD
%ATHR.DeviceDesc.30A1%     = ATHR_DEV_OS61_T30A1.ndi,    PCI\VEN_168C&DEV_002B&SUBSYS_660111AD
%ATHR.DeviceDesc.7163144F% = ATHR_DEV_OS61_7163144F.ndi, PCI\VEN_168C&DEV_002A&SUBSYS_7163144F
%ATHR.DeviceDesc.30A1%     = ATHR_DEV_OS61_T30A1.ndi,    PCI\VEN_168C&DEV_002B&SUBSYS_7164144F
%ATHR.DeviceDesc.7163144F% = ATHR_DEV_OS61_7163144F.ndi, PCI\VEN_168C&DEV_002A&SUBSYS_E019105B
%ATHR.DeviceDesc.30A1%     = ATHR_DEV_OS61_T30A1.ndi,    PCI\VEN_168C&DEV_002B&SUBSYS_E01A105B
%ATHR.DeviceDesc.30A1%     = ATHR_DEV_OS61_T30A1.ndi,    PCI\VEN_168C&DEV_002B&SUBSYS_43051A32
%ATHR.DeviceDesc.7163144F% = ATHR_DEV_OS61_7163144F.ndi, PCI\VEN_168C&DEV_002A&SUBSYS_43061A32
%ATHR.DeviceDesc.3067%     = ATHR_DEV_OS61_001C.ndi,     PCI\VEN_168C&DEV_001C&SUBSYS_A6011113
%ATHR.DeviceDesc.30A1%     = ATHR_DEV_OS61_T30A1.ndi,    PCI\VEN_168C&DEV_002B&SUBSYS_E6111113
%ATHR.DeviceDesc.7141144F% = ATHR_DEV_OS61_7136144F.ndi, PCI\VEN_168C&DEV_002A&SUBSYS_E6221113
%ATHR.DeviceDesc.7136144F% = ATHR_DEV_OS61_7136144F.ndi, PCI\VEN_168C&DEV_002A&SUBSYS_D6221113
%ATHR.DeviceDesc.30A1%     = ATHR_DEV_OS61_T30A1.ndi,    PCI\VEN_168C&DEV_002B&SUBSYS_E8111113
%ATHR.DeviceDesc.7163144F% = ATHR_DEV_OS61_7163144F.ndi, PCI\VEN_168C&DEV_002A&SUBSYS_F8221113
%ATHR.DeviceDesc.7136144F% = ATHR_DEV_OS61_7136144F.ndi, PCI\VEN_168C&DEV_002A&SUBSYS_A8221113
%ATHR.DeviceDesc.7136144F% = ATHR_DEV_OS61_7136144F.ndi, PCI\VEN_168C&DEV_002A&SUBSYS_B8221113
%ATHR.DeviceDesc.7136144F% = ATHR_DEV_OS61_7136144F.ndi, PCI\VEN_168C&DEV_002A&SUBSYS_45071A32
%ATHR.DeviceDesc.7136144F% = ATHR_DEV_OS61_7136144F.ndi, PCI\VEN_168C&DEV_002A&SUBSYS_65071A32
%ATHR.DeviceDesc.30A4%     = ATHR_DEV_OS61_T30A4.ndi,    PCI\VEN_168C&DEV_002E&SUBSYS_43091A32
%ATHR.DeviceDesc.30ABLT%   = ATHR_DEV_OS61_7173144Fw.ndi,PCI\VEN_168C&DEV_002B&SUBSYS_7173144F
%ATHR.DeviceDesc.30ABLT%   = ATHR_DEV_OS61_7173144Fw.ndi,PCI\VEN_168C&DEV_002B&SUBSYS_661311AD
%ATHR.DeviceDesc.30ABLT%   = ATHR_DEV_OS61_7173144Fw.ndi,PCI\VEN_168C&DEV_002B&SUBSYS_10001B14
%ATHR.DeviceDesc.938x%     = ATHR_DEV_OS61_T938x.ndi,    PCI\VEN_168C&DEV_0030&SUBSYS_7188144F
%ATHR.DeviceDesc.938x%     = ATHR_DEV_OS61_T938x.ndi,    PCI\VEN_168C&DEV_0030&SUBSYS_650311AD
%ATHR.DeviceDesc.30ABLT%   = ATHR_DEV_OS61_7173144Fw.ndi,PCI\VEN_168C&DEV_002B&SUBSYS_EE321113
%ATHR.DeviceDesc.9485%     = ATHR_DEV_OS61_T9485.ndi,    PCI\VEN_168C&DEV_0032&SUBSYS_660711AD
%ATHR.DeviceDesc.3119%     = ATHR_DEV_OS61_T3119.ndi,    PCI\VEN_168C&DEV_0032&SUBSYS_660811AD
%ATHR.DeviceDesc.9485%     = ATHR_DEV_OS61_T9485.ndi,    PCI\VEN_168C&DEV_0032&SUBSYS_7192144F
%ATHR.DeviceDesc.3119%     = ATHR_DEV_OS61_T3119.ndi,    PCI\VEN_168C&DEV_0032&SUBSYS_7193144F
%ATHR.DeviceDesc.9485%     = ATHR_DEV_OS61_T9485.ndi,    PCI\VEN_168C&DEV_0032&SUBSYS_B8411113
%ATHR.DeviceDesc.3119%     = ATHR_DEV_OS61_T3119.ndi,    PCI\VEN_168C&DEV_0032&SUBSYS_B8421113
%ATHR.DeviceDesc.9485%     = ATHR_DEV_OS61_T9485.ndi,    PCI\VEN_168C&DEV_0032&SUBSYS_43181A32
%ATHR.DeviceDesc.30A1%     = ATHR_DEV_OS61_T30A1.ndi,    PCI\VEN_168C&DEV_002B&SUBSYS_7194144F
%ATHR.DeviceDesc.946x%     = ATHR_DEV_OS61_T946x.ndi,    PCI\VEN_168C&DEV_0034&SUBSYS_7055144F
%ATHR.DeviceDesc.946x%     = ATHR_DEV_OS61_T946x.ndi,    PCI\VEN_168C&DEV_0034&SUBSYS_661111AD
%ATHR.DeviceDesc.946x%     = ATHR_DEV_OS61_T946x.ndi,    PCI\VEN_168C&DEV_0034&SUBSYS_2C001B9A
%ATHR.DeviceDesc.956x%     = ATHR_DEV_OS61_T956x.ndi,    PCI\VEN_168C&DEV_0036&SUBSYS_061211AD
%ATHR.DeviceDesc.956x%     = ATHR_DEV_OS61_T956x.ndi,    PCI\VEN_168C&DEV_0036&SUBSYS_7202144F
%ATHR.DeviceDesc.956x%     = ATHR_DEV_OS61_T956x.ndi,    PCI\VEN_168C&DEV_0036&SUBSYS_28101B9A
%ATHR.DeviceDesc.956x%     = ATHR_DEV_OS61_T956x.ndi,    PCI\VEN_168C&DEV_0036&SUBSYS_28A21B9A
%ATHR.DeviceDesc.956x%     = ATHR_DEV_OS61_21821A3B.ndi, PCI\VEN_168C&DEV_0036&SUBSYS_21821A3B
%ATHR.DeviceDesc.956x%     = ATHR_DEV_OS61_T956x_1.ndi,  PCI\VEN_168C&DEV_0036&SUBSYS_28A11B9A
%ATHR.DeviceDesc.956x%     = ATHR_DEV_OS61_T956x_1.ndi,  PCI\VEN_168C&DEV_0036&SUBSYS_218A1A3B
%ATHR.DeviceDesc.956x%     = ATHR_DEV_OS61_T956x.ndi,    PCI\VEN_168C&DEV_0036&SUBSYS_083211AD
%ATHR.DeviceDesc.956x%     = ATHR_DEV_OS61_T956x_1.ndi,  PCI\VEN_168C&DEV_0036&SUBSYS_084211AD
%ATHR.DeviceDesc.946x%     = ATHR_DEV_OS61_T946x.ndi,    PCI\VEN_168C&DEV_0034&SUBSYS_802A11AD
%ATHR.DeviceDesc.946x%     = ATHR_DEV_OS61_T946x.ndi,    PCI\VEN_168C&DEV_0034&SUBSYS_2C031B9A
%ATHR.DeviceDesc.946x%     = ATHR_DEV_OS61_T946x.ndi,    PCI\VEN_168C&DEV_0034&SUBSYS_21851A3B
%ATHR.DeviceDesc.946x%     = ATHR_DEV_OS61_T946x.ndi,	 PCI\VEN_168C&DEV_0034&SUBSYS_2F851A3B
%ATHR.DeviceDesc.956x%     = ATHR_DEV_OS61_21821A3B.ndi, PCI\VEN_168C&DEV_0036&SUBSYS_2F821A3B
%ATHR.DeviceDesc.956x%     = ATHR_DEV_OS61_T956x_1.ndi,	 PCI\VEN_168C&DEV_0036&SUBSYS_218A1A3B
%ATHR.DeviceDesc.956x%     = ATHR_DEV_OS61_T956x_1.ndi,	 PCI\VEN_168C&DEV_0036&SUBSYS_2F8A1A3B
%ATHR.DeviceDesc.946x%     = ATHR_DEV_OS61_T946x.ndi,	 PCI\VEN_168C&DEV_0034&SUBSYS_2C041B9A
%ATHR.DeviceDesc.956x%     = ATHR_DEV_OS61_T956x.ndi,	 PCI\VEN_168C&DEV_0036&SUBSYS_28A41B9A
%ATHR.DeviceDesc.956x%     = ATHR_DEV_OS61_T956x_1.ndi,	 PCI\VEN_168C&DEV_0036&SUBSYS_28A31B9A
%ATHR.DeviceDesc.9485%     = ATHR_DEV_OS61_T9485.ndi,    PCI\VEN_168C&DEV_0032&SUBSYS_863111AD
%ATHR.DeviceDesc.9485%     = ATHR_DEV_OS61_T9485.ndi,    PCI\VEN_168C&DEV_0032&SUBSYS_862111AD
%ATHR.DeviceDesc.9485%     = ATHR_DEV_OS61_T9485.ndi,    PCI\VEN_168C&DEV_0032&SUBSYS_861111AD  
%ATHR.DeviceDesc.956x%     = ATHR_DEV_OS61_T956x.ndi,    PCI\VEN_168C&DEV_0036&SUBSYS_183211AD
%ATHR.DeviceDesc.956x%     = ATHR_DEV_OS61_T956x_1.ndi,  PCI\VEN_168C&DEV_0036&SUBSYS_184211AD
%ATHR.DeviceDesc.946x%     = ATHR_DEV_OS61_T946x.ndi,    PCI\VEN_168C&DEV_0034&SUBSYS_812A11AD
%ATHR.DeviceDesc.9485%     = ATHR_DEV_OS61_T9485.ndi,    PCI\VEN_168C&DEV_0032&SUBSYS_21871A3B
%ATHR.DeviceDesc.9485%     = ATHR_DEV_OS61_T9485.ndi,    PCI\VEN_168C&DEV_0032&SUBSYS_2F871A3B
%ATHR.DeviceDesc.9485%     = ATHR_DEV_OS61_T9485.ndi,    PCI\VEN_168C&DEV_0032&SUBSYS_2A871A3B
%ATHR.DeviceDesc.9485%     = ATHR_DEV_OS61_T9485.ndi,    PCI\VEN_168C&DEV_0032&SUBSYS_2B871A3B
%ATHR.DeviceDesc.9485%     = ATHR_DEV_OS61_T9485.ndi,    PCI\VEN_168C&DEV_0032&SUBSYS_860111AD
; Sony
%ATHR.DeviceDesc.3091%     = ATHR_DEV_OS61_E007105B.ndi, PCI\VEN_168C&DEV_002A&SUBSYS_E007105B
%ATHR.DeviceDesc.04231468% = ATHR_DEV_OS61_E000105B.ndi, PCI\VEN_168C&DEV_001C&SUBSYS_E000105B
%ATHR.DeviceDesc.04231468% = ATHR_DEV_OS61_E002105B.ndi, PCI\VEN_168C&DEV_001C&SUBSYS_E002105B
%ATHR.DeviceDesc.04061468% = ATHR_DEV_OS61_04061468.ndi, PCI\VEN_168C&DEV_0013&SUBSYS_04061468
%ATHR.DeviceDesc.04071468% = ATHR_DEV_OS61_04061468.ndi, PCI\VEN_168C&DEV_0013&SUBSYS_04071468 
%ATHR.DeviceDesc.04231468% = ATHR_DEV_OS61_04231468.ndi, PCI\VEN_168C&DEV_001C&SUBSYS_04231468 
%ATHR.DeviceDesc.04231468% = ATHR_DEV_OS61_04231468.ndi, PCI\VEN_168C&DEV_001C&SUBSYS_0423168C
%ATHR.DeviceDesc.30A1%     = ATHR_DEV_OS61_S30A1.ndi,    PCI\VEN_168C&DEV_002B&SUBSYS_E017105B
%ATHR.DeviceDesc.30A4%     = ATHR_DEV_OS61_SS30A1.ndi,   PCI\VEN_168C&DEV_002E&SUBSYS_E030105B
%ATHR.DeviceDesc.30A1%     = ATHR_DEV_OS61_S30A1w.ndi,   PCI\VEN_168C&DEV_002B&SUBSYS_E037105B
%ATHR.DeviceDesc.3119%     = ATHR_DEV_OS61_S3119.ndi,    PCI\VEN_168C&DEV_0032&SUBSYS_E044105B
%ATHR.DeviceDesc.956x%     = ATHR_DEV_OS61_956x.ndi,     PCI\VEN_168C&DEV_0036&SUBSYS_E069105B
%ATHR.DeviceDesc.946x%     = ATHR_DEV_OS61_3117104D.ndi, PCI\VEN_168C&DEV_0034&SUBSYS_3117104D
%ATHR.DeviceDesc.956x%     = ATHR_DEV_OS61_956xv.ndi,    PCI\VEN_168C&DEV_0036&SUBSYS_E081105B
; HP Desktop
%ATHR.DeviceDesc.2A5F103C% = ATHR_DEV_OS61_2A5F103C.ndi, PCI\VEN_168C&DEV_0024&SUBSYS_2A5F103C
%ATHR.DeviceDesc.500011AD% = ATHR_DEV_OS61_11AD.ndi,     PCI\VEN_168C&DEV_001B&SUBSYS_500011AD
%ATHR.DeviceDesc.500111AD% = ATHR_DEV_OS61_11AD.ndi,     PCI\VEN_168C&DEV_001B&SUBSYS_500111AD
%ATHR.DeviceDesc.1000168c% = ATHR_DEV_OS61_1000168C.ndi, PCI\VEN_168C&DEV_002A&SUBSYS_1000168C
%ATHR.DeviceDesc.1000168c% = ATHR_DEV_OS61_1001168C.ndi, PCI\VEN_168C&DEV_002A&SUBSYS_1001168C
; HP LT
%ATHR.DeviceDesc.30ABLT%   = ATHR_DEV_OS61_30ABLT.ndi,   PCI\VEN_168C&DEV_002B&SUBSYS_30AB1895
%ATHR.DeviceDesc.30A1%     = ATHR_DEV_OS61_30A1LT.ndi,   PCI\VEN_168C&DEV_002B&SUBSYS_30A11895
; HP laptop
%ATHR.DeviceDesc.H3067%    = ATHR_DEV_OS61_H001C.ndi,    PCI\VEN_168C&DEV_001C&SUBSYS_303F103C
%ATHR.DeviceDesc.H3067%    = ATHR_DEV_OS61_H001C.ndi,    PCI\VEN_168C&DEV_001C&SUBSYS_3040103C
%ATHR.DeviceDesc.H3067%    = ATHR_DEV_OS61_H001C.ndi,    PCI\VEN_168C&DEV_001C&SUBSYS_137A103C
%ATHR.DeviceDesc.H3067%    = ATHR_DEV_OS61_H001C.ndi,    PCI\VEN_168C&DEV_001C&SUBSYS_137B103C
%ATHR.DeviceDesc.H2063%    = ATHR_DEV_OS61_H2063.ndi,    PCI\VEN_168C&DEV_001C&SUBSYS_1385103C
%ATHR.DeviceDesc.H2063%    = ATHR_DEV_OS61_H2063.ndi,    PCI\VEN_168C&DEV_001C&SUBSYS_1386103C
%ATHR.DeviceDesc.H3096%    = ATHR_DEV_OS61_H002A.ndi,    PCI\VEN_168C&DEV_002A&SUBSYS_1381103C
%ATHR.DeviceDesc.H3096%    = ATHR_DEV_OS61_H002A.ndi,    PCI\VEN_168C&DEV_002A&SUBSYS_1382103C
%ATHR.DeviceDesc.H3096%    = ATHR_DEV_OS61_H002A.ndi,    PCI\VEN_168C&DEV_002A&SUBSYS_3041103C
%ATHR.DeviceDesc.H3096%    = ATHR_DEV_OS61_H002A.ndi,    PCI\VEN_168C&DEV_002A&SUBSYS_3042103C
%ATHR.DeviceDesc.H30A1%    = ATHR_DEV_OS61_H30A1.ndi,    PCI\VEN_168C&DEV_002B&SUBSYS_303F103C
%ATHR.DeviceDesc.H30A1%    = ATHR_DEV_OS61_H30A1.ndi,    PCI\VEN_168C&DEV_002B&SUBSYS_3040103C
%ATHR.DeviceDesc.H30AB%    = ATHR_DEV_OS61_H30AB.ndi,    PCI\VEN_168C&DEV_002B&SUBSYS_1461103C
%ATHR.DeviceDesc.H30A4%    = ATHR_DEV_OS61_H30A4.ndi,    PCI\VEN_168C&DEV_002E&SUBSYS_1462103C
%ATHR.DeviceDesc.H3197%    = ATHR_DEV_OS61_H3197.ndi,    PCI\VEN_168C&DEV_002E&SUBSYS_1626103C
%ATHR.DeviceDesc.H3116%    = ATHR_DEV_OS61_H3116.ndi,    PCI\VEN_168C&DEV_0030&SUBSYS_1628103C
%ATHR.DeviceDesc.H3112%    = ATHR_DEV_OS61_H3112.ndi,    PCI\VEN_168C&DEV_0030&SUBSYS_1627103C
%ATHR.DeviceDesc.H3119%    = ATHR_DEV_OS61_H3119.ndi,    PCI\VEN_168C&DEV_0032&SUBSYS_1785103C
%ATHR.DeviceDesc.H3119%    = ATHR_DEV_OS61_H3119.ndi,    PCI\VEN_168C&DEV_0032&SUBSYS_179F103C
%ATHR.DeviceDesc.H3118%    = ATHR_DEV_OS61_H3118.ndi,    PCI\VEN_168C&DEV_0032&SUBSYS_1838103C
%ATHR.DeviceDesc.H3118%    = ATHR_DEV_OS61_H3118.ndi,    PCI\VEN_168C&DEV_0032&SUBSYS_2B32103C
%ATHR.DeviceDesc.H3118%    = ATHR_DEV_OS61_H3118.ndi,    PCI\VEN_168C&DEV_0032&SUBSYS_2B33103C
%ATHR.DeviceDesc.H3118%    = ATHR_DEV_OS61_H3118.ndi,    PCI\VEN_168C&DEV_0032&SUBSYS_191A103C
%ATHR.DeviceDesc.H3335%    = ATHR_DEV_OS61_H3335.ndi,    PCI\VEN_168C&DEV_0034&SUBSYS_1864103C
%ATHR.DeviceDesc.H9565%    = ATHR_DEV_OS61_H9565.ndi,    PCI\VEN_168C&DEV_0036&SUBSYS_18E3103C
%ATHR.DeviceDesc.H9565%    = ATHR_DEV_OS61_H9565.ndi,    PCI\VEN_168C&DEV_0036&SUBSYS_217F103C
%ATHR.DeviceDesc.H9565%    = ATHR_DEV_OS61_HNFA335.ndi,  PCI\VEN_168C&DEV_0036&SUBSYS_2005103C
; Asus
%ATHR.DeviceDesc.3062%     = ATHR_DEV_OS61_2062.ndi,     PCI\VEN_168C&DEV_001C&SUBSYS_7112144f
%ATHR.DeviceDesc.3091%     = ATHR_DEV_OS61_3091.ndi,     PCI\VEN_168C&DEV_002A&SUBSYS_7137144F
%ATHR.DeviceDesc.3072%     = ATHR_DEV_OS61_3072.ndi,     PCI\VEN_168C&DEV_0024&SUBSYS_7122144F
%ATHR.DeviceDesc.3072%     = ATHR_DEV_OS61_1071.ndi,     PCI\VEN_168C&DEV_0024&SUBSYS_7132144F
%ATHR.DeviceDesc.3072%     = ATHR_DEV_OS61_1071.ndi,     PCI\VEN_168C&DEV_0024&SUBSYS_2072144F
%ATHR.DeviceDesc.30A1%     = ATHR_DEV_OS61_10891A3B.ndi, PCI\VEN_168C&DEV_002B&SUBSYS_7182144F
%ATHR.DeviceDesc.30A1%     = ATHR_DEV_OS61_10891A3B.ndi, PCI\VEN_168C&DEV_002B&SUBSYS_7183144F
%ATHR.DeviceDesc.30A1%     = ATHR_DEV_OS61_10891A3B.ndi, PCI\VEN_168C&DEV_002B&SUBSYS_A0111113
%ATHR.DeviceDesc.30A1%     = ATHR_DEV_OS61_1A891A3B.ndi, PCI\VEN_168C&DEV_002B&SUBSYS_A8311113
%ATHR.DeviceDesc.30ABLT%   = ATHR_DEV_OS61_30AB2C37.ndi, PCI\VEN_168C&DEV_002B&SUBSYS_A8421113
%ATHR.DeviceDesc.2A371A3B% = ATHR_DEV_OS61_2A371A3B.ndi, PCI\VEN_168C&DEV_002B&SUBSYS_A8411113
%ATHR.DeviceDesc.30A1%     = ATHR_DEV_OS61_10891A3B.ndi, PCI\VEN_168C&DEV_002B&SUBSYS_E049105B
%ATHR.DeviceDesc.30ABLT%   = ATHR_DEV_OS61_30AB2C37.ndi, PCI\VEN_168C&DEV_002B&SUBSYS_E048105B
%ATHR.DeviceDesc.30A1%     = ATHR_DEV_OS61_10891A3B.ndi, PCI\VEN_168C&DEV_002B&SUBSYS_666111AD
%ATHR.DeviceDesc.30ABLT%   = ATHR_DEV_OS61_30AB2C37.ndi, PCI\VEN_168C&DEV_002B&SUBSYS_662311AD
%ATHR.DeviceDesc.30A1%     = ATHR_DEV_OS61_10891A3B.ndi, PCI\VEN_168C&DEV_002B&SUBSYS_E03E105B
%ATHR.DeviceDesc.9485%     = ATHR_DEV_OS61_11861A3B_1.ndi, PCI\VEN_168C&DEV_0032&SUBSYS_E04E105B
%ATHR.DeviceDesc.9485%     = ATHR_DEV_OS61_850D1043.ndi, PCI\VEN_168C&DEV_0032&SUBSYS_850D1043
%ATHR.DeviceDesc.3119%     = ATHR_DEV_OS61_2C971A3B_1.ndi, PCI\VEN_168C&DEV_0032&SUBSYS_E04F105B
%ATHR.DeviceDesc.3119%     = ATHR_DEV_OS61_2C971A3B_1.ndi, PCI\VEN_168C&DEV_0032&SUBSYS_7197144F
%ATHR.DeviceDesc.946x%     = ATHR_DEV_OS61_850E1043.ndi, PCI\VEN_168C&DEV_0034&SUBSYS_850E1043
%ATHR.DeviceDesc.946x%     = ATHR_DEV_OS61_21161A3B.ndi, PCI\VEN_168C&DEV_0034&SUBSYS_21161A3B
%ATHR.DeviceDesc.946x%     = ATHR_DEV_OS61_WB222SB_BTC.ndi,  PCI\VEN_168C&DEV_0034&SUBSYS_22081A3B
%ATHR.DeviceDesc.946x%     = ATHR_DEV_OS61_WB222SB.ndi,  PCI\VEN_168C&DEV_0034&SUBSYS_22341A3B
%ATHR.DeviceDesc.3119%     = ATHR_DEV_OS61_CUS198_1.ndi, PCI\VEN_168C&DEV_0032&SUBSYS_E075105B
%ATHR.DeviceDesc.3119%     = ATHR_DEV_OS61_CUS198_1.ndi, PCI\VEN_168C&DEV_0032&SUBSYS_21521A3B
%ATHR.DeviceDesc.956x%     = ATHR_DEV_OS61_21301A3B_WoW.ndi, PCI\VEN_168C&DEV_0036&SUBSYS_21301A3B
%ATHR.DeviceDesc.956x%     = ATHR_DEV_OS61_218D1A3B.ndi, PCI\VEN_168C&DEV_0036&SUBSYS_066211AD
%ATHR.DeviceDesc.956x%     = ATHR_DEV_OS61_21761A3B.ndi, PCI\VEN_168C&DEV_0036&SUBSYS_21761A3B
%ATHR.DeviceDesc.956x%     = ATHR_DEV_OS61_213A1A3B.ndi, PCI\VEN_168C&DEV_0036&SUBSYS_213A1A3B
%ATHR.DeviceDesc.956x%     = ATHR_DEV_OS61_213C1A3B.ndi, PCI\VEN_168C&DEV_0036&SUBSYS_213C1A3B
%ATHR.DeviceDesc.3119%     = ATHR_DEV_OS61_CUS198_2.ndi, PCI\VEN_168C&DEV_0032&SUBSYS_126A1A3B
%ATHR.DeviceDesc.946x%     = ATHR_DEV_OS61_082211AD.ndi, PCI\VEN_168C&DEV_0034&SUBSYS_082211AD
%ATHR.DeviceDesc.9485%     = ATHR_DEV_OS61_11861A3B.ndi, PCI\VEN_168C&DEV_0032&SUBSYS_E080105B
%ATHR.DeviceDesc.956x%     = ATHR_DEV_OS61_213B1A3B.ndi, PCI\VEN_168C&DEV_0036&SUBSYS_213B1A3B
%ATHR.DeviceDesc.956x%     = ATHR_DEV_OS61_85F21043.ndi, PCI\VEN_168C&DEV_0036&SUBSYS_85F21043
%ATHR.DeviceDesc.9485%     = ATHR_DEV_OS61_11861A3B.ndi, PCI\VEN_168C&DEV_0032&SUBSYS_665711AD
%ATHR.DeviceDesc.946x%     = ATHR_DEV_OS61_082211AD.ndi, PCI\VEN_168C&DEV_0034&SUBSYS_086211AD
%ATHR.DeviceDesc.956x%     = ATHR_DEV_OS61_E08F105B.ndi, PCI\VEN_168C&DEV_0036&SUBSYS_E08F105B
%ATHR.DeviceDesc.956x%     = ATHR_DEV_OS61_21301A3B_WoW.ndi, PCI\VEN_168C&DEV_0036&SUBSYS_E099105B
%ATHR.DeviceDesc.956x%     = ATHR_DEV_OS61_218D1A3B.ndi, PCI\VEN_168C&DEV_0036&SUBSYS_218D1A3B
; Sharp(Mitac)
%ATHR.DeviceDesc.3091%     = ATHR_DEV_OS61_3091.ndi,     PCI\VEN_168C&DEV_002A&SUBSYS_7138144F 
%ATHR.DeviceDesc.3091%     = ATHR_DEV_OS61_3091.ndi,     PCI\VEN_168C&DEV_002A&SUBSYS_7139144F
%ATHR.DeviceDesc.3091%     = ATHR_DEV_OS61_3091.ndi,     PCI\VEN_168C&DEV_002A&SUBSYS_7140144F 
; Fujitsu
%ATHR.DeviceDesc.3072%     = ATHR_DEV_OS61_13C010CF.ndi, PCI\VEN_168C&DEV_0024&SUBSYS_13C010CF
%ATHR.DeviceDesc.3091%     = ATHR_DEV_OS61_147C10CF.ndi, PCI\VEN_168C&DEV_002A&SUBSYS_147C10CF
%ATHR.DeviceDesc.3091%     = ATHR_DEV_OS61_147D10CF.ndi, PCI\VEN_168C&DEV_002A&SUBSYS_147D10CF
%ATHR.DeviceDesc.1071%     = ATHR_DEV_OS61_13C010CF.ndi, PCI\VEN_168C&DEV_0023&SUBSYS_147E10CF
%ATHR.DeviceDesc.0013%     = ATHR_DEV_OS61_F013.ndi,     PCI\VEN_168C&DEV_0013&SUBSYS_123410CF
%ATHR.DeviceDesc.0013%     = ATHR_DEV_OS61_F013.ndi,     PCI\VEN_168C&DEV_0013&SUBSYS_123510CF
%ATHR.DeviceDesc.10CF%     = ATHR_DEV_OS61_F013.ndi,     PCI\VEN_168C&DEV_0013&SUBSYS_123610CF
%ATHR.DeviceDesc.001B%     = ATHR_DEV_OS61_F013.ndi,     PCI\VEN_168C&DEV_001B&SUBSYS_132910CF
%ATHR.DeviceDesc.10CF%     = ATHR_DEV_OS61_F013.ndi,     PCI\VEN_168C&DEV_001B&SUBSYS_134F10CF
%ATHR.DeviceDesc.3062%     = ATHR_DEV_OS61_F013C.ndi,    PCI\VEN_168C&DEV_001C&SUBSYS_139C10CF
%ATHR.DeviceDesc.3067%     = ATHR_DEV_OS61_F01C.ndi,     PCI\VEN_168C&DEV_001C&SUBSYS_142E10CF
%ATHR.DeviceDesc.30A1%     = ATHR_DEV_OS61_153710CF.ndi, PCI\VEN_168C&DEV_002B&SUBSYS_153710CF
%ATHR.DeviceDesc.7163144F% = ATHR_DEV_OS61_147D10CF.ndi, PCI\VEN_168C&DEV_002A&SUBSYS_153610CF
%ATHR.DeviceDesc.30A4%     = ATHR_DEV_OS61_158F10CF.ndi, PCI\VEN_168C&DEV_002E&SUBSYS_158F10CF
%ATHR.DeviceDesc.30ABLT%   = ATHR_DEV_OS61_161910CF.ndi, PCI\VEN_168C&DEV_002B&SUBSYS_161910CF
%ATHR.DeviceDesc.938x%     = ATHR_DEV_OS61_16A810CF.ndi, PCI\VEN_168C&DEV_0030&SUBSYS_16A810CF
%ATHR.DeviceDesc.946x%     = ATHR_DEV_OS61_178310CF.ndi, PCI\VEN_168C&DEV_0034&SUBSYS_178310CF
%ATHR.DeviceDesc.946x%     = ATHR_DEV_OS61_180E10CF.ndi, PCI\VEN_168C&DEV_0034&SUBSYS_180E10CF
%ATHR.DeviceDesc.946x%     = ATHR_DEV_OS61_180E10CF.ndi, PCI\VEN_168C&DEV_0034&SUBSYS_18CD10CF
; WNC
%ATHR.DeviceDesc.CM9%      = ATHR_DEV_OS61_2042.ndi,     PCI\VEN_168C&DEV_0013&SUBSYS_1012185F
%ATHR.DeviceDesc.30AB%     = ATHR_DEV_OS61_03051A32w.ndi,PCI\VEN_168C&DEV_002B&SUBSYS_30AE185F
%ATHR.DeviceDesc.30A1%     = ATHR_DEV_OS61_E016105B.ndi, PCI\VEN_168C&DEV_002B&SUBSYS_30A1185F
%ATHR.DeviceDesc.30A4%     = ATHR_DEV_OS61_03091A32.ndi, PCI\VEN_168C&DEV_002E&SUBSYS_30B3185F
%ATHR.DeviceDesc.3119%     = ATHR_DEV_OS61_3119185F.ndi, PCI\VEN_168C&DEV_0032&SUBSYS_3119185F
%ATHR.DeviceDesc.956x%     = ATHR_DEV_OS61_3027185F.ndi, PCI\VEN_168C&DEV_0036&SUBSYS_3027185F
%ATHR.DeviceDesc.956x%     = ATHR_DEV_OS61_956x.ndi,     PCI\VEN_168C&DEV_0036&SUBSYS_3028185F
; TPLINK
%ATHR.DeviceDesc.1ACE%     = ATHR_DEV_OS61_T3091.ndi,    PCI\VEN_168C&DEV_0029&SUBSYS_92231ACE
%ATHR.DeviceDesc.0300T%    = ATHR_DEV_OS61_30A4TP.ndi,   PCI\VEN_168C&DEV_002D&SUBSYS_0300168C
%ATHR.DeviceDesc.0301T%    = ATHR_DEV_OS61_30A4TP.ndi,   PCI\VEN_168C&DEV_002D&SUBSYS_0301168C
; Pegatron
%ATHR.DeviceDesc.00341B0A% = ATHR_DEV_OS61_3091.ndi,     PCI\VEN_168C&DEV_002A&SUBSYS_00341B0A
; Belkin
%ATHR.DeviceDesc.001A%     = ATHR_DEV_OS61_001A.ndi,     PCI\VEN_168C&DEV_001A&SUBSYS_701D1799
%ATHR.DeviceDesc.001A%     = ATHR_DEV_OS61_001A.ndi,     PCI\VEN_168C&DEV_001A&SUBSYS_700D1799
%ATHR.DeviceDesc.F6D3000%  = ATHR_DEV_OS61_0013.ndi,     PCI\VEN_168C&DEV_0013&SUBSYS_30001799
%ATHR.DeviceDesc.F6D3000%  = ATHR_DEV_OS61_001B.ndi,     PCI\VEN_168C&DEV_001B&SUBSYS_30001799
%ATHR.DeviceDesc.80111799% = ATHR_DEV_OS61_80111799.ndi, PCI\VEN_168C&DEV_0023&SUBSYS_80111799
; NEC 
%ATHR.DeviceDesc.3062%     = ATHR_DEV_OS61_N2062.ndi,    PCI\VEN_168C&DEV_001C&SUBSYS_102010E9
%ATHR.DeviceDesc.3062%     = ATHR_DEV_OS61_N2062.ndi,    PCI\VEN_168C&DEV_001C&SUBSYS_102510E9
%ATHR.DeviceDesc.3072%     = ATHR_DEV_OS61_N3072.ndi,    PCI\VEN_168C&DEV_0024&SUBSYS_102210E9
%ATHR.DeviceDesc.3072%     = ATHR_DEV_OS61_N3073.ndi,    PCI\VEN_168C&DEV_0024&SUBSYS_102610E9
%ATHR.DeviceDesc.30A1%     = ATHR_DEV_OS61_03051A32.ndi, PCI\VEN_168C&DEV_002B&SUBSYS_03051A32
%ATHR.DeviceDesc.30A1%     = ATHR_DEV_OS61_03051A32.ndi, PCI\VEN_168C&DEV_002B&SUBSYS_83051A32
%ATHR.DeviceDesc.938x%     = ATHR_DEV_OS61_651311AD.ndi, PCI\VEN_168C&DEV_0030&SUBSYS_05081A32
; IO Data
%ATHR.DeviceDesc.D05B10FC% = ATHR_DEV_OS61_D05B10FC.ndi, PCI\VEN_168C&DEV_0029&SUBSYS_D05B10FC
; SEMCO
%ATHR.DeviceDesc.30AB%     = ATHR_DEV_OS61_BA91167D.ndi, PCI\VEN_168C&DEV_002B&SUBSYS_BA91167D
; Dell LT
%ATHR.DeviceDesc.D3067%    = ATHR_DEV_OS61_02B0.ndi,     PCI\VEN_168C&DEV_001C&SUBSYS_02B01028
%ATHR.DeviceDesc.D3067%    = ATHR_DEV_OS61_02B0.ndi,     PCI\VEN_168C&DEV_001C&SUBSYS_02B11028
%ATHR.DeviceDesc.D3067%    = ATHR_DEV_OS61_02B0.ndi,     PCI\VEN_168C&DEV_001C&SUBSYS_02D61028
%ATHR.DeviceDesc.D3067%    = ATHR_DEV_OS61_D001C.ndi,    PCI\VEN_168C&DEV_001C&SUBSYS_0202168C
%ATHR.DeviceDesc.D30A1%    = ATHR_DEV_OS61_D30A1.ndi,    PCI\VEN_168C&DEV_002B&SUBSYS_0204168C
%ATHR.DeviceDesc.D30AB%    = ATHR_DEV_OS61_D30AB.ndi,    PCI\VEN_168C&DEV_002B&SUBSYS_0205168C
%ATHR.DeviceDesc.D30AB%    = ATHR_DEV_OS61_D30ABHZ.ndi,  PCI\VEN_168C&DEV_002B&SUBSYS_04641028
%ATHR.DeviceDesc.D30AB%    = ATHR_DEV_OS61_D30A1.ndi,    PCI\VEN_168C&DEV_002B&SUBSYS_30AF185F
%ATHR.DeviceDesc.D30AB%    = ATHR_DEV_OS61_D30A1.ndi,    PCI\VEN_168C&DEV_002B&SUBSYS_A3051A32
; Xavi 
%ATHR.DeviceDesc.30A1%     = ATHR_DEV_OS61_10891A3B.ndi, PCI\VEN_168C&DEV_002B&SUBSYS_04001B9A 
%ATHR.DeviceDesc.30A4%     = ATHR_DEV_OS61_03091A32.ndi, PCI\VEN_168C&DEV_002E&SUBSYS_08001B9A 
%ATHR.DeviceDesc.30ABLT%   = ATHR_DEV_OS61_30AB.ndi,     PCI\VEN_168C&DEV_002B&SUBSYS_0C001B9A 
%ATHR.DeviceDesc.30A1%     = ATHR_DEV_OS61_10891A3B.ndi, PCI\VEN_168C&DEV_002B&SUBSYS_04011B9A 
%ATHR.DeviceDesc.30A1%     = ATHR_DEV_OS61_10891A3B.ndi, PCI\VEN_168C&DEV_002B&SUBSYS_04021B9A 
%ATHR.DeviceDesc.30A1%     = ATHR_DEV_OS61_04031B9A.ndi, PCI\VEN_168C&DEV_002B&SUBSYS_04031B9A 
%ATHR.DeviceDesc.30A1%     = ATHR_DEV_OS61_10891A3B.ndi, PCI\VEN_168C&DEV_002B&SUBSYS_04101B9A 
%ATHR.DeviceDesc.30A1%     = ATHR_DEV_OS61_10891A3B.ndi, PCI\VEN_168C&DEV_002B&SUBSYS_04111B9A 
%ATHR.DeviceDesc.30A4%     = ATHR_DEV_OS61_03091A32.ndi, PCI\VEN_168C&DEV_002E&SUBSYS_08011B9A 
%ATHR.DeviceDesc.30A4%     = ATHR_DEV_OS61_03091A32.ndi, PCI\VEN_168C&DEV_002E&SUBSYS_08021B9A 
%ATHR.DeviceDesc.30ABLT%   = ATHR_DEV_OS61_30AB.ndi,     PCI\VEN_168C&DEV_002B&SUBSYS_0C011B9A 
%ATHR.DeviceDesc.30ABLT%   = ATHR_DEV_OS61_30AB.ndi,     PCI\VEN_168C&DEV_002B&SUBSYS_0C021B9A 
%ATHR.DeviceDesc.30ABLT%   = ATHR_DEV_OS61_30AB.ndi,     PCI\VEN_168C&DEV_002B&SUBSYS_0C031B9A
%ATHR.DeviceDesc.30ABLT%   = ATHR_DEV_OS61_30AB.ndi,     PCI\VEN_168C&DEV_002B&SUBSYS_0C041B9A
%ATHR.DeviceDesc.30ABLT%   = ATHR_DEV_OS61_30AB.ndi,     PCI\VEN_168C&DEV_002B&SUBSYS_0C051B9A
%ATHR.DeviceDesc.30ABLT%   = ATHR_DEV_OS61_30AB2C37.ndi, PCI\VEN_168C&DEV_002B&SUBSYS_0C101B9A
%ATHR.DeviceDesc.2A371A3B% = ATHR_DEV_OS61_2A371A3B.ndi, PCI\VEN_168C&DEV_002B&SUBSYS_0C111B9A
%ATHR.DeviceDesc.938x%     = ATHR_DEV_OS61_651311AD.ndi, PCI\VEN_168C&DEV_0030&SUBSYS_18001B9A
%ATHR.DeviceDesc.938x%     = ATHR_DEV_OS61_651311AD.ndi, PCI\VEN_168C&DEV_0030&SUBSYS_18011B9A
%ATHR.DeviceDesc.938x%     = ATHR_DEV_OS61_651311AD.ndi, PCI\VEN_168C&DEV_0030&SUBSYS_18021B9A
%ATHR.DeviceDesc.9485%     = ATHR_DEV_OS61_11861A3B_1.ndi, PCI\VEN_168C&DEV_0032&SUBSYS_1C001B9A
%ATHR.DeviceDesc.9485%     = ATHR_DEV_OS61_11861A3B_1.ndi, PCI\VEN_168C&DEV_0032&SUBSYS_1C011B9A
%ATHR.DeviceDesc.3119%     = ATHR_DEV_OS61_2C971A3B_1.ndi, PCI\VEN_168C&DEV_0032&SUBSYS_20001B9A
%ATHR.DeviceDesc.3119%     = ATHR_DEV_OS61_2C971A3B_1.ndi, PCI\VEN_168C&DEV_0032&SUBSYS_20011B9A
%ATHR.DeviceDesc.956x%     = ATHR_DEV_OS61_01186931_LED.ndi,   PCI\VEN_168C&DEV_0036&SUBSYS_28111B9A
%ATHR.DeviceDesc.956x%     = ATHR_DEV_OS61_01186931.ndi,   PCI\VEN_168C&DEV_0036&SUBSYS_28121B9A
; Via
%ATHR.DeviceDesc.3B001106% = ATHR_DEV_OS61_30A1.ndi,     PCI\VEN_168C&DEV_002B&SUBSYS_3B001106
; USI
%ATHR.DeviceDesc.946x%     = ATHR_DEV_OS61_946x.ndi,     PCI\VEN_168C&DEV_0034&SUBSYS_006314CD
%ATHR.DeviceDesc.946x%     = ATHR_DEV_OS61_946x.ndi,     PCI\VEN_168C&DEV_0034&SUBSYS_006414CD
; Compex
%ATHR.DeviceDesc.3091%     = ATHR_DEV_OS61_20001071.ndi, PCI\VEN_168C&DEV_002A&SUBSYS_20001071

[Gigabyte.NTamd64.6.2]
%GIGA.DeviceDesc.E801%     = GIGA_DEV_OS61_E801.ndi,     PCI\VEN_168C&DEV_0013&SUBSYS_E8011458
%GIGA.DeviceDesc.E811%     = GIGA_DEV_OS61_E811.ndi,     PCI\VEN_168C&DEV_0013&SUBSYS_E8111458
%GIGA.DeviceDesc.E814%     = GIGA_DEV_OS61_E814.ndi,     PCI\VEN_168C&DEV_0013&SUBSYS_E8141458
%GIGA.DeviceDesc.0013%     = GIGA_DEV_OS61_0013.ndi,     PCI\VEN_168C&DEV_0013&SUBSYS_E9011458
%GIGA.DeviceDesc.E901%     = GIGA_DEV_OS61_E901.ndi,     PCI\VEN_168C&DEV_001B&SUBSYS_E9011458
%GIGA.DeviceDesc.E911%     = GIGA_DEV_OS61_E911.ndi,     PCI\VEN_168C&DEV_0013&SUBSYS_E9111458
%GIGA.DeviceDesc.E912%     = GIGA_DEV_OS61_E912.ndi,     PCI\VEN_168C&DEV_0013&SUBSYS_E9121458
%GIGA.DeviceDesc.E913%     = GIGA_DEV_OS61_E913.ndi,     PCI\VEN_168C&DEV_001C&SUBSYS_E9131458
%GIGA.DeviceDesc.E917%     = GIGA_DEV_OS61_E917.ndi,     PCI\VEN_168C&DEV_001C&SUBSYS_E9171458
%GIGA.DeviceDesc.E815%     = GIGA_DEV_OS61_E914.ndi,     PCI\VEN_168C&DEV_0024&SUBSYS_E8151458
%GIGA.DeviceDesc.E914%     = GIGA_DEV_OS61_E914.ndi,     PCI\VEN_168C&DEV_0023&SUBSYS_E9141458
%GIGA.DeviceDesc.E915%     = GIGA_DEV_OS61_E914.ndi,     PCI\VEN_168C&DEV_0024&SUBSYS_E9151458
%GIGA.DeviceDesc.E916%     = GIGA_DEV_OS61_E916.ndi,     PCI\VEN_168C&DEV_0024&SUBSYS_E9161458
%GIGA.DeviceDesc.E918%     = GIGA_DEV_OS61_E918.ndi,     PCI\VEN_168C&DEV_001C&SUBSYS_E9181458
%GIGA.DeviceDesc.E9191458% = ATHR_DEV_OS61_03011A32.ndi, PCI\VEN_168C&DEV_002A&SUBSYS_E9191458 
; Chicony
%ATHR.DeviceDesc.946x%     = ATHR_DEV_OS61_Chicony_946x.ndi, PCI\VEN_168C&DEV_0034&SUBSYS_097517ED

;
; OS 6.1 Manufacturer section
;
[GIGA_DEV_OS61_E801.ndi.NTamd64]
Characteristics = 0x84
BusType         = 5
AddReg          = atheros_os61.reg, atheros.reg, customer_GigaByteLed0.reg
DelReg          = atheros.DelReg
CopyFiles       = atheros.CopyFiles
*IfType         = 71            ; IF_TYPE_IEEE80211
*MediaType      = 16            ; NdisMediumNative802_11
*PhysicalMediaType = 9          ; NdisPhysicalMediumNative802_11
Include         = netvwifibus.inf, machine.inf
Needs           = VWiFiBus.CopyFiles

[GIGA_DEV_OS61_E801.ndi.NTamd64.Services]
AddService = athr, 2, atheros.Service, atheros.EventLog
Include    = netvwifibus.inf
Needs      = VWiFiBus.Services

[GIGA_DEV_OS61_E801.ndi.NTamd64.HW]
Include = netvwifibus.inf
Needs   = VWiFiBus.PnPFilterRegistration

[GIGA_DEV_OS61_E811.ndi.NTamd64]
Characteristics = 0x84
BusType         = 5
AddReg          = atheros_os61.reg, atheros.reg, customer_GigaByteLed0.reg
DelReg          = atheros.DelReg
CopyFiles       = atheros.CopyFiles
*IfType         = 71            ; IF_TYPE_IEEE80211
*MediaType      = 16            ; NdisMediumNative802_11
*PhysicalMediaType = 9          ; NdisPhysicalMediumNative802_11
Include         = netvwifibus.inf, machine.inf
Needs           = VWiFiBus.CopyFiles

[GIGA_DEV_OS61_E811.ndi.NTamd64.Services]
AddService = athr, 2, atheros.Service, atheros.EventLog
Include    = netvwifibus.inf
Needs      = VWiFiBus.Services

[GIGA_DEV_OS61_E811.ndi.NTamd64.HW]
Include = netvwifibus.inf
Needs   = VWiFiBus.PnPFilterRegistration

[GIGA_DEV_OS61_E814.ndi.NTamd64]
Characteristics = 0x84
BusType         = 5
AddReg          = atheros_os61.reg, atheros.reg, customer_GigaByteLed0.reg
DelReg          = atheros.DelReg
CopyFiles       = atheros.CopyFiles
*IfType         = 71            ; IF_TYPE_IEEE80211
*MediaType      = 16            ; NdisMediumNative802_11
*PhysicalMediaType = 9          ; NdisPhysicalMediumNative802_11
Include         = netvwifibus.inf, machine.inf
Needs           = VWiFiBus.CopyFiles

[GIGA_DEV_OS61_E814.ndi.NTamd64.Services]
AddService = athr, 2, atheros.Service, atheros.EventLog
Include    = netvwifibus.inf
Needs      = VWiFiBus.Services

[GIGA_DEV_OS61_E814.ndi.NTamd64.HW]
Include = netvwifibus.inf
Needs   = VWiFiBus.PnPFilterRegistration

[GIGA_DEV_OS61_0013.ndi.NTamd64]
Characteristics = 0x84
BusType         = 5
AddReg          = atheros_os61.reg, atheros.reg, customer_GigaByteLed0.reg
DelReg          = atheros.DelReg
CopyFiles       = atheros.CopyFiles
*IfType         = 71            ; IF_TYPE_IEEE80211
*MediaType      = 16            ; NdisMediumNative802_11
*PhysicalMediaType = 9          ; NdisPhysicalMediumNative802_11
Include         = netvwifibus.inf, machine.inf
Needs           = VWiFiBus.CopyFiles

[GIGA_DEV_OS61_0013.ndi.NTamd64.Services]
AddService = athr, 2, atheros.Service, atheros.EventLog
Include    = netvwifibus.inf
Needs      = VWiFiBus.Services

[GIGA_DEV_OS61_0013.ndi.NTamd64.HW]
Include = netvwifibus.inf
Needs   = VWiFiBus.PnPFilterRegistration

[GIGA_DEV_OS61_E901.ndi.NTamd64]
Characteristics = 0x84
BusType         = 5
AddReg          = atheros_os61.reg, atheros.reg, customer_GigaByteLed0.reg
DelReg          = atheros.DelReg
CopyFiles       = atheros.CopyFiles
*IfType         = 71            ; IF_TYPE_IEEE80211
*MediaType      = 16            ; NdisMediumNative802_11
*PhysicalMediaType = 9          ; NdisPhysicalMediumNative802_11
Include         = netvwifibus.inf, machine.inf
Needs           = VWiFiBus.CopyFiles

[GIGA_DEV_OS61_E901.ndi.NTamd64.Services]
AddService = athr, 2, atheros.Service, atheros.EventLog
Include    = netvwifibus.inf
Needs      = VWiFiBus.Services

[GIGA_DEV_OS61_E901.ndi.NTamd64.HW]
Include = netvwifibus.inf
Needs   = VWiFiBus.PnPFilterRegistration

[GIGA_DEV_OS61_E911.ndi.NTamd64]
Characteristics = 0x84
BusType         = 5
AddReg          = atheros_os61.reg, atheros.reg, customer_GigaByteLed0.reg
DelReg          = atheros.DelReg
CopyFiles       = atheros.CopyFiles
*IfType         = 71            ; IF_TYPE_IEEE80211
*MediaType      = 16            ; NdisMediumNative802_11
*PhysicalMediaType = 9          ; NdisPhysicalMediumNative802_11
Include         = netvwifibus.inf, machine.inf
Needs           = VWiFiBus.CopyFiles

[GIGA_DEV_OS61_E911.ndi.NTamd64.Services]
AddService = athr, 2, atheros.Service, atheros.EventLog
Include    = netvwifibus.inf
Needs      = VWiFiBus.Services

[GIGA_DEV_OS61_E911.ndi.NTamd64.HW]
Include = netvwifibus.inf
Needs   = VWiFiBus.PnPFilterRegistration

[GIGA_DEV_OS61_E912.ndi.NTamd64]
Characteristics = 0x84
BusType         = 5
AddReg          = atheros_os61.reg, atheros.reg, customer_GigaByteLed0.reg
DelReg          = atheros.DelReg
CopyFiles       = atheros.CopyFiles
*IfType         = 71            ; IF_TYPE_IEEE80211
*MediaType      = 16            ; NdisMediumNative802_11
*PhysicalMediaType = 9          ; NdisPhysicalMediumNative802_11
Include         = netvwifibus.inf, machine.inf
Needs           = VWiFiBus.CopyFiles

[GIGA_DEV_OS61_E912.ndi.NTamd64.Services]
AddService = athr, 2, atheros.Service, atheros.EventLog
Include    = netvwifibus.inf
Needs      = VWiFiBus.Services

[GIGA_DEV_OS61_E912.ndi.NTamd64.HW]
Include = netvwifibus.inf
Needs   = VWiFiBus.PnPFilterRegistration

[GIGA_DEV_OS61_E913.ndi.NTamd64]
Characteristics = 0x84
BusType         = 5
AddReg          = atheros_os61.reg, atheros.reg, customer_GigaByteLed1.reg
DelReg          = atheros.DelReg
CopyFiles       = atheros.CopyFiles
*IfType         = 71            ; IF_TYPE_IEEE80211
*MediaType      = 16            ; NdisMediumNative802_11
*PhysicalMediaType = 9          ; NdisPhysicalMediumNative802_11
Include         = netvwifibus.inf, machine.inf
Needs           = VWiFiBus.CopyFiles

[GIGA_DEV_OS61_E913.ndi.NTamd64.Services]
AddService = athr, 2, atheros.Service, atheros.EventLog
Include    = netvwifibus.inf
Needs      = VWiFiBus.Services

[GIGA_DEV_OS61_E913.ndi.NTamd64.HW]
Include = netvwifibus.inf
Needs   = VWiFiBus.PnPFilterRegistration

[GIGA_DEV_OS61_E917.ndi.NTamd64]
Characteristics = 0x84
BusType         = 5
AddReg          = atheros_os61.reg, atheros.reg, customer_GigaByteLed1.reg
DelReg          = atheros.DelReg
CopyFiles       = atheros.CopyFiles
*IfType         = 71            ; IF_TYPE_IEEE80211
*MediaType      = 16            ; NdisMediumNative802_11
*PhysicalMediaType = 9          ; NdisPhysicalMediumNative802_11
Include         = netvwifibus.inf, machine.inf
Needs           = VWiFiBus.CopyFiles

[GIGA_DEV_OS61_E917.ndi.NTamd64.Services]
AddService = athr, 2, atheros.Service, atheros.EventLog
Include    = netvwifibus.inf
Needs      = VWiFiBus.Services

[GIGA_DEV_OS61_E917.ndi.NTamd64.HW]
Include = netvwifibus.inf
Needs   = VWiFiBus.PnPFilterRegistration

[GIGA_DEV_OS61_E918.ndi.NTamd64]
Characteristics = 0x84
BusType         = 5
AddReg          = atheros_os61.reg, atheros.reg, customer_GigaByteLed2.reg
DelReg          = atheros.DelReg
CopyFiles       = atheros.CopyFiles
*IfType         = 71            ; IF_TYPE_IEEE80211
*MediaType      = 16            ; NdisMediumNative802_11
*PhysicalMediaType = 9          ; NdisPhysicalMediumNative802_11
Include         = netvwifibus.inf, machine.inf
Needs           = VWiFiBus.CopyFiles

[GIGA_DEV_OS61_E918.ndi.NTamd64.Services]
AddService = athr, 2, atheros.Service, atheros.EventLog
Include    = netvwifibus.inf
Needs      = VWiFiBus.Services

[GIGA_DEV_OS61_E918.ndi.NTamd64.HW]
Include = netvwifibus.inf
Needs   = VWiFiBus.PnPFilterRegistration

[GIGA_DEV_OS61_E914.ndi.NTamd64]
Characteristics = 0x84
BusType         = 5
AddReg          = atheros_os61.reg, atheros11n.reg, customer_GigaByte.reg, customer_GigaByteLed0.reg, 5416.antennacontrols.reg, htAdhoc.reg
DelReg          = atheros.DelReg
CopyFiles       = atheros.CopyFiles
*IfType         = 71            ; IF_TYPE_IEEE80211
*MediaType      = 16            ; NdisMediumNative802_11
*PhysicalMediaType = 9          ; NdisPhysicalMediumNative802_11
Include         = netvwifibus.inf, machine.inf
Needs           = VWiFiBus.CopyFiles

[GIGA_DEV_OS61_E914.ndi.NTamd64.Services]
AddService = athr, 2, atheros.Service, atheros.EventLog
Include    = netvwifibus.inf
Needs      = VWiFiBus.Services

[GIGA_DEV_OS61_E914.ndi.NTamd64.HW]
Include = netvwifibus.inf
Needs   = VWiFiBus.PnPFilterRegistration

[GIGA_DEV_OS61_E916.ndi.NTamd64]
Characteristics = 0x84
BusType         = 5
AddReg          = atheros_os61.reg, atheros11n.reg, customer_GigaByte.reg, customer_GigaByteLed1.reg, 5416.antennacontrols.reg, htAdhoc.reg
DelReg          = atheros.DelReg
CopyFiles       = atheros.CopyFiles
*IfType         = 71        ; IF_TYPE_IEEE80211
*MediaType      = 16        ; NdisMediumNative802_11
*PhysicalMediaType = 9      ; NdisPhysicalMediumNative802_11
Include         = netvwifibus.inf, machine.inf
Needs           = VWiFiBus.CopyFiles

[GIGA_DEV_OS61_E916.ndi.NTamd64.Services]
AddService = athr, 2, atheros.Service, atheros.EventLog
Include    = netvwifibus.inf
Needs      = VWiFiBus.Services

[GIGA_DEV_OS61_E916.ndi.NTamd64.HW]
Include = netvwifibus.inf
Needs   = VWiFiBus.PnPFilterRegistration

[ATHR_DEV_OS61_OSPEMU.ndi.NTamd64]
Characteristics = 0x84
BusType         = 5
AddReg          = atheros_os61.reg, atheros11n.reg, smpsDynamic.reg, htAdhoc.reg
DelReg          = atheros.DelReg
CopyFiles       = atheros.CopyFiles
*IfType         = 71        ; IF_TYPE_IEEE80211
*MediaType      = 16        ; NdisMediumNative802_11
*PhysicalMediaType = 9      ; NdisPhysicalMediumNative802_11
Include         = netvwifibus.inf, machine.inf
Needs           = VWiFiBus.CopyFiles

[ATHR_DEV_OS61_OSPEMU.ndi.NTamd64.Services]
AddService = athr, 2, atheros.Service, atheros.EventLog
Include    = netvwifibus.inf
Needs      = VWiFiBus.Services

[ATHR_DEV_OS61_OSPEMU.ndi.NTamd64.HW]
AddReg  = MSI.reg
Include = netvwifibus.inf
Needs   = VWiFiBus.PnPFilterRegistration

[ATHR_DEV_OS61_9485.ndi.NTamd64]
Characteristics = 0x84
BusType         = 5
AddReg          = atheros_os61.reg, atheros11n.reg, htAdhoc.reg, paprdenable.reg, customer2GreenTx.reg
DelReg          = atheros.DelReg
CopyFiles       = atheros.CopyFiles
*IfType         = 71        ; IF_TYPE_IEEE80211
*MediaType      = 16        ; NdisMediumNative802_11
*PhysicalMediaType = 9      ; NdisPhysicalMediumNative802_11
Include         = netvwifibus.inf, machine.inf
Needs           = VWiFiBus.CopyFiles

[ATHR_DEV_OS61_9485.ndi.NTamd64.Services]
AddService = athr, 2, atheros.Service, atheros.EventLog
Include    = netvwifibus.inf
Needs      = VWiFiBus.Services

[ATHR_DEV_OS61_9485.ndi.NTamd64.HW]
Include = netvwifibus.inf
Needs   = PciASPMOptIn, VWiFiBus.PnPFilterRegistration

[ATHR_DEV_OS61_312F168C.ndi.NTamd64]
Characteristics = 0x84
BusType         = 5
AddReg          = atheros_os61.reg, atheros11n.reg, htAdhoc.reg, paprdenable.reg, customer2GreenTx.reg, cemspecled_func0_6_Hi.reg
DelReg          = atheros.DelReg
CopyFiles       = atheros.CopyFiles
*IfType         = 71        ; IF_TYPE_IEEE80211
*MediaType      = 16        ; NdisMediumNative802_11
*PhysicalMediaType = 9      ; NdisPhysicalMediumNative802_11
Include         = netvwifibus.inf, machine.inf
Needs           = VWiFiBus.CopyFiles

[ATHR_DEV_OS61_312F168C.ndi.NTamd64.Services]
AddService = athr, 2, atheros.Service, atheros.EventLog
Include    = netvwifibus.inf
Needs      = VWiFiBus.Services

[ATHR_DEV_OS61_312F168C.ndi.NTamd64.HW]
Include = netvwifibus.inf
Needs   = PciASPMOptIn, VWiFiBus.PnPFilterRegistration

[ATHR_DEV_OS61_T9485.ndi.NTamd64]
Characteristics = 0x84
BusType         = 5
AddReg          = atheros_os61.reg, atheros11n.reg, htAdhoc.reg, paprdenable.reg, customer2GreenTx.reg, cfpignore.reg, customer_power_Toshiba.reg
DelReg          = atheros.DelReg
CopyFiles       = atheros.CopyFiles
*IfType         = 71        ; IF_TYPE_IEEE80211
*MediaType      = 16        ; NdisMediumNative802_11
*PhysicalMediaType = 9      ; NdisPhysicalMediumNative802_11
Include         = netvwifibus.inf, machine.inf
Needs           = VWiFiBus.CopyFiles

[ATHR_DEV_OS61_T9485.ndi.NTamd64.Services]
AddService = athr, 2, atheros.Service, atheros.EventLog
Include    = netvwifibus.inf
Needs      = VWiFiBus.Services

[ATHR_DEV_OS61_T9485.ndi.NTamd64.HW]
Include = netvwifibus.inf
Needs   = PciASPMOptIn, VWiFiBus.PnPFilterRegistration

[ATHR_DEV_OS61_9485s.ndi.NTamd64]
Characteristics = 0x84
BusType         = 5
AddReg          = atheros_os61.reg, atheros11n.reg, htAdhoc.reg, paprdenable.reg, customer2GreenTx.reg, cmdRegister.reg, ignore11denable.reg, c3war.reg, miracast_scc.reg, miracast_usepass_chl.reg
DelReg          = atheros.DelReg
CopyFiles       = atheros.CopyFiles
*IfType         = 71        ; IF_TYPE_IEEE80211
*MediaType      = 16        ; NdisMediumNative802_11
*PhysicalMediaType = 9      ; NdisPhysicalMediumNative802_11
Include         = netvwifibus.inf, machine.inf
Needs           = VWiFiBus.CopyFiles

[ATHR_DEV_OS61_9485s.ndi.NTamd64.Services]
AddService = athr, 2, atheros.Service, atheros.EventLog
Include    = netvwifibus.inf
Needs      = VWiFiBus.Services

[ATHR_DEV_OS61_9485s.ndi.NTamd64.HW]
Include = netvwifibus.inf
Needs   = PciASPMOptIn, VWiFiBus.PnPFilterRegistration

[ATHR_DEV_OS61_1111.ndi.NTamd64]
Characteristics = 0x84
BusType         = 5
AddReg          = atheros_os61.reg, atheros11n.reg, htAdhoc.reg, paprdenable.reg, customer2GreenTx.reg
DelReg          = atheros.DelReg
CopyFiles       = atheros.CopyFiles
*IfType         = 71        ; IF_TYPE_IEEE80211
*MediaType      = 16        ; NdisMediumNative802_11
*PhysicalMediaType = 9      ; NdisPhysicalMediumNative802_11
Include         = netvwifibus.inf, machine.inf
Needs           = VWiFiBus.CopyFiles

[ATHR_DEV_OS61_1111.ndi.NTamd64.Services]
AddService = athr, 2, atheros.Service, atheros.EventLog
Include    = netvwifibus.inf
Needs      = VWiFiBus.Services

[ATHR_DEV_OS61_1111.ndi.NTamd64.HW]
Include = netvwifibus.inf
Needs   = PciASPMOptIn, VWiFiBus.PnPFilterRegistration

[ATHR_DEV_OS61_3119.ndi.NTamd64]
Characteristics = 0x84
BusType         = 5
AddReg          = atheros_os61.reg, atheros11n.reg, htAdhoc.reg, 9485BTcoex.reg, customer2GreenTx.reg, paprdenable.reg, 9485LnaDivUseBtAntEnable.reg, cemspecled_func0_6.reg
DelReg          = atheros.DelReg
CopyFiles       = atheros.CopyFiles
*IfType         = 71        ; IF_TYPE_IEEE80211
*MediaType      = 16        ; NdisMediumNative802_11
*PhysicalMediaType = 9      ; NdisPhysicalMediumNative802_11
Include         = netvwifibus.inf, machine.inf
Needs           = VWiFiBus.CopyFiles

[ATHR_DEV_OS61_3119.ndi.NTamd64.Services]
AddService = athr, 2, atheros.Service, atheros.EventLog
Include    = netvwifibus.inf
Needs      = VWiFiBus.Services

[ATHR_DEV_OS61_3119.ndi.NTamd64.HW]
Include = netvwifibus.inf
Needs   = PciASPMOptIn, VWiFiBus.PnPFilterRegistration

[ATHR_DEV_OS61_3119185F.ndi.NTamd64]
Characteristics = 0x84
BusType         = 5
AddReg          = atheros_os61.reg, atheros11n.reg, htAdhoc.reg, 9485BTcoex.reg, customer2GreenTx.reg, paprdenable.reg, 9485LnaDivUseBtAntEnable.reg, cemspecled_func1_6.reg
DelReg          = atheros.DelReg
CopyFiles       = atheros.CopyFiles
*IfType         = 71        ; IF_TYPE_IEEE80211
*MediaType      = 16        ; NdisMediumNative802_11
*PhysicalMediaType = 9      ; NdisPhysicalMediumNative802_11
Include         = netvwifibus.inf, machine.inf
Needs           = VWiFiBus.CopyFiles

[ATHR_DEV_OS61_3119185F.ndi.NTamd64.Services]
AddService = athr, 2, atheros.Service, atheros.EventLog
Include    = netvwifibus.inf
Needs      = VWiFiBus.Services

[ATHR_DEV_OS61_3119185F.ndi.NTamd64.HW]
Include = netvwifibus.inf
Needs   = PciASPMOptIn, VWiFiBus.PnPFilterRegistration

[ATHR_DEV_OS61_3119s.ndi.NTamd64]
Characteristics = 0x84
BusType         = 5
AddReg          = atheros_os61.reg, atheros11n.reg, htAdhoc.reg, cmdRegister.reg, 9485BTcoex.reg, c3war.reg, rxLatencyWar.reg, customer2GreenTx.reg, paprdenable.reg, 9485LnaDivUseBtAntEnable.reg, ignore11denable.reg, miracast_scc.reg, miracast_usepass_chl.reg
DelReg          = atheros.DelReg
CopyFiles       = atheros.CopyFiles
*IfType         = 71        ; IF_TYPE_IEEE80211
*MediaType      = 16        ; NdisMediumNative802_11
*PhysicalMediaType = 9      ; NdisPhysicalMediumNative802_11
Include         = netvwifibus.inf, machine.inf
Needs           = VWiFiBus.CopyFiles

[ATHR_DEV_OS61_3119s.ndi.NTamd64.Services]
AddService = athr, 2, atheros.Service, atheros.EventLog
Include    = netvwifibus.inf
Needs      = VWiFiBus.Services

[ATHR_DEV_OS61_3119s.ndi.NTamd64.HW]
Include = netvwifibus.inf
Needs   = VWiFiBus.PnPFilterRegistration

[ATHR_DEV_OS61_4107144D.ndi.NTamd64]
Characteristics = 0x84
BusType         = 5
AddReg          = atheros_os61.reg, atheros11n.reg, smpsDynamic.reg, htAdhoc.reg, cmdRegister.reg, c3war.reg, rxLatencyWar.reg, customer_Samsung.reg, ignore11denable.reg
DelReg          = atheros.DelReg
CopyFiles       = atheros.CopyFiles
*IfType         = 71            ; IF_TYPE_IEEE80211
*MediaType      = 16            ; NdisMediumNative802_11
*PhysicalMediaType = 9          ; NdisPhysicalMediumNative802_11
Include         = netvwifibus.inf, machine.inf
Needs           = VWiFiBus.CopyFiles

[ATHR_DEV_OS61_4107144D.ndi.NTamd64.Services]
AddService = athr, 2, atheros.Service, atheros.EventLog
Include    = netvwifibus.inf
Needs      = VWiFiBus.Services

[ATHR_DEV_OS61_4107144D.ndi.NTamd64.HW]
AddReg  = MSI.reg
Include = netvwifibus.inf
Needs   = VWiFiBus.PnPFilterRegistration

[ATHR_DEV_OS61_T3119.ndi.NTamd64]
Characteristics = 0x84
BusType         = 5
AddReg          = atheros_os61.reg, atheros11n.reg, htAdhoc.reg, 9485BTCoexAgent0.reg, customer2GreenTx.reg, paprdenable.reg, ampGUID.reg, cfpignore.reg
DelReg          = atheros.DelReg
CopyFiles       = atheros.CopyFiles
*IfType         = 71        ; IF_TYPE_IEEE80211
*MediaType      = 16        ; NdisMediumNative802_11
*PhysicalMediaType = 9      ; NdisPhysicalMediumNative802_11
Include         = netvwifibus.inf, machine.inf
Needs           = VWiFiBus.CopyFiles

[ATHR_DEV_OS61_T3119.ndi.NTamd64.Services]
AddService = athr, 2, atheros.Service, atheros.EventLog
Include    = netvwifibus.inf
Needs      = VWiFiBus.Services

[ATHR_DEV_OS61_T3119.ndi.NTamd64.HW]
Include = netvwifibus.inf
Needs   = PciASPMOptIn, VWiFiBus.PnPFilterRegistration

[ATHR_DEV_OS61_OSPREY.ndi.NTamd64]
Characteristics = 0x84
BusType         = 5
AddReg          = atheros_os61.reg, atheros11n.reg, smpsDynamic.reg, htAdhoc.reg
DelReg          = atheros.DelReg
CopyFiles       = atheros.CopyFiles
*IfType         = 71        ; IF_TYPE_IEEE80211
*MediaType      = 16        ; NdisMediumNative802_11
*PhysicalMediaType = 9      ; NdisPhysicalMediumNative802_11
Include         = netvwifibus.inf, machine.inf
Needs           = VWiFiBus.CopyFiles

[ATHR_DEV_OS61_OSPREY.ndi.NTamd64.Services]
AddService = athr, 2, atheros.Service, atheros.EventLog
Include    = netvwifibus.inf
Needs      = VWiFiBus.Services

[ATHR_DEV_OS61_OSPREY.ndi.NTamd64.HW]
AddReg  = MSI.reg
Include = netvwifibus.inf
Needs   = VWiFiBus.PnPFilterRegistration

[ATHR_DEV_OS61_K110x.ndi.NTamd64]
Characteristics = 0x84
BusType         = 5
AddReg          = atheros_os61.reg, atheros11n.reg, smpsDynamic.reg, led_func0_10.reg, htAdhoc.reg
DelReg          = atheros.DelReg
CopyFiles       = atheros.CopyFiles
*IfType         = 71        ; IF_TYPE_IEEE80211
*MediaType      = 16        ; NdisMediumNative802_11
*PhysicalMediaType = 9      ; NdisPhysicalMediumNative802_11
Include         = netvwifibus.inf, machine.inf
Needs           = VWiFiBus.CopyFiles

[ATHR_DEV_OS61_K110x.ndi.NTamd64.Services]
AddService = athr, 2, atheros.Service, atheros.EventLog
Include    = netvwifibus.inf
Needs      = VWiFiBus.Services

[ATHR_DEV_OS61_K110x.ndi.NTamd64.HW]
AddReg  = MSI.reg
Include = netvwifibus.inf
Needs   = VWiFiBus.PnPFilterRegistration

[ATHR_DEV_OS61_938x.ndi.NTamd64]
Characteristics = 0x84
BusType         = 5
AddReg          = atheros_os61.reg, atheros11n.reg, smpsDynamic.reg, htAdhoc.reg
DelReg          = atheros.DelReg
CopyFiles       = atheros.CopyFiles
*IfType         = 71        ; IF_TYPE_IEEE80211
*MediaType      = 16        ; NdisMediumNative802_11
*PhysicalMediaType = 9      ; NdisPhysicalMediumNative802_11
Include         = netvwifibus.inf, machine.inf
Needs           = VWiFiBus.CopyFiles

[ATHR_DEV_OS61_938x.ndi.NTamd64.Services]
AddService = athr, 2, atheros.Service, atheros.EventLog
Include    = netvwifibus.inf
Needs      = VWiFiBus.Services

[ATHR_DEV_OS61_938x.ndi.NTamd64.HW]
AddReg  = MSI.reg
Include = netvwifibus.inf
Needs   = PciASPMOptIn, VWiFiBus.PnPFilterRegistration

[ATHR_DEV_OS61_T938x.ndi.NTamd64]
Characteristics = 0x84
BusType         = 5
AddReg          = atheros_os61.reg, atheros11n.reg, smpsDynamic.reg, htAdhoc.reg, cfpignore.reg
DelReg          = atheros.DelReg
CopyFiles       = atheros.CopyFiles
*IfType         = 71        ; IF_TYPE_IEEE80211
*MediaType      = 16        ; NdisMediumNative802_11
*PhysicalMediaType = 9      ; NdisPhysicalMediumNative802_11
Include         = netvwifibus.inf, machine.inf
Needs           = VWiFiBus.CopyFiles

[ATHR_DEV_OS61_T938x.ndi.NTamd64.Services]
AddService = athr, 2, atheros.Service, atheros.EventLog
Include    = netvwifibus.inf
Needs      = VWiFiBus.Services

[ATHR_DEV_OS61_T938x.ndi.NTamd64.HW]
AddReg  = MSI.reg
Include = netvwifibus.inf
Needs   = PciASPMOptIn, VWiFiBus.PnPFilterRegistration

[ATHR_DEV_OS61_946x.ndi.NTamd64]
Characteristics = 0x84
BusType         = 5
AddReg          = atheros_os61.reg, atheros11n.reg, smpsDynamic.reg, htAdhoc.reg, jupiter2ant.reg, wowenable.reg
DelReg          = atheros.DelReg
CopyFiles       = atheros.CopyFiles
*IfType         = 71        ; IF_TYPE_IEEE80211
*MediaType      = 16        ; NdisMediumNative802_11
*PhysicalMediaType = 9      ; NdisPhysicalMediumNative802_11
Include         = netvwifibus.inf, machine.inf
Needs           = VWiFiBus.CopyFiles

[ATHR_DEV_OS61_946x.ndi.NTamd64.Services]
AddService = athr, 2, atheros.Service, atheros.EventLog
Include    = netvwifibus.inf
Needs      = VWiFiBus.Services

[ATHR_DEV_OS61_946x.ndi.NTamd64.HW]
Include = netvwifibus.inf
Needs   = PciASPMOptIn, VWiFiBus.PnPFilterRegistration

[ATHR_DEV_OS61_Chicony_946x.ndi.NTamd64]
Characteristics = 0x84
BusType         = 5
AddReg          = atheros_os61.reg, atheros11n.reg, smpsDynamic.reg, htAdhoc.reg, jupiter2ant.reg, 5416.bandselect.reg, cemspecled_func0_4.reg
DelReg          = atheros.DelReg
CopyFiles       = atheros.CopyFiles
*IfType         = 71        ; IF_TYPE_IEEE80211
*MediaType      = 16        ; NdisMediumNative802_11
*PhysicalMediaType = 9      ; NdisPhysicalMediumNative802_11
Include         = netvwifibus.inf, machine.inf
Needs           = VWiFiBus.CopyFiles

[ATHR_DEV_OS61_Chicony_946x.ndi.NTamd64.Services]
AddService = athr, 2, atheros.Service, atheros.EventLog
Include    = netvwifibus.inf
Needs      = VWiFiBus.Services

[ATHR_DEV_OS61_Chicony_946x.ndi.NTamd64.HW]
Include = netvwifibus.inf
Needs   = PciASPMOptIn, VWiFiBus.PnPFilterRegistration

[ATHR_DEV_OS61_K1202.ndi.NTamd64]
Characteristics = 0x84
BusType         = 5
AddReg          = atheros_os61.reg, atheros11n.reg, smpsDynamic.reg, led_func0_4.reg, htAdhoc.reg, jupiter2ant.reg, bt30_high_speed.reg
DelReg          = atheros.DelReg
CopyFiles       = atheros.CopyFiles
*IfType         = 71        ; IF_TYPE_IEEE80211
*MediaType      = 16        ; NdisMediumNative802_11
*PhysicalMediaType = 9      ; NdisPhysicalMediumNative802_11
Include         = netvwifibus.inf, machine.inf
Needs           = VWiFiBus.CopyFiles

[ATHR_DEV_OS61_K1202.ndi.NTamd64.Services]
AddService = athr, 2, atheros.Service, atheros.EventLog
Include    = netvwifibus.inf
Needs      = VWiFiBus.Services

[ATHR_DEV_OS61_K1202.ndi.NTamd64.HW]
Include = netvwifibus.inf
Needs   = PciASPMOptIn, VWiFiBus.PnPFilterRegistration


[ATHR_DEV_OS61_21101A3B.ndi.NTamd64]
Characteristics = 0x84
BusType         = 5
AddReg          = atheros_os61.reg, atheros11n.reg, smpsDynamic.reg, htAdhoc.reg, jupiter2ant.reg, wowenable.reg, cemspecled_func0_4.reg, bt30_high_speed.reg 
DelReg          = atheros.DelReg
CopyFiles       = atheros.CopyFiles
*IfType         = 71        ; IF_TYPE_IEEE80211
*MediaType      = 16        ; NdisMediumNative802_11
*PhysicalMediaType = 9      ; NdisPhysicalMediumNative802_11
Include         = netvwifibus.inf, machine.inf
Needs           = VWiFiBus.CopyFiles

[ATHR_DEV_OS61_21101A3B.ndi.NTamd64.Services]
AddService = athr, 2, atheros.Service, atheros.EventLog
Include    = netvwifibus.inf
Needs      = VWiFiBus.Services

[ATHR_DEV_OS61_21101A3B.ndi.NTamd64.HW]
Include = netvwifibus.inf
Needs   = PciASPMOptIn, VWiFiBus.PnPFilterRegistration

[ATHR_DEV_OS61_664111AD.ndi.NTamd64]
Characteristics = 0x84
BusType         = 5
AddReg          = atheros_os61.reg, atheros11n.reg, smpsDynamic.reg, htAdhoc.reg, jupiter2ant.reg, wowenable.reg, bt30_high_speed.reg
DelReg          = atheros.DelReg
CopyFiles       = atheros.CopyFiles
*IfType         = 71        ; IF_TYPE_IEEE80211
*MediaType      = 16        ; NdisMediumNative802_11
*PhysicalMediaType = 9      ; NdisPhysicalMediumNative802_11
Include         = netvwifibus.inf, machine.inf
Needs           = VWiFiBus.CopyFiles

[ATHR_DEV_OS61_664111AD.ndi.NTamd64.Services]
AddService = athr, 2, atheros.Service, atheros.EventLog
Include    = netvwifibus.inf
Needs      = VWiFiBus.Services

[ATHR_DEV_OS61_664111AD.ndi.NTamd64.HW]
Include = netvwifibus.inf
Needs   = PciASPMOptIn, VWiFiBus.PnPFilterRegistration

[ATHR_DEV_OS61_946xs.ndi.NTamd64]
Characteristics = 0x84
BusType         = 5
AddReg          = atheros_os61.reg, atheros11n.reg, smpsDynamic.reg, htAdhoc.reg, jupiter2ant.reg, cmdRegister.reg, ignore11denable.reg, halShortRetry.reg, ConnectionFailure.reg, miracast_scc.reg, miracast_usepass_chl.reg
DelReg          = atheros.DelReg
CopyFiles       = atheros.CopyFiles
*IfType         = 71        ; IF_TYPE_IEEE80211
*MediaType      = 16        ; NdisMediumNative802_11
*PhysicalMediaType = 9      ; NdisPhysicalMediumNative802_11
Include         = netvwifibus.inf, machine.inf
Needs           = VWiFiBus.CopyFiles

[ATHR_DEV_OS61_946xs.ndi.NTamd64.Services]
AddService = athr, 2, atheros.Service, atheros.EventLog
Include    = netvwifibus.inf
Needs      = VWiFiBus.Services

[ATHR_DEV_OS61_946xs.ndi.NTamd64.HW]
Include = netvwifibus.inf
Needs   = PciASPMOptIn, VWiFiBus.PnPFilterRegistration

[ATHR_DEV_OS61_T946x.ndi.NTamd64]
Characteristics = 0x84
BusType         = 5
AddReg          = atheros_os61.reg, atheros11n.reg, smpsDynamic.reg, htAdhoc.reg, jupiter2ant.reg, ampGUID.reg, ampTFilter.reg, cfpignore.reg, customer_power_Toshiba.reg, paprdDisablePartialTime.reg
DelReg          = atheros.DelReg
CopyFiles       = atheros.CopyFiles
*IfType         = 71        ; IF_TYPE_IEEE80211
*MediaType      = 16        ; NdisMediumNative802_11
*PhysicalMediaType = 9      ; NdisPhysicalMediumNative802_11
Include         = netvwifibus.inf, machine.inf
Needs           = VWiFiBus.CopyFiles

[ATHR_DEV_OS61_T946x.ndi.NTamd64.Services]
AddService = athr, 2, atheros.Service, atheros.EventLog
Include    = netvwifibus.inf
Needs      = VWiFiBus.Services

[ATHR_DEV_OS61_T946x.ndi.NTamd64.HW]
Include = netvwifibus.inf
Needs   = PciASPMOptIn, VWiFiBus.PnPFilterRegistration

[ATHR_DEV_OS61_CUS217.ndi.NTamd64]
Characteristics = 0x84
BusType         = 5
AddReg          = atheros_os61.reg, atheros11n.reg, smpsDynamic.reg, htAdhoc.reg, jupiter2ant2.reg
DelReg          = atheros.DelReg
CopyFiles       = atheros.CopyFiles
*IfType         = 71        ; IF_TYPE_IEEE80211
*MediaType      = 16        ; NdisMediumNative802_11
*PhysicalMediaType = 9      ; NdisPhysicalMediumNative802_11
Include         = netvwifibus.inf, machine.inf
Needs           = VWiFiBus.CopyFiles

[ATHR_DEV_OS61_CUS217.ndi.NTamd64.Services]
AddService = athr, 2, atheros.Service, atheros.EventLog
Include    = netvwifibus.inf
Needs      = VWiFiBus.Services

[ATHR_DEV_OS61_CUS217.ndi.NTamd64.HW]
Include = netvwifibus.inf
Needs   = PciASPMOptIn, VWiFiBus.PnPFilterRegistration

[ATHR_DEV_OS61_21161A3B.ndi.NTamd64]
Characteristics = 0x84
BusType         = 5
AddReg          = atheros_os61.reg, atheros11n.reg, smpsDynamic.reg, htAdhoc.reg, jupiter2ant2.reg, cemspecled_func0_4.reg, RestoreSettingCount.reg
DelReg          = atheros.DelReg
CopyFiles       = atheros.CopyFiles
*IfType         = 71        ; IF_TYPE_IEEE80211
*MediaType      = 16        ; NdisMediumNative802_11
*PhysicalMediaType = 9      ; NdisPhysicalMediumNative802_11
Include         = netvwifibus.inf, machine.inf
Needs           = VWiFiBus.CopyFiles

[ATHR_DEV_OS61_21161A3B.ndi.NTamd64.Services]
AddService = athr, 2, atheros.Service, atheros.EventLog
Include    = netvwifibus.inf
Needs      = VWiFiBus.Services

[ATHR_DEV_OS61_21161A3B.ndi.NTamd64.HW]
Include = netvwifibus.inf
Needs   = PciASPMOptIn, VWiFiBus.PnPFilterRegistration

[ATHR_DEV_OS61_WB222SB.ndi.NTamd64]
Characteristics = 0x84
BusType         = 5
AddReg          = atheros_os61.reg, atheros11n.reg, smpsDynamic.reg, htAdhoc.reg, jupiter2ant.reg, cemspecled_func0_4.reg, RestoreSettingCount.reg, WB222SB.reg, wowenable.reg, ctlPowerTableChangeEnable.reg, bt30_high_speed.reg
DelReg          = atheros.DelReg
CopyFiles       = atheros.CopyFiles
*IfType         = 71        ; IF_TYPE_IEEE80211
*MediaType      = 16        ; NdisMediumNative802_11
*PhysicalMediaType = 9      ; NdisPhysicalMediumNative802_11
Include         = netvwifibus.inf, machine.inf
Needs           = VWiFiBus.CopyFiles

[ATHR_DEV_OS61_WB222SB.ndi.NTamd64.Services]
AddService = athr, 2, atheros.Service, atheros.EventLog
Include    = netvwifibus.inf
Needs      = VWiFiBus.Services

[ATHR_DEV_OS61_WB222SB.ndi.NTamd64.HW]
Include = netvwifibus.inf
Needs   = PciASPMOptIn, VWiFiBus.PnPFilterRegistration

[ATHR_DEV_OS61_WB222SB_BTC.ndi.NTamd64]
Characteristics = 0x84
BusType         = 5
AddReg          = atheros_os61.reg, atheros11n.reg, smpsDynamic.reg, htAdhoc.reg, jupiter2ant.reg, cemspecled_func0_4.reg, RestoreSettingCount.reg, WB222SB.reg, wowenable.reg, ctlPowerTableChangeEnable.reg, bt30_high_speed.reg
DelReg          = atheros.DelReg
CopyFiles       = atheros.CopyFiles
*IfType         = 71        ; IF_TYPE_IEEE80211
*MediaType      = 16        ; NdisMediumNative802_11
*PhysicalMediaType = 9      ; NdisPhysicalMediumNative802_11
Include         = netvwifibus.inf, machine.inf
Needs           = VWiFiBus.CopyFiles

[ATHR_DEV_OS61_WB222SB_BTC.ndi.NTamd64.Services]
AddService = athr, 2, atheros.Service, atheros.EventLog
Include    = netvwifibus.inf
Needs      = VWiFiBus.Services

[ATHR_DEV_OS61_WB222SB_BTC.ndi.NTamd64.HW]
Include = netvwifibus.inf
Needs   = PciASPMOptIn, VWiFiBus.PnPFilterRegistration

[ATHR_DEV_OS61_082211AD.ndi.NTamd64]
Characteristics = 0x84
BusType         = 5
AddReg          = atheros_os61.reg, atheros11n.reg, smpsDynamic.reg, htAdhoc.reg, jupiter2ant2.reg, cemspecled_func0_4.reg, RestoreSettingCount.reg, wowenable.reg, bt30_high_speed.reg
DelReg          = atheros.DelReg
CopyFiles       = atheros.CopyFiles
*IfType         = 71        ; IF_TYPE_IEEE80211
*MediaType      = 16        ; NdisMediumNative802_11
*PhysicalMediaType = 9      ; NdisPhysicalMediumNative802_11
Include         = netvwifibus.inf, machine.inf
Needs           = VWiFiBus.CopyFiles

[ATHR_DEV_OS61_082211AD.ndi.NTamd64.Services]
AddService = athr, 2, atheros.Service, atheros.EventLog
Include    = netvwifibus.inf
Needs      = VWiFiBus.Services

[ATHR_DEV_OS61_082211AD.ndi.NTamd64.HW]
Include = netvwifibus.inf
Needs   = PciASPMOptIn, VWiFiBus.PnPFilterRegistration

[ATHR_DEV_OS61_850E1043.ndi.NTamd64]
Characteristics = 0x84
BusType         = 5
AddReg          = atheros_os61.reg, atheros11n.reg, smpsDynamic.reg, htAdhoc.reg, jupiter2ant.reg, customer3h.reg, S5wow.reg, DisWakeOnAPLost.reg
DelReg          = atheros.DelReg
CopyFiles       = atheros.CopyFiles
*IfType         = 71        ; IF_TYPE_IEEE80211
*MediaType      = 16        ; NdisMediumNative802_11
*PhysicalMediaType = 9      ; NdisPhysicalMediumNative802_11
Include         = netvwifibus.inf, machine.inf
Needs           = VWiFiBus.CopyFiles

[ATHR_DEV_OS61_850E1043.ndi.NTamd64.Services]
AddService = athr, 2, atheros.Service, atheros.EventLog
Include    = netvwifibus.inf
Needs      = VWiFiBus.Services

[ATHR_DEV_OS61_850E1043.ndi.NTamd64.HW]
Include = netvwifibus.inf
Needs   = PciASPMOptIn, VWiFiBus.PnPFilterRegistration

[ATHR_DEV_OS61_211C1A3B.ndi.NTamd64]
Characteristics = 0x84
BusType         = 5
AddReg          = atheros_os61.reg, atheros11n.reg, smpsDynamic.reg, htAdhoc.reg, jupiter2ant.reg, customer3h.reg, S5wow.reg, bt30_high_speed.reg
DelReg          = atheros.DelReg
CopyFiles       = atheros.CopyFiles
*IfType         = 71        ; IF_TYPE_IEEE80211
*MediaType      = 16        ; NdisMediumNative802_11
*PhysicalMediaType = 9      ; NdisPhysicalMediumNative802_11
Include         = netvwifibus.inf, machine.inf
Needs           = VWiFiBus.CopyFiles

[ATHR_DEV_OS61_211C1A3B.ndi.NTamd64.Services]
AddService = athr, 2, atheros.Service, atheros.EventLog
Include    = netvwifibus.inf
Needs      = VWiFiBus.Services

[ATHR_DEV_OS61_211C1A3B.ndi.NTamd64.HW]
Include = netvwifibus.inf
Needs   = PciASPMOptIn, VWiFiBus.PnPFilterRegistration

[ATHR_DEV_OS61_311711AD.ndi.NTamd64]
Characteristics = 0x84
BusType         = 5
AddReg          = atheros_os61.reg, atheros11n.reg, smpsDynamic.reg, htAdhoc.reg, jupiter2ant2.reg, customer3h.reg, roamPolicy2.reg, AdjustRSSI.reg, halShortRetry.reg, SleepTimePwrSaveMax1000.reg, FilterOutCCK.reg, wirelessmode.all.reg, acer.preferredband.reg, MCCStaTputAdjust.reg
DelReg          = atheros.DelReg
CopyFiles       = atheros.CopyFiles
*IfType         = 71        ; IF_TYPE_IEEE80211
*MediaType      = 16        ; NdisMediumNative802_11
*PhysicalMediaType = 9      ; NdisPhysicalMediumNative802_11
Include         = netvwifibus.inf, machine.inf
Needs           = VWiFiBus.CopyFiles

[ATHR_DEV_OS61_311711AD.ndi.NTamd64.Services]
AddService = athr, 2, atheros.Service, atheros.EventLog
Include    = netvwifibus.inf
Needs      = VWiFiBus.Services

[ATHR_DEV_OS61_311711AD.ndi.NTamd64.HW]
Include = netvwifibus.inf
Needs   = PciASPMOptIn, VWiFiBus.PnPFilterRegistration

[ATHR_DEV_OS61_080211AD.ndi.NTamd64]
Characteristics = 0x84
BusType         = 5
AddReg          = atheros_os61.reg, atheros11n.reg, smpsDynamic.reg, htAdhoc.reg, jupiter2ant2.reg, customer3h.reg, roamPolicy2.reg, AdjustRSSI.reg, halShortRetry.reg, SleepTimePwrSaveMax1000.reg, FilterOutCCK.reg, j21swwow.reg, wirelessmode.all.reg, acer.preferredband.reg, heavyClipFuncEnable.reg, MCCStaTputAdjust.reg, acerCtlPowerChangeEnable.reg
DelReg          = atheros.DelReg
CopyFiles       = atheros.CopyFiles
*IfType         = 71        ; IF_TYPE_IEEE80211
*MediaType      = 16        ; NdisMediumNative802_11
*PhysicalMediaType = 9      ; NdisPhysicalMediumNative802_11
Include         = netvwifibus.inf, machine.inf
Needs           = VWiFiBus.CopyFiles

[ATHR_DEV_OS61_080211AD.ndi.NTamd64.Services]
AddService = athr, 2, atheros.Service, atheros.EventLog
Include    = netvwifibus.inf
Needs      = VWiFiBus.Services

[ATHR_DEV_OS61_080211AD.ndi.NTamd64.HW]
Include = netvwifibus.inf
Needs   = PciASPMOptIn, VWiFiBus.PnPFilterRegistration

[ATHR_DEV_OS61_E086105B.ndi.NTamd64]
Characteristics = 0x84
BusType         = 5
AddReg          = atheros_os61.reg, atheros11n.reg, smpsDynamic.reg, htAdhoc.reg, jupiter2ant2.reg, customer3h.reg, roamPolicy2.reg, AdjustRSSI.reg, halShortRetry.reg, SleepTimePwrSaveMax1000.reg, FilterOutCCK.reg, j21swwow.reg, wirelessmode.all.reg, acer.preferredband.reg, heavyClipFuncEnable.reg, MCCStaTputAdjust.reg
DelReg          = atheros.DelReg
CopyFiles       = atheros.CopyFiles
*IfType         = 71        ; IF_TYPE_IEEE80211
*MediaType      = 16        ; NdisMediumNative802_11
*PhysicalMediaType = 9      ; NdisPhysicalMediumNative802_11
Include         = netvwifibus.inf, machine.inf
Needs           = VWiFiBus.CopyFiles

[ATHR_DEV_OS61_E086105B.ndi.NTamd64.Services]
AddService = athr, 2, atheros.Service, atheros.EventLog
Include    = netvwifibus.inf
Needs      = VWiFiBus.Services

[ATHR_DEV_OS61_E086105B.ndi.NTamd64.HW]
Include = netvwifibus.inf
Needs   = PciASPMOptIn, VWiFiBus.PnPFilterRegistration

[ATHR_DEV_OS61_1186788.ndi.NTamd64]
Characteristics = 0x84
BusType         = 5
AddReg          = atheros_os61.reg, atheros11n.reg, smpsDynamic.reg, htAdhoc.reg, jupiter2ant2.reg, customer3h.reg, roamPolicy2.reg, AdjustRSSI.reg, halShortRetry.reg, SleepTimePwrSaveMax1000.reg, FilterOutCCK.reg, wirelessmode.all.reg, acer.preferredband.reg, MCCStaTputAdjust.reg, acerCtlPowerChangeEnable.reg
DelReg          = atheros.DelReg
CopyFiles       = atheros.CopyFiles
*IfType         = 71        ; IF_TYPE_IEEE80211
*MediaType      = 16        ; NdisMediumNative802_11
*PhysicalMediaType = 9      ; NdisPhysicalMediumNative802_11
Include         = netvwifibus.inf, machine.inf
Needs           = VWiFiBus.CopyFiles

[ATHR_DEV_OS61_1186788.ndi.NTamd64.Services]
AddService = athr, 2, atheros.Service, atheros.EventLog
Include    = netvwifibus.inf
Needs      = VWiFiBus.Services

[ATHR_DEV_OS61_1186788.ndi.NTamd64.HW]
Include = netvwifibus.inf
Needs   = PciASPMOptIn, VWiFiBus.PnPFilterRegistration

[ATHR_DEV_OS61_956x.ndi.NTamd64]
Characteristics = 0x84
BusType         = 5
AddReg          = atheros_os61.reg, atheros11n.reg, htAdhoc.reg, aphroditeant.reg, aphrodite_coex.reg, ledcontrol8.reg, ConnectionFailure.reg, aphroditeantdiv.reg
DelReg          = atheros.DelReg
CopyFiles       = atheros.CopyFiles
*IfType         = 71        ; IF_TYPE_IEEE80211
*MediaType      = 16        ; NdisMediumNative802_11
*PhysicalMediaType = 9      ; NdisPhysicalMediumNative802_11
Include         = netvwifibus.inf, machine.inf
Needs           = VWiFiBus.CopyFiles

[ATHR_DEV_OS61_956x.ndi.NTamd64.Services]
AddService = athr, 2, atheros.Service, atheros.EventLog
Include    = netvwifibus.inf
Needs      = VWiFiBus.Services

[ATHR_DEV_OS61_956x.ndi.NTamd64.HW]
Include = netvwifibus.inf
Needs   = PciASPMOptIn, VWiFiBus.PnPFilterRegistration

[ATHR_DEV_OS61_956xv.ndi.NTamd64]
Characteristics = 0x84
BusType         = 5
AddReg          = atheros_os61.reg, atheros11n.reg, htAdhoc.reg, aphroditeant2.reg, aphrodite_coex2.reg, ledcontrol8.reg, ConnectionFailure.reg, aphroditeantdiv2.reg, A11swwow.reg 
DelReg          = atheros.DelReg
CopyFiles       = atheros.CopyFiles
*IfType         = 71        ; IF_TYPE_IEEE80211
*MediaType      = 16        ; NdisMediumNative802_11
*PhysicalMediaType = 9      ; NdisPhysicalMediumNative802_11
Include         = netvwifibus.inf, machine.inf
Needs           = VWiFiBus.CopyFiles

[ATHR_DEV_OS61_956xv.ndi.NTamd64.Services]
AddService = athr, 2, atheros.Service, atheros.EventLog
Include    = netvwifibus.inf
Needs      = VWiFiBus.Services

[ATHR_DEV_OS61_956xv.ndi.NTamd64.HW]
AddReg  = MSI.reg
Include = netvwifibus.inf
Needs   = PciASPMOptIn, VWiFiBus.PnPFilterRegistration

[ATHR_DEV_OS61_956xs.ndi.NTamd64]
Characteristics = 0x84
BusType         = 5
AddReg          = atheros_os61.reg, atheros11n.reg, htAdhoc.reg, aphroditeant2.reg, aphrodite_coex2.reg, ledcontrol8.reg, ConnectionFailure.reg, ignore11denable.reg, miracast_scc.reg, miracast_usepass_chl.reg, aphroditeantdiv2.reg
DelReg          = atheros.DelReg
CopyFiles       = atheros.CopyFiles
*IfType         = 71        ; IF_TYPE_IEEE80211
*MediaType      = 16        ; NdisMediumNative802_11
*PhysicalMediaType = 9      ; NdisPhysicalMediumNative802_11
Include         = netvwifibus.inf, machine.inf
Needs           = VWiFiBus.CopyFiles

[ATHR_DEV_OS61_956xs.ndi.NTamd64.Services]
AddService = athr, 2, atheros.Service, atheros.EventLog
Include    = netvwifibus.inf
Needs      = VWiFiBus.Services

[ATHR_DEV_OS61_956xs.ndi.NTamd64.HW]
Include = netvwifibus.inf
Needs   = PciASPMOptIn, VWiFiBus.PnPFilterRegistration

[ATHR_DEV_OS61_SS335.ndi.NTamd64]
Characteristics = 0x84
BusType         = 5
AddReg          = atheros_os61.reg, atheros11n.reg, htAdhoc.reg, aphroditeant2.reg, aphrodite_coex2.reg, ledcontrol8.reg, ConnectionFailure.reg, ignore11denable.reg, miracast_scc.reg, miracast_usepass_chl.reg, aphroditeantdiv2.reg
DelReg          = atheros.DelReg
CopyFiles       = atheros.CopyFiles
*IfType         = 71        ; IF_TYPE_IEEE80211
*MediaType      = 16        ; NdisMediumNative802_11
*PhysicalMediaType = 9      ; NdisPhysicalMediumNative802_11
Include         = netvwifibus.inf, machine.inf
Needs           = VWiFiBus.CopyFiles

[ATHR_DEV_OS61_SS335.ndi.NTamd64.Services]
AddService = athr, 2, atheros.Service, atheros.EventLog
Include    = netvwifibus.inf
Needs      = VWiFiBus.Services

[ATHR_DEV_OS61_SS335.ndi.NTamd64.HW]
Include = netvwifibus.inf
Needs   = PciASPMOptIn, VWiFiBus.PnPFilterRegistration

[ATHR_DEV_OS61_ACER956x.ndi.NTamd64]
Characteristics = 0x84
BusType         = 5
AddReg          = atheros_os61.reg, atheros11n.reg, htAdhoc.reg, aphroditeant.reg, aphrodite_coex_ts.reg, ledcontrol8.reg, delayNWSleep.reg, FilterOutCCK.reg, miracast_off.reg, MCCStaTputAdjust.reg, wirelessmode.2g.reg
DelReg          = atheros.DelReg
CopyFiles       = atheros.CopyFiles
*IfType         = 71        ; IF_TYPE_IEEE80211
*MediaType      = 16        ; NdisMediumNative802_11
*PhysicalMediaType = 9      ; NdisPhysicalMediumNative802_11
Include         = netvwifibus.inf, machine.inf
Needs           = VWiFiBus.CopyFiles

[ATHR_DEV_OS61_ACER956x.ndi.NTamd64.Services]
AddService = athr, 2, atheros.Service, atheros.EventLog
Include    = netvwifibus.inf
Needs      = VWiFiBus.Services

[ATHR_DEV_OS61_ACER956x.ndi.NTamd64.HW]
Include = netvwifibus.inf
Needs   = PciASPMOptIn, VWiFiBus.PnPFilterRegistration

[ATHR_DEV_OS61_ACER_956x_CH2.ndi.NTamd64]
Characteristics = 0x84
BusType         = 5
AddReg          = atheros_os61.reg, atheros11n.reg, htAdhoc.reg, aphroditeant2.reg, aphrodite_coex2.reg, ledcontrol8.reg, delayNWSleep.reg, aphroditeantdiv2.reg, AphroditeMitiShift.reg, customer_power.reg, MCCStaTputAdjust.reg, wirelessmode.2g.reg
DelReg          = atheros.DelReg
CopyFiles       = atheros.CopyFiles
*IfType         = 71        ; IF_TYPE_IEEE80211
*MediaType      = 16        ; NdisMediumNative802_11
*PhysicalMediaType = 9      ; NdisPhysicalMediumNative802_11
Include         = netvwifibus.inf, machine.inf
Needs           = VWiFiBus.CopyFiles

[ATHR_DEV_OS61_ACER_956x_CH2.ndi.NTamd64.Services]
AddService = athr, 2, atheros.Service, atheros.EventLog
Include    = netvwifibus.inf
Needs      = VWiFiBus.Services

[ATHR_DEV_OS61_ACER_956x_CH2.ndi.NTamd64.HW]
Include = netvwifibus.inf
Needs   = PciASPMOptIn, VWiFiBus.PnPFilterRegistration

[ATHR_DEV_OS61_ACER_A11_CH2.ndi.NTamd64]
Characteristics = 0x84
BusType         = 5
AddReg          = atheros_os61.reg, atheros11n.reg, htAdhoc.reg, aphroditeant2.reg, aphrodite_coex2.reg, ledcontrol8acthi.reg, delayNWSleep.reg, aphroditeantdiv2.reg, AphroditeMitiShift.reg, customer_power.reg, bt30_high_speed.reg, wirelessmode.2g.reg
DelReg          = atheros.DelReg
CopyFiles       = atheros.CopyFiles
*IfType         = 71        ; IF_TYPE_IEEE80211
*MediaType      = 16        ; NdisMediumNative802_11
*PhysicalMediaType = 9      ; NdisPhysicalMediumNative802_11
Include         = netvwifibus.inf, machine.inf
Needs           = VWiFiBus.CopyFiles

[ATHR_DEV_OS61_ACER_A11_CH2.ndi.NTamd64.Services]
AddService = athr, 2, atheros.Service, atheros.EventLog
Include    = netvwifibus.inf
Needs      = VWiFiBus.Services

[ATHR_DEV_OS61_ACER_A11_CH2.ndi.NTamd64.HW]
Include = netvwifibus.inf
Needs   = PciASPMOptIn, VWiFiBus.PnPFilterRegistration

[ATHR_DEV_OS61_A120185F.ndi.NTamd64]
Characteristics = 0x84
BusType         = 5
AddReg          = atheros_os61.reg, atheros11n.reg, htAdhoc.reg, aphroditeant2.reg, aphrodite_coex2.reg, ledcontrol8.reg, delayNWSleep.reg, aphroditeantdiv2.reg, AphroditeMitiShift.reg, customer_power.reg, MCCStaTputAdjust.reg, wirelessmode.2g.reg
DelReg          = atheros.DelReg
CopyFiles       = atheros.CopyFiles
*IfType         = 71        ; IF_TYPE_IEEE80211
*MediaType      = 16        ; NdisMediumNative802_11
*PhysicalMediaType = 9      ; NdisPhysicalMediumNative802_11
Include         = netvwifibus.inf, machine.inf
Needs           = VWiFiBus.CopyFiles

[ATHR_DEV_OS61_A120185F.ndi.NTamd64.Services]
AddService = athr, 2, atheros.Service, atheros.EventLog
Include    = netvwifibus.inf
Needs      = VWiFiBus.Services

[ATHR_DEV_OS61_A120185F.ndi.NTamd64.HW]
Include = netvwifibus.inf
Needs   = PciASPMOptIn, VWiFiBus.PnPFilterRegistration

[ATHR_DEV_OS61_01186931.ndi.NTamd64]
Characteristics = 0x84
BusType         = 5
AddReg          = atheros_os61.reg, atheros11n.reg, htAdhoc.reg, aphroditeant.reg, aphrodite_coex.reg, ledcontrol8.reg, ConnectionFailure.reg, FilterOutCCK.reg
DelReg          = atheros.DelReg
CopyFiles       = atheros.CopyFiles
*IfType         = 71        ; IF_TYPE_IEEE80211
*MediaType      = 16        ; NdisMediumNative802_11
*PhysicalMediaType = 9      ; NdisPhysicalMediumNative802_11
Include         = netvwifibus.inf, machine.inf
Needs           = VWiFiBus.CopyFiles

[ATHR_DEV_OS61_01186931.ndi.NTamd64.Services]
AddService = athr, 2, atheros.Service, atheros.EventLog
Include    = netvwifibus.inf
Needs      = VWiFiBus.Services

[ATHR_DEV_OS61_01186931.ndi.NTamd64.HW]
Include = netvwifibus.inf
Needs   = PciASPMOptIn, VWiFiBus.PnPFilterRegistration

[ATHR_DEV_OS61_01186931_LED.ndi.NTamd64]
Characteristics = 0x84
BusType         = 5
AddReg          = atheros_os61.reg, atheros11n.reg, htAdhoc.reg, aphroditeant.reg, aphrodite_coex.reg, ledcontrol9_blink.reg, ConnectionFailure.reg, FilterOutCCK.reg
DelReg          = atheros.DelReg
CopyFiles       = atheros.CopyFiles
*IfType         = 71        ; IF_TYPE_IEEE80211
*MediaType      = 16        ; NdisMediumNative802_11
*PhysicalMediaType = 9      ; NdisPhysicalMediumNative802_11
Include         = netvwifibus.inf, machine.inf
Needs           = VWiFiBus.CopyFiles

[ATHR_DEV_OS61_01186931_LED.ndi.NTamd64.Services]
AddService = athr, 2, atheros.Service, atheros.EventLog
Include    = netvwifibus.inf
Needs      = VWiFiBus.Services

[ATHR_DEV_OS61_01186931_LED.ndi.NTamd64.HW]
Include = netvwifibus.inf
Needs   = PciASPMOptIn, VWiFiBus.PnPFilterRegistration

[ATHR_DEV_OS61_21301A3B.ndi.NTamd64]
Characteristics = 0x84
BusType         = 5
AddReg          = atheros_os61.reg, atheros11n.reg, htAdhoc.reg, aphroditeant2.reg, aphrodite_coex2.reg, ledcontrol8.reg, ConnectionFailure.reg, aphroditeantdiv2.reg, bt30_high_speed.reg
DelReg          = atheros.DelReg
CopyFiles       = atheros.CopyFiles
*IfType         = 71        ; IF_TYPE_IEEE80211
*MediaType      = 16        ; NdisMediumNative802_11
*PhysicalMediaType = 9      ; NdisPhysicalMediumNative802_11
Include         = netvwifibus.inf, machine.inf
Needs           = VWiFiBus.CopyFiles

[ATHR_DEV_OS61_21301A3B.ndi.NTamd64.Services]
AddService = athr, 2, atheros.Service, atheros.EventLog
Include    = netvwifibus.inf
Needs      = VWiFiBus.Services

[ATHR_DEV_OS61_21301A3B.ndi.NTamd64.HW]
Include = netvwifibus.inf
Needs   = PciASPMOptIn, VWiFiBus.PnPFilterRegistration

;21301A3B + WoWEnable
[ATHR_DEV_OS61_21301A3B_WoW.ndi.NTamd64]
Characteristics = 0x84
BusType         = 5
AddReg          = atheros_os61.reg, atheros11n.reg, htAdhoc.reg, aphroditeant2.reg, aphrodite_coex2.reg, ledcontrol8.reg, ConnectionFailure.reg, aphroditeantdiv2.reg, bt30_high_speed.reg, wowenable.reg
DelReg          = atheros.DelReg
CopyFiles       = atheros.CopyFiles
*IfType         = 71        ; IF_TYPE_IEEE80211
*MediaType      = 16        ; NdisMediumNative802_11
*PhysicalMediaType = 9      ; NdisPhysicalMediumNative802_11
Include         = netvwifibus.inf, machine.inf
Needs           = VWiFiBus.CopyFiles

[ATHR_DEV_OS61_21301A3B_WoW.ndi.NTamd64.Services]
AddService = athr, 2, atheros.Service, atheros.EventLog
Include    = netvwifibus.inf
Needs      = VWiFiBus.Services

[ATHR_DEV_OS61_21301A3B_WoW.ndi.NTamd64.HW]
Include = netvwifibus.inf
Needs   = PciASPMOptIn, VWiFiBus.PnPFilterRegistration

[ATHR_DEV_OS61_218D1A3B.ndi.NTamd64]
Characteristics = 0x84
BusType         = 5
AddReg          = atheros_os61.reg, atheros11n.reg, htAdhoc.reg, aphroditeant.reg, aphrodite_coex_ts.reg, ledcontrol8acthi.reg, ConnectionFailure.reg, aphroditeantdiv.reg, wowenable.reg, bt30_high_speed.reg, halBtcTSWar.reg
DelReg          = atheros.DelReg
CopyFiles       = atheros.CopyFiles
*IfType         = 71        ; IF_TYPE_IEEE80211
*MediaType      = 16        ; NdisMediumNative802_11
*PhysicalMediaType = 9      ; NdisPhysicalMediumNative802_11
Include         = netvwifibus.inf, machine.inf
Needs           = VWiFiBus.CopyFiles

[ATHR_DEV_OS61_218D1A3B.ndi.NTamd64.Services]
AddService = athr, 2, atheros.Service, atheros.EventLog
Include    = netvwifibus.inf
Needs      = VWiFiBus.Services

[ATHR_DEV_OS61_218D1A3B.ndi.NTamd64.HW]
Include = netvwifibus.inf
Needs   = PciASPMOptIn, VWiFiBus.PnPFilterRegistration

; 065211AD
[ATHR_DEV_OS61_065211AD.ndi.NTamd64]
Characteristics = 0x84
BusType         = 5
AddReg          = atheros_os61.reg, atheros11n.reg, htAdhoc.reg, aphroditeant2.reg, aphrodite_coex2.reg, ledcontrol8.reg, ConnectionFailure.reg, aphroditeantdiv2.reg, bt30_high_speed.reg, wowenable.reg
DelReg          = atheros.DelReg
CopyFiles       = atheros.CopyFiles
*IfType         = 71        ; IF_TYPE_IEEE80211
*MediaType      = 16        ; NdisMediumNative802_11
*PhysicalMediaType = 9      ; NdisPhysicalMediumNative802_11
Include         = netvwifibus.inf, machine.inf
Needs           = VWiFiBus.CopyFiles

[ATHR_DEV_OS61_065211AD.ndi.NTamd64.Services]
AddService = athr, 2, atheros.Service, atheros.EventLog
Include    = netvwifibus.inf
Needs      = VWiFiBus.Services

[ATHR_DEV_OS61_065211AD.ndi.NTamd64.HW]
Include = netvwifibus.inf
Needs   = PciASPMOptIn, VWiFiBus.PnPFilterRegistration

[ATHR_DEV_OS61_213B1A3B.ndi.NTamd64]
Characteristics = 0x84
BusType         = 5
AddReg          = atheros_os61.reg, atheros11n.reg, htAdhoc.reg, aphroditeant2.reg, aphrodite_coex2.reg, ledcontrol8.reg, ConnectionFailure.reg, aphroditeantdiv2.reg, A11swwow.reg, bt30_high_speed.reg
DelReg          = atheros.DelReg
CopyFiles       = atheros.CopyFiles
*IfType         = 71        ; IF_TYPE_IEEE80211
*MediaType      = 16        ; NdisMediumNative802_11
*PhysicalMediaType = 9      ; NdisPhysicalMediumNative802_11
Include         = netvwifibus.inf, machine.inf
Needs           = VWiFiBus.CopyFiles

[ATHR_DEV_OS61_213B1A3B.ndi.NTamd64.Services]
AddService = athr, 2, atheros.Service, atheros.EventLog
Include    = netvwifibus.inf
Needs      = VWiFiBus.Services

[ATHR_DEV_OS61_213B1A3B.ndi.NTamd64.HW]
AddReg  = MSI.reg
Include = netvwifibus.inf
Needs   = PciASPMOptIn, VWiFiBus.PnPFilterRegistration

[ATHR_DEV_OS61_85F21043.ndi.NTamd64]
Characteristics = 0x84
BusType         = 5
AddReg          = atheros_os61.reg, atheros11n.reg, htAdhoc.reg, aphroditeant2.reg, aphrodite_coex2.reg, ledcontrol8.reg, ConnectionFailure.reg, aphroditeantdiv2.reg
DelReg          = atheros.DelReg
CopyFiles       = atheros.CopyFiles
*IfType         = 71        ; IF_TYPE_IEEE80211
*MediaType      = 16        ; NdisMediumNative802_11
*PhysicalMediaType = 9      ; NdisPhysicalMediumNative802_11
Include         = netvwifibus.inf, machine.inf
Needs           = VWiFiBus.CopyFiles

[ATHR_DEV_OS61_85F21043.ndi.NTamd64.Services]
AddService = athr, 2, atheros.Service, atheros.EventLog
Include    = netvwifibus.inf
Needs      = VWiFiBus.Services

[ATHR_DEV_OS61_85F21043.ndi.NTamd64.HW]
Include = netvwifibus.inf
Needs   = PciASPMOptIn, VWiFiBus.PnPFilterRegistration

[ATHR_DEV_OS61_E08F105B.ndi.NTamd64]
Characteristics = 0x84
BusType         = 5
AddReg          = atheros_os61.reg, atheros11n.reg, htAdhoc.reg, aphroditeant2.reg, aphrodite_coex2.reg, ledcontrol8.reg, ConnectionFailure.reg, aphroditeantdiv2.reg
DelReg          = atheros.DelReg
CopyFiles       = atheros.CopyFiles
*IfType         = 71        ; IF_TYPE_IEEE80211
*MediaType      = 16        ; NdisMediumNative802_11
*PhysicalMediaType = 9      ; NdisPhysicalMediumNative802_11
Include         = netvwifibus.inf, machine.inf
Needs           = VWiFiBus.CopyFiles

[ATHR_DEV_OS61_E08F105B.ndi.NTamd64.Services]
AddService = athr, 2, atheros.Service, atheros.EventLog
Include    = netvwifibus.inf
Needs      = VWiFiBus.Services

[ATHR_DEV_OS61_E08F105B.ndi.NTamd64.HW]
Include = netvwifibus.inf
Needs   = PciASPMOptIn, VWiFiBus.PnPFilterRegistration

; Levi add for liteon pcie 1.1
[ATHR_DEV_OS61_067211AD_PCIE_1_1.ndi.NTamd64]
Characteristics = 0x84
BusType         = 5
AddReg          = atheros_os61.reg, atheros11n.reg, htAdhoc.reg, aphroditeant.reg, aphrodite_coex.reg, customer3gpcie11.reg, ConnectionFailure.reg, aphroditeantdiv.reg, wowenable.reg
DelReg          = atheros.DelReg
CopyFiles       = atheros.CopyFiles
*IfType         = 71        ; IF_TYPE_IEEE80211
*MediaType      = 16        ; NdisMediumNative802_11
*PhysicalMediaType = 9      ; NdisPhysicalMediumNative802_11
Include         = netvwifibus.inf, machine.inf
Needs           = VWiFiBus.CopyFiles

[ATHR_DEV_OS61_067211AD_PCIE_1_1.ndi.NTamd64.Services]
AddService = athr, 2, atheros.Service, atheros.EventLog
Include    = netvwifibus.inf
Needs      = VWiFiBus.Services

[ATHR_DEV_OS61_067211AD_PCIE_1_1.ndi.NTamd64.HW]
Include = netvwifibus.inf
Needs   = PciASPMOptIn, VWiFiBus.PnPFilterRegistration

[ATHR_DEV_OS61_081211AD.ndi.NTamd64]
Characteristics = 0x84
BusType         = 5
AddReg          = atheros_os61.reg, atheros11n.reg, smpsDynamic.reg, htAdhoc.reg, jupiter2ant.reg, wowenable.reg, customer3gpcie11.reg
DelReg          = atheros.DelReg
CopyFiles       = atheros.CopyFiles
*IfType         = 71        ; IF_TYPE_IEEE80211
*MediaType      = 16        ; NdisMediumNative802_11
*PhysicalMediaType = 9      ; NdisPhysicalMediumNative802_11
Include         = netvwifibus.inf, machine.inf
Needs           = VWiFiBus.CopyFiles

[ATHR_DEV_OS61_081211AD.ndi.NTamd64.Services]
AddService = athr, 2, atheros.Service, atheros.EventLog
Include    = netvwifibus.inf
Needs      = VWiFiBus.Services

[ATHR_DEV_OS61_081211AD.ndi.NTamd64.HW]
Include = netvwifibus.inf
Needs   = PciASPMOptIn, VWiFiBus.PnPFilterRegistration

[ATHR_DEV_OS61_066211AD.ndi.NTamd64]
Characteristics = 0x84
BusType         = 5
AddReg          = atheros_os61.reg, atheros11n.reg, htAdhoc.reg, aphroditeant.reg, aphrodite_coex.reg, ledcontrol8.reg, ConnectionFailure.reg, aphroditeantdiv.reg, bt30_high_speed.reg, wowenable.reg
DelReg          = atheros.DelReg
CopyFiles       = atheros.CopyFiles
*IfType         = 71        ; IF_TYPE_IEEE80211
*MediaType      = 16        ; NdisMediumNative802_11
*PhysicalMediaType = 9      ; NdisPhysicalMediumNative802_11
Include         = netvwifibus.inf, machine.inf
Needs           = VWiFiBus.CopyFiles

[ATHR_DEV_OS61_066211AD.ndi.NTamd64.Services]
AddService = athr, 2, atheros.Service, atheros.EventLog
Include    = netvwifibus.inf
Needs      = VWiFiBus.Services

[ATHR_DEV_OS61_066211AD.ndi.NTamd64.HW]
Include = netvwifibus.inf
Needs   = PciASPMOptIn, VWiFiBus.PnPFilterRegistration

[ATHR_DEV_OS61_218B1A3B.ndi.NTamd64]
Characteristics = 0x84
BusType         = 5
AddReg          = atheros_os61.reg, atheros11n.reg, htAdhoc.reg, aphroditeant2.reg, aphrodite_coex2.reg, ledcontrol8acthi.reg, ConnectionFailure.reg, aphroditeantdiv2.reg, AphroditeMitiShift.reg, customer_power.reg, cfpignore.reg, A11swwow.reg
DelReg          = atheros.DelReg
CopyFiles       = atheros.CopyFiles
*IfType         = 71        ; IF_TYPE_IEEE80211
*MediaType      = 16        ; NdisMediumNative802_11
*PhysicalMediaType = 9      ; NdisPhysicalMediumNative802_11
Include         = netvwifibus.inf, machine.inf
Needs           = VWiFiBus.CopyFiles

[ATHR_DEV_OS61_218B1A3B.ndi.NTamd64.Services]
AddService = athr, 2, atheros.Service, atheros.EventLog
Include    = netvwifibus.inf
Needs      = VWiFiBus.Services

[ATHR_DEV_OS61_218B1A3B.ndi.NTamd64.HW]
Include = netvwifibus.inf
Needs   = PciASPMOptIn, VWiFiBus.PnPFilterRegistration

[ATHR_DEV_OS61_21761A3B.ndi.NTamd64]
Characteristics = 0x84
BusType         = 5
AddReg          = atheros_os61.reg, atheros11n.reg, htAdhoc.reg, aphroditeant2.reg, aphrodite_coex2.reg, ledcontrol8.reg, ConnectionFailure.reg, aphroditeantdiv2.reg, bt30_high_speed.reg
DelReg          = atheros.DelReg
CopyFiles       = atheros.CopyFiles
*IfType         = 71        ; IF_TYPE_IEEE80211
*MediaType      = 16        ; NdisMediumNative802_11
*PhysicalMediaType = 9      ; NdisPhysicalMediumNative802_11
Include         = netvwifibus.inf, machine.inf
Needs           = VWiFiBus.CopyFiles

[ATHR_DEV_OS61_21761A3B.ndi.NTamd64.Services]
AddService = athr, 2, atheros.Service, atheros.EventLog
Include    = netvwifibus.inf
Needs      = VWiFiBus.Services

[ATHR_DEV_OS61_21761A3B.ndi.NTamd64.HW]
Include = netvwifibus.inf
Needs   = PciASPMOptIn, VWiFiBus.PnPFilterRegistration

[ATHR_DEV_OS61_213A1A3B.ndi.NTamd64]
Characteristics = 0x84
BusType         = 5
AddReg          = atheros_os61.reg, atheros11n.reg, htAdhoc.reg, aphroditeant.reg, aphrodite_coex_ts.reg, ledcontrol8.reg, ConnectionFailure.reg, aphroditeantdiv.reg, bt30_high_speed.reg, wowenable.reg, halBtcTSWar.reg
DelReg          = atheros.DelReg
CopyFiles       = atheros.CopyFiles
*IfType         = 71        ; IF_TYPE_IEEE80211
*MediaType      = 16        ; NdisMediumNative802_11
*PhysicalMediaType = 9      ; NdisPhysicalMediumNative802_11
Include         = netvwifibus.inf, machine.inf
Needs           = VWiFiBus.CopyFiles

[ATHR_DEV_OS61_213A1A3B.ndi.NTamd64.Services]
AddService = athr, 2, atheros.Service, atheros.EventLog
Include    = netvwifibus.inf
Needs      = VWiFiBus.Services

[ATHR_DEV_OS61_213A1A3B.ndi.NTamd64.HW]
Include = netvwifibus.inf
Needs   = PciASPMOptIn, VWiFiBus.PnPFilterRegistration

[ATHR_DEV_OS61_213C1A3B.ndi.NTamd64]
Characteristics = 0x84
BusType         = 5
AddReg          = atheros_os61.reg, atheros11n.reg, htAdhoc.reg, aphroditeant.reg, aphrodite_coex.reg, ledcontrol8.reg, ConnectionFailure.reg, aphroditeantdiv.reg, bt30_high_speed.reg, wowEnable.reg
DelReg          = atheros.DelReg
CopyFiles       = atheros.CopyFiles
*IfType         = 71        ; IF_TYPE_IEEE80211
*MediaType      = 16        ; NdisMediumNative802_11
*PhysicalMediaType = 9      ; NdisPhysicalMediumNative802_11
Include         = netvwifibus.inf, machine.inf
Needs           = VWiFiBus.CopyFiles

[ATHR_DEV_OS61_213C1A3B.ndi.NTamd64.Services]
AddService = athr, 2, atheros.Service, atheros.EventLog
Include    = netvwifibus.inf
Needs      = VWiFiBus.Services

[ATHR_DEV_OS61_213C1A3B.ndi.NTamd64.HW]
Include = netvwifibus.inf
Needs   = PciASPMOptIn, VWiFiBus.PnPFilterRegistration

[ATHR_DEV_OS61_T956x.ndi.NTamd64]
Characteristics = 0x84
BusType         = 5
AddReg          = atheros_os61.reg, atheros11n.reg, htAdhoc.reg, aphroditeant2.reg, aphrodite_coex2.reg, ledcontrol8.reg, ConnectionFailure.reg, aphroditeantdiv2.reg, AphroditeMitiShift.reg, customer_power_Toshiba.reg, cfpignore.reg, wowenable.reg
DelReg          = atheros.DelReg
CopyFiles       = atheros.CopyFiles
*IfType         = 71        ; IF_TYPE_IEEE80211
*MediaType      = 16        ; NdisMediumNative802_11
*PhysicalMediaType = 9      ; NdisPhysicalMediumNative802_11
Include         = netvwifibus.inf, machine.inf
Needs           = VWiFiBus.CopyFiles

[ATHR_DEV_OS61_T956x.ndi.NTamd64.Services]
AddService = athr, 2, atheros.Service, atheros.EventLog
Include    = netvwifibus.inf
Needs      = VWiFiBus.Services

[ATHR_DEV_OS61_T956x.ndi.NTamd64.HW]
Include = netvwifibus.inf
Needs   = PciASPMOptIn, VWiFiBus.PnPFilterRegistration

[ATHR_DEV_OS61_T956x_1.ndi.NTamd64]
Characteristics = 0x84
BusType         = 5
AddReg          = atheros_os61.reg, atheros11n.reg, htAdhoc.reg, aphroditeant.reg, aphrodite_coex.reg, ledcontrol8.reg, ConnectionFailure.reg, AphroditeMitiShift.reg, customer_power_Toshiba.reg, cfpignore.reg, wowenable.reg
DelReg          = atheros.DelReg
CopyFiles       = atheros.CopyFiles
*IfType         = 71        ; IF_TYPE_IEEE80211
*MediaType      = 16        ; NdisMediumNative802_11
*PhysicalMediaType = 9      ; NdisPhysicalMediumNative802_11
Include         = netvwifibus.inf, machine.inf
Needs           = VWiFiBus.CopyFiles

[ATHR_DEV_OS61_T956x_1.ndi.NTamd64.Services]
AddService = athr, 2, atheros.Service, atheros.EventLog
Include    = netvwifibus.inf
Needs      = VWiFiBus.Services

[ATHR_DEV_OS61_T956x_1.ndi.NTamd64.HW]
Include = netvwifibus.inf
Needs   = PciASPMOptIn, VWiFiBus.PnPFilterRegistration

[ATHR_DEV_OS61_21821A3B.ndi.NTamd64]
Characteristics = 0x84
BusType         = 5
AddReg          = atheros_os61.reg, atheros11n.reg, htAdhoc.reg, aphroditeant2.reg, aphrodite_coex2.reg, ledcontrol8acthi.reg, ConnectionFailure.reg, aphroditeantdiv2.reg, AphroditeMitiShift.reg, customer_power_Toshiba.reg, cfpignore.reg, wowenable.reg
DelReg          = atheros.DelReg
CopyFiles       = atheros.CopyFiles
*IfType         = 71        ; IF_TYPE_IEEE80211
*MediaType      = 16        ; NdisMediumNative802_11
*PhysicalMediaType = 9      ; NdisPhysicalMediumNative802_11
Include         = netvwifibus.inf, machine.inf
Needs           = VWiFiBus.CopyFiles

[ATHR_DEV_OS61_21821A3B.ndi.NTamd64.Services]
AddService = athr, 2, atheros.Service, atheros.EventLog
Include    = netvwifibus.inf
Needs      = VWiFiBus.Services

[ATHR_DEV_OS61_21821A3B.ndi.NTamd64.HW]
Include = netvwifibus.inf
Needs   = PciASPMOptIn, VWiFiBus.PnPFilterRegistration

[ATHR_DEV_OS61_3027168C.ndi.NTamd64]
Characteristics = 0x84
BusType         = 5
AddReg          = atheros_os61.reg, atheros11n.reg, htAdhoc.reg, aphroditeant2.reg, aphrodite_coex2.reg, ledcontrol8.reg, ConnectionFailure.reg, aphroditeantdiv2.reg
DelReg          = atheros.DelReg
CopyFiles       = atheros.CopyFiles
*IfType         = 71        ; IF_TYPE_IEEE80211
*MediaType      = 16        ; NdisMediumNative802_11
*PhysicalMediaType = 9      ; NdisPhysicalMediumNative802_11
Include         = netvwifibus.inf, machine.inf
Needs           = VWiFiBus.CopyFiles

[ATHR_DEV_OS61_3027168C.ndi.NTamd64.Services]
AddService = athr, 2, atheros.Service, atheros.EventLog
Include    = netvwifibus.inf
Needs      = VWiFiBus.Services

[ATHR_DEV_OS61_3027168C.ndi.NTamd64.HW]
Include = netvwifibus.inf
Needs   = PciASPMOptIn, VWiFiBus.PnPFilterRegistration

[ATHR_DEV_OS61_3028.ndi.NTamd64]
Characteristics = 0x84
BusType         = 5
AddReg          = atheros_os61.reg, atheros11n.reg, htAdhoc.reg, aphroditeant2.reg, aphrodite_coex2.reg, ledcontrol8.reg, ConnectionFailure.reg, aphroditeantdiv2.reg
DelReg          = atheros.DelReg
CopyFiles       = atheros.CopyFiles
*IfType         = 71        ; IF_TYPE_IEEE80211
*MediaType      = 16        ; NdisMediumNative802_11
*PhysicalMediaType = 9      ; NdisPhysicalMediumNative802_11
Include         = netvwifibus.inf, machine.inf
Needs           = VWiFiBus.CopyFiles

[ATHR_DEV_OS61_3028.ndi.NTamd64.Services]
AddService = athr, 2, atheros.Service, atheros.EventLog
Include    = netvwifibus.inf
Needs      = VWiFiBus.Services

[ATHR_DEV_OS61_3028.ndi.NTamd64.HW]
Include = netvwifibus.inf
Needs   = PciASPMOptIn, VWiFiBus.PnPFilterRegistration

[ATHR_DEV_OS61_302617AA.ndi.NTamd64]
Characteristics = 0x84
BusType         = 5
AddReg          = atheros_os61.reg, atheros11n.reg, htAdhoc.reg, aphroditeant2.reg, aphrodite_coex2.reg, ledcontrol8.reg, ConnectionFailure.reg, wowenable.reg, aphroditeantdiv2.reg, bt30_high_speed.reg, MAEnable.reg
DelReg          = atheros.DelReg
CopyFiles       = atheros.CopyFiles
*IfType         = 71        ; IF_TYPE_IEEE80211
*MediaType      = 16        ; NdisMediumNative802_11
*PhysicalMediaType = 9      ; NdisPhysicalMediumNative802_11
Include         = netvwifibus.inf, machine.inf
Needs           = VWiFiBus.CopyFiles

[ATHR_DEV_OS61_302617AA.ndi.NTamd64.Services]
AddService = athr, 2, atheros.Service, atheros.EventLog
Include    = netvwifibus.inf
Needs      = VWiFiBus.Services

[ATHR_DEV_OS61_302617AA.ndi.NTamd64.HW]
Include = netvwifibus.inf
Needs   = PciASPMOptIn, VWiFiBus.PnPFilterRegistration

[ATHR_DEV_OS61_402617AA.ndi.NTamd64]
Characteristics = 0x84
BusType         = 5
AddReg          = atheros_os61.reg, atheros11n.reg, htAdhoc.reg, aphroditeant2.reg, aphrodite_coex2.reg, ledcontrol8acthi.reg, ConnectionFailure.reg, wowenable.reg, aphroditeantdiv2.reg, bt30_high_speed.reg, MAEnable.reg, aphrodite_coexPTA_34_25.reg, customer_power.reg, forceMaxPowerSave.reg
DelReg          = atheros.DelReg
CopyFiles       = atheros.CopyFiles
*IfType         = 71        ; IF_TYPE_IEEE80211
*MediaType      = 16        ; NdisMediumNative802_11
*PhysicalMediaType = 9      ; NdisPhysicalMediumNative802_11
Include         = netvwifibus.inf, machine.inf
Needs           = VWiFiBus.CopyFiles

[ATHR_DEV_OS61_402617AA.ndi.NTamd64.Services]
AddService = athr, 2, atheros.Service, atheros.EventLog
Include    = netvwifibus.inf
Needs      = VWiFiBus.Services

[ATHR_DEV_OS61_402617AA.ndi.NTamd64.HW]
Include = netvwifibus.inf
Needs   = PciASPMOptIn, VWiFiBus.PnPFilterRegistration

[ATHR_DEV_OS61_9580.ndi.NTamd64]
Characteristics = 0x84
BusType         = 5
AddReg          = atheros_os61.reg, atheros11n.reg, smpsDynamic.reg, htAdhoc.reg
DelReg          = atheros.DelReg
CopyFiles       = atheros.CopyFiles
*IfType         = 71        ; IF_TYPE_IEEE80211
*MediaType      = 16        ; NdisMediumNative802_11
*PhysicalMediaType = 9      ; NdisPhysicalMediumNative802_11
Include         = netvwifibus.inf, machine.inf
Needs           = VWiFiBus.CopyFiles

[ATHR_DEV_OS61_9580.ndi.NTamd64.Services]
AddService = athr, 2, atheros.Service, atheros.EventLog
Include    = netvwifibus.inf
Needs      = VWiFiBus.Services

[ATHR_DEV_OS61_9580.ndi.NTamd64.HW]
AddReg  = MSI.reg
Include = netvwifibus.inf
Needs   = PciASPMOptIn, VWiFiBus.PnPFilterRegistration

[ATHR_DEV_OS61_651311AD.ndi.NTamd64]
Characteristics = 0x84
BusType         = 5
AddReg          = atheros_os61.reg, atheros11n.reg, smpsDynamic.reg, htAdhoc.reg, cemspecled_func2_10.reg
DelReg          = atheros.DelReg
CopyFiles       = atheros.CopyFiles
*IfType         = 71        ; IF_TYPE_IEEE80211
*MediaType      = 16        ; NdisMediumNative802_11
*PhysicalMediaType = 9      ; NdisPhysicalMediumNative802_11
Include         = netvwifibus.inf, machine.inf
Needs           = VWiFiBus.CopyFiles

[ATHR_DEV_OS61_651311AD.ndi.NTamd64.Services]
AddService = athr, 2, atheros.Service, atheros.EventLog
Include    = netvwifibus.inf
Needs      = VWiFiBus.Services

[ATHR_DEV_OS61_651311AD.ndi.NTamd64.HW]
AddReg  = MSI.reg
Include = netvwifibus.inf
Needs   = VWiFiBus.PnPFilterRegistration

[ATHR_DEV_OS61_652311AD.ndi.NTamd64]
Characteristics = 0x84
BusType         = 5
AddReg          = atheros_os61.reg, atheros11n.reg, smpsDynamic.reg, htAdhoc.reg, cemspecled_func1_10.reg
DelReg          = atheros.DelReg
CopyFiles       = atheros.CopyFiles
*IfType         = 71        ; IF_TYPE_IEEE80211
*MediaType      = 16        ; NdisMediumNative802_11
*PhysicalMediaType = 9      ; NdisPhysicalMediumNative802_11
Include         = netvwifibus.inf, machine.inf
Needs           = VWiFiBus.CopyFiles

[ATHR_DEV_OS61_652311AD.ndi.NTamd64.Services]
AddService = athr, 2, atheros.Service, atheros.EventLog
Include    = netvwifibus.inf
Needs      = VWiFiBus.Services

[ATHR_DEV_OS61_652311AD.ndi.NTamd64.HW]
AddReg  = MSI.reg
Include = netvwifibus.inf
Needs   = VWiFiBus.PnPFilterRegistration

[ATHR_DEV_OS61_0013.ndi.NTamd64]
Characteristics = 0x84
BusType         = 5
AddReg          = atheros_os61.reg, atheros.reg
DelReg          = atheros.DelReg
CopyFiles       = atheros.CopyFiles
*IfType         = 71        ; IF_TYPE_IEEE80211
*MediaType      = 16        ; NdisMediumNative802_11
*PhysicalMediaType = 9      ; NdisPhysicalMediumNative802_11
Include         = netvwifibus.inf, machine.inf
Needs           = VWiFiBus.CopyFiles

[ATHR_DEV_OS61_0013.ndi.NTamd64.Services]
AddService = athr, 2, atheros.Service, atheros.EventLog
Include    = netvwifibus.inf
Needs      = VWiFiBus.Services

[ATHR_DEV_OS61_0013.ndi.NTamd64.HW]
Include = netvwifibus.inf
Needs   = VWiFiBus.PnPFilterRegistration

[ATHR_DEV_OS61_001A.ndi.NTamd64]
Characteristics = 0x84
BusType         = 5
AddReg          = atheros_os61.reg, atheros.reg, cfpignore.reg
DelReg          = atheros.DelReg
CopyFiles       = atheros.CopyFiles
*IfType         = 71        ; IF_TYPE_IEEE80211
*MediaType      = 16        ; NdisMediumNative802_11
*PhysicalMediaType = 9      ; NdisPhysicalMediumNative802_11
Include         = netvwifibus.inf, machine.inf
Needs           = VWiFiBus.CopyFiles

[ATHR_DEV_OS61_001A.ndi.NTamd64.Services]
AddService = athr, 2, atheros.Service, atheros.EventLog
Include    = netvwifibus.inf
Needs      = VWiFiBus.Services

[ATHR_DEV_OS61_001A.ndi.NTamd64.HW]
Include = netvwifibus.inf
Needs   = VWiFiBus.PnPFilterRegistration

[ATHR_DEV_OS61_001B.ndi.NTamd64]
Characteristics = 0x84
BusType         = 5
AddReg          = atheros_os61.reg, atheros.reg, cfpignore.reg
DelReg          = atheros.DelReg
CopyFiles       = atheros.CopyFiles
*IfType         = 71        ; IF_TYPE_IEEE80211
*MediaType      = 16        ; NdisMediumNative802_11
*PhysicalMediaType = 9      ; NdisPhysicalMediumNative802_11
Include         = netvwifibus.inf, machine.inf
Needs           = VWiFiBus.CopyFiles

[ATHR_DEV_OS61_001B.ndi.NTamd64.Services]
AddService = athr, 2, atheros.Service, atheros.EventLog
Include    = netvwifibus.inf
Needs      = VWiFiBus.Services

[ATHR_DEV_OS61_001B.ndi.NTamd64.HW]
Include = netvwifibus.inf
Needs   = VWiFiBus.PnPFilterRegistration

[ATHR_DEV_OS61_001C.ndi.NTamd64]
Characteristics = 0x84
BusType         = 5
AddReg          = atheros_os61.reg, atheros.reg, cfpignore.reg
DelReg          = atheros.DelReg
CopyFiles       = atheros.CopyFiles
*IfType         = 71        ; IF_TYPE_IEEE80211
*MediaType      = 16        ; NdisMediumNative802_11
*PhysicalMediaType = 9      ; NdisPhysicalMediumNative802_11
Include         = netvwifibus.inf, machine.inf
Needs           = VWiFiBus.CopyFiles

[ATHR_DEV_OS61_001C.ndi.NTamd64.Services]
AddService = athr, 2, atheros.Service, atheros.EventLog
Include    = netvwifibus.inf
Needs      = VWiFiBus.Services

[ATHR_DEV_OS61_001C.ndi.NTamd64.HW]
Include = netvwifibus.inf
Needs   = VWiFiBus.PnPFilterRegistration

[ATHR_DEV_OS61_6313.ndi.NTamd64]
Characteristics = 0x84
BusType         = 5
AddReg          = atheros_os61.reg, atheros.reg, cemspecled_func1_3.reg, d3hot.reg
DelReg          = atheros.DelReg
CopyFiles       = atheros.CopyFiles
*IfType         = 71        ; IF_TYPE_IEEE80211
*MediaType      = 16        ; NdisMediumNative802_11
*PhysicalMediaType = 9      ; NdisPhysicalMediumNative802_11
Include         = netvwifibus.inf, machine.inf
Needs           = VWiFiBus.CopyFiles

[ATHR_DEV_OS61_6313.ndi.NTamd64.Services]
AddService = athr, 2, atheros.Service, atheros.EventLog
Include    = netvwifibus.inf
Needs      = VWiFiBus.Services

[ATHR_DEV_OS61_6313.ndi.NTamd64.HW]
Include = netvwifibus.inf
Needs   = VWiFiBus.PnPFilterRegistration

[ATHR_DEV_OS61_3064.ndi.NTamd64]
Characteristics = 0x84
BusType         = 5
AddReg          = atheros_os61.reg, atheros.reg
DelReg          = atheros.DelReg
CopyFiles       = atheros.CopyFiles
*IfType         = 71        ; IF_TYPE_IEEE80211
*MediaType      = 16        ; NdisMediumNative802_11
*PhysicalMediaType = 9      ; NdisPhysicalMediumNative802_11
Include         = netvwifibus.inf, machine.inf
Needs           = VWiFiBus.CopyFiles

[ATHR_DEV_OS61_3064.ndi.NTamd64.Services]
AddService = athr, 2, atheros.Service, atheros.EventLog
Include    = netvwifibus.inf
Needs      = VWiFiBus.Services

[ATHR_DEV_OS61_3064.ndi.NTamd64.HW]
Include = netvwifibus.inf
Needs   = VWiFiBus.PnPFilterRegistration

[ATHR_DEV_OS61_1055.ndi.NTamd64]
Characteristics = 0x84
BusType         = 5
AddReg          = atheros_os61.reg, atheros.reg, gpioled.reg
DelReg          = atheros.DelReg
CopyFiles       = atheros.CopyFiles
*IfType         = 71        ; IF_TYPE_IEEE80211
*MediaType      = 16        ; NdisMediumNative802_11
*PhysicalMediaType = 9      ; NdisPhysicalMediumNative802_11
Include         = netvwifibus.inf, machine.inf
Needs           = VWiFiBus.CopyFiles

[ATHR_DEV_OS61_1055.ndi.NTamd64.Services]
AddService = athr, 2, atheros.Service, atheros.EventLog
Include    = netvwifibus.inf
Needs      = VWiFiBus.Services

[ATHR_DEV_OS61_1055.ndi.NTamd64.HW]
Include = netvwifibus.inf
Needs   = VWiFiBus.PnPFilterRegistration

[ATHR_DEV_OS61_2055.ndi.NTamd64]
Characteristics = 0x84
BusType         = 5
AddReg          = atheros_os61.reg, atheros.reg
DelReg          = atheros.DelReg
CopyFiles       = atheros.CopyFiles
*IfType         = 71        ; IF_TYPE_IEEE80211
*MediaType      = 16        ; NdisMediumNative802_11
*PhysicalMediaType = 9      ; NdisPhysicalMediumNative802_11
Include         = netvwifibus.inf, machine.inf
Needs           = VWiFiBus.CopyFiles

[ATHR_DEV_OS61_2055.ndi.NTamd64.Services]
AddService = athr, 2, atheros.Service, atheros.EventLog
Include    = netvwifibus.inf
Needs      = VWiFiBus.Services

[ATHR_DEV_OS61_2055.ndi.NTamd64.HW]
Include = netvwifibus.inf
Needs   = VWiFiBus.PnPFilterRegistration

[ATHR_DEV_OS61_1030.ndi.NTamd64]
Characteristics = 0x84
BusType         = 5
AddReg          = atheros_os61.reg, atheros.reg
DelReg          = atheros.DelReg
CopyFiles       = atheros.CopyFiles
*IfType         = 71        ; IF_TYPE_IEEE80211
*MediaType      = 16        ; NdisMediumNative802_11
*PhysicalMediaType = 9      ; NdisPhysicalMediumNative802_11
Include         = netvwifibus.inf, machine.inf
Needs           = VWiFiBus.CopyFiles

[ATHR_DEV_OS61_1030.ndi.NTamd64.Services]
AddService = athr, 2, atheros.Service, atheros.EventLog
Include    = netvwifibus.inf
Needs      = VWiFiBus.Services

[ATHR_DEV_OS61_1030.ndi.NTamd64.HW]
Include = netvwifibus.inf
Needs   = VWiFiBus.PnPFilterRegistration

[ATHR_DEV_OS61_2030.ndi.NTamd64]
Characteristics = 0x84
BusType         = 5
AddReg          = atheros_os61.reg, atheros.reg
DelReg          = atheros.DelReg
CopyFiles       = atheros.CopyFiles
*IfType         = 71        ; IF_TYPE_IEEE80211
*MediaType      = 16        ; NdisMediumNative802_11
*PhysicalMediaType = 9      ; NdisPhysicalMediumNative802_11
Include         = netvwifibus.inf, machine.inf
Needs           = VWiFiBus.CopyFiles

[ATHR_DEV_OS61_2030.ndi.NTamd64.Services]
AddService = athr, 2, atheros.Service, atheros.EventLog
Include    = netvwifibus.inf
Needs      = VWiFiBus.Services

[ATHR_DEV_OS61_2030.ndi.NTamd64.HW]
Include = netvwifibus.inf
Needs   = VWiFiBus.PnPFilterRegistration

[ATHR_DEV_OS61_1031.ndi.NTamd64]
Characteristics = 0x84
BusType         = 5
AddReg          = atheros_os61.reg, atheros.reg
DelReg          = atheros.DelReg
CopyFiles       = atheros.CopyFiles
*IfType         = 71        ; IF_TYPE_IEEE80211
*MediaType      = 16        ; NdisMediumNative802_11
*PhysicalMediaType = 9      ; NdisPhysicalMediumNative802_11
Include         = netvwifibus.inf, machine.inf
Needs           = VWiFiBus.CopyFiles

[ATHR_DEV_OS61_1031.ndi.NTamd64.Services]
AddService = athr, 2, atheros.Service, atheros.EventLog
Include    = netvwifibus.inf
Needs      = VWiFiBus.Services

[ATHR_DEV_OS61_1031.ndi.NTamd64.HW]
Include = netvwifibus.inf
Needs   = VWiFiBus.PnPFilterRegistration

[ATHR_DEV_OS61_2031.ndi.NTamd64]
Characteristics = 0x84
BusType         = 5
AddReg          = atheros_os61.reg, atheros.reg
DelReg          = atheros.DelReg
CopyFiles       = atheros.CopyFiles
*IfType         = 71        ; IF_TYPE_IEEE80211
*MediaType      = 16        ; NdisMediumNative802_11
*PhysicalMediaType = 9      ; NdisPhysicalMediumNative802_11
Include         = netvwifibus.inf, machine.inf
Needs           = VWiFiBus.CopyFiles

[ATHR_DEV_OS61_2031.ndi.NTamd64.Services]
AddService = athr, 2, atheros.Service, atheros.EventLog
Include    = netvwifibus.inf
Needs      = VWiFiBus.Services

[ATHR_DEV_OS61_2031.ndi.NTamd64.HW]
Include = netvwifibus.inf
Needs   = VWiFiBus.PnPFilterRegistration

[ATHR_DEV_OS61_1041.ndi.NTamd64]
Characteristics = 0x84
BusType         = 5
AddReg          = atheros_os61.reg, atheros.reg
DelReg          = atheros.DelReg
CopyFiles       = atheros.CopyFiles
*IfType         = 71        ; IF_TYPE_IEEE80211
*MediaType      = 16        ; NdisMediumNative802_11
*PhysicalMediaType = 9      ; NdisPhysicalMediumNative802_11
Include         = netvwifibus.inf, machine.inf
Needs           = VWiFiBus.CopyFiles

[ATHR_DEV_OS61_1041.ndi.NTamd64.Services]
AddService = athr, 2, atheros.Service, atheros.EventLog
Include    = netvwifibus.inf
Needs      = VWiFiBus.Services

[ATHR_DEV_OS61_1041.ndi.NTamd64.HW]
Include = netvwifibus.inf
Needs   = VWiFiBus.PnPFilterRegistration

[ATHR_DEV_OS61_2041.ndi.NTamd64]
Characteristics = 0x84
BusType         = 5
AddReg          = atheros_os61.reg, atheros.reg, cfpignore.reg
DelReg          = atheros.DelReg
CopyFiles       = atheros.CopyFiles
*IfType         = 71        ; IF_TYPE_IEEE80211
*MediaType      = 16        ; NdisMediumNative802_11
*PhysicalMediaType = 9      ; NdisPhysicalMediumNative802_11
Include         = netvwifibus.inf, machine.inf
Needs           = VWiFiBus.CopyFiles

[ATHR_DEV_OS61_2041.ndi.NTamd64.Services]
AddService = athr, 2, atheros.Service, atheros.EventLog
Include    = netvwifibus.inf
Needs      = VWiFiBus.Services

[ATHR_DEV_OS61_2041.ndi.NTamd64.HW]
Include = netvwifibus.inf
Needs   = VWiFiBus.PnPFilterRegistration

[ATHR_DEV_OS61_1042.ndi.NTamd64]
Characteristics = 0x84
BusType         = 5
AddReg          = atheros_os61.reg, atheros.reg
DelReg          = atheros.DelReg
CopyFiles       = atheros.CopyFiles
*IfType         = 71        ; IF_TYPE_IEEE80211
*MediaType      = 16        ; NdisMediumNative802_11
*PhysicalMediaType = 9      ; NdisPhysicalMediumNative802_11
Include         = netvwifibus.inf, machine.inf
Needs           = VWiFiBus.CopyFiles

[ATHR_DEV_OS61_1042.ndi.NTamd64.Services]
AddService = athr, 2, atheros.Service, atheros.EventLog
Include    = netvwifibus.inf
Needs      = VWiFiBus.Services

[ATHR_DEV_OS61_1042.ndi.NTamd64.HW]
Include = netvwifibus.inf
Needs   = VWiFiBus.PnPFilterRegistration

[ATHR_DEV_OS61_2042.ndi.NTamd64]
Characteristics = 0x84
BusType         = 5
AddReg          = atheros_os61.reg, atheros.reg, cfpignore.reg
DelReg          = atheros.DelReg
CopyFiles       = atheros.CopyFiles
*IfType         = 71        ; IF_TYPE_IEEE80211
*MediaType      = 16        ; NdisMediumNative802_11
*PhysicalMediaType = 9      ; NdisPhysicalMediumNative802_11
Include         = netvwifibus.inf, machine.inf
Needs           = VWiFiBus.CopyFiles

[ATHR_DEV_OS61_2042.ndi.NTamd64.Services]
AddService = athr, 2, atheros.Service, atheros.EventLog
Include    = netvwifibus.inf
Needs      = VWiFiBus.Services

[ATHR_DEV_OS61_2042.ndi.NTamd64.HW]
Include = netvwifibus.inf
Needs   = VWiFiBus.PnPFilterRegistration

[ATHR_DEV_OS61_1051.ndi.NTamd64]
Characteristics = 0x84
BusType         = 5
AddReg          = atheros_os61.reg, atheros.reg
DelReg          = atheros.DelReg
CopyFiles       = atheros.CopyFiles
*IfType         = 71        ; IF_TYPE_IEEE80211
*MediaType      = 16        ; NdisMediumNative802_11
*PhysicalMediaType = 9      ; NdisPhysicalMediumNative802_11
Include         = netvwifibus.inf, machine.inf
Needs           = VWiFiBus.CopyFiles

[ATHR_DEV_OS61_1051.ndi.NTamd64.Services]
AddService = athr, 2, atheros.Service, atheros.EventLog
Include    = netvwifibus.inf
Needs      = VWiFiBus.Services

[ATHR_DEV_OS61_1051.ndi.NTamd64.HW]
Include = netvwifibus.inf
Needs   = VWiFiBus.PnPFilterRegistration

[ATHR_DEV_OS61_2051.ndi.NTamd64]
Characteristics = 0x84
BusType         = 5
AddReg          = atheros_os61.reg, atheros.reg, cfpignore.reg
DelReg          = atheros.DelReg
CopyFiles       = atheros.CopyFiles
*IfType         = 71        ; IF_TYPE_IEEE80211
*MediaType      = 16        ; NdisMediumNative802_11
*PhysicalMediaType = 9      ; NdisPhysicalMediumNative802_11
Include         = netvwifibus.inf, machine.inf
Needs           = VWiFiBus.CopyFiles

[ATHR_DEV_OS61_2051.ndi.NTamd64.Services]
AddService = athr, 2, atheros.Service, atheros.EventLog
Include    = netvwifibus.inf
Needs      = VWiFiBus.Services

[ATHR_DEV_OS61_2051.ndi.NTamd64.HW]
Include = netvwifibus.inf
Needs   = VWiFiBus.PnPFilterRegistration

[ATHR_DEV_OS61_7111144F.ndi.NTamd64]
Characteristics = 0x84
BusType         = 5
AddReg          = atheros_os61.reg, atheros.reg, expresscardaspmoff.reg
DelReg          = atheros.DelReg
CopyFiles       = atheros.CopyFiles
*IfType         = 71        ; IF_TYPE_IEEE80211
*MediaType      = 16        ; NdisMediumNative802_11
*PhysicalMediaType = 9      ; NdisPhysicalMediumNative802_11
Include         = netvwifibus.inf, machine.inf
Needs           = VWiFiBus.CopyFiles

[ATHR_DEV_OS61_7111144F.ndi.NTamd64.Services]
AddService = athr, 2, atheros.Service, atheros.EventLog
Include    = netvwifibus.inf
Needs      = VWiFiBus.Services

[ATHR_DEV_OS61_7111144F.ndi.NTamd64.HW]
Include = netvwifibus.inf
Needs   = VWiFiBus.PnPFilterRegistration

[ATHR_DEV_OS61_1052.ndi.NTamd64]
Characteristics = 0x84
BusType         = 5
AddReg          = atheros_os61.reg, atheros.reg
DelReg          = atheros.DelReg
CopyFiles       = atheros.CopyFiles
*IfType         = 71        ; IF_TYPE_IEEE80211
*MediaType      = 16        ; NdisMediumNative802_11
*PhysicalMediaType = 9      ; NdisPhysicalMediumNative802_11
Include         = netvwifibus.inf, machine.inf
Needs           = VWiFiBus.CopyFiles

[ATHR_DEV_OS61_1052.ndi.NTamd64.Services]
AddService = athr, 2, atheros.Service, atheros.EventLog
Include    = netvwifibus.inf
Needs      = VWiFiBus.Services

[ATHR_DEV_OS61_1052.ndi.NTamd64.HW]
Include = netvwifibus.inf
Needs   = VWiFiBus.PnPFilterRegistration

[ATHR_DEV_OS61_2052.ndi.NTamd64]
Characteristics = 0x84
BusType         = 5
AddReg          = atheros_os61.reg, atheros.reg, cfpignore.reg
DelReg          = atheros.DelReg
CopyFiles       = atheros.CopyFiles
*IfType         = 71        ; IF_TYPE_IEEE80211
*MediaType      = 16        ; NdisMediumNative802_11
*PhysicalMediaType = 9      ; NdisPhysicalMediumNative802_11
Include         = netvwifibus.inf, machine.inf
Needs           = VWiFiBus.CopyFiles

[ATHR_DEV_OS61_2052.ndi.NTamd64.Services]
AddService = athr, 2, atheros.Service, atheros.EventLog
Include    = netvwifibus.inf
Needs      = VWiFiBus.Services

[ATHR_DEV_OS61_2052.ndi.NTamd64.HW]
Include = netvwifibus.inf
Needs   = VWiFiBus.PnPFilterRegistration

[ATHR_DEV_OS61_01001A32.ndi.NTamd64]
Characteristics = 0x84
BusType         = 5
AddReg          = atheros_os61.reg, atheros.reg, customer9Led.reg
DelReg          = atheros.DelReg
CopyFiles       = atheros.CopyFiles
*IfType         = 71        ; IF_TYPE_IEEE80211
*MediaType      = 16        ; NdisMediumNative802_11
*PhysicalMediaType = 9      ; NdisPhysicalMediumNative802_11
Include         = netvwifibus.inf, machine.inf
Needs           = VWiFiBus.CopyFiles

[ATHR_DEV_OS61_01001A32.ndi.NTamd64.Services]
AddService = athr, 2, atheros.Service, atheros.EventLog
Include    = netvwifibus.inf
Needs      = VWiFiBus.Services

[ATHR_DEV_OS61_01001A32.ndi.NTamd64.HW]
Include = netvwifibus.inf
Needs   = VWiFiBus.PnPFilterRegistration

[ATHR_DEV_OS61_1053.ndi.NTamd64]
Characteristics = 0x84
BusType         = 5
AddReg          = atheros_os61.reg, atheros.reg
DelReg          = atheros.DelReg
CopyFiles       = atheros.CopyFiles
*IfType         = 71        ; IF_TYPE_IEEE80211
*MediaType      = 16        ; NdisMediumNative802_11
*PhysicalMediaType = 9      ; NdisPhysicalMediumNative802_11
Include         = netvwifibus.inf, machine.inf
Needs           = VWiFiBus.CopyFiles

[ATHR_DEV_OS61_1053.ndi.NTamd64.Services]
AddService = athr, 2, atheros.Service, atheros.EventLog
Include    = netvwifibus.inf
Needs      = VWiFiBus.Services

[ATHR_DEV_OS61_1053.ndi.NTamd64.HW]
Include = netvwifibus.inf
Needs   = VWiFiBus.PnPFilterRegistration

[ATHR_DEV_OS61_2053.ndi.NTamd64]
Characteristics = 0x84
BusType         = 5
AddReg          = atheros_os61.reg, atheros.reg
DelReg          = atheros.DelReg
CopyFiles       = atheros.CopyFiles
*IfType         = 71        ; IF_TYPE_IEEE80211
*MediaType      = 16        ; NdisMediumNative802_11
*PhysicalMediaType = 9      ; NdisPhysicalMediumNative802_11
Include         = netvwifibus.inf, machine.inf
Needs           = VWiFiBus.CopyFiles

[ATHR_DEV_OS61_2053.ndi.NTamd64.Services]
AddService = athr, 2, atheros.Service, atheros.EventLog
Include    = netvwifibus.inf
Needs      = VWiFiBus.Services

[ATHR_DEV_OS61_2053.ndi.NTamd64.HW]
Include = netvwifibus.inf
Needs   = VWiFiBus.PnPFilterRegistration

[ATHR_DEV_OS61_1054.ndi.NTamd64]
Characteristics = 0x84
BusType         = 5
AddReg          = atheros_os61.reg, atheros.reg
DelReg          = atheros.DelReg
CopyFiles       = atheros.CopyFiles
*IfType         = 71        ; IF_TYPE_IEEE80211
*MediaType      = 16        ; NdisMediumNative802_11
*PhysicalMediaType = 9      ; NdisPhysicalMediumNative802_11
Include         = netvwifibus.inf, machine.inf
Needs           = VWiFiBus.CopyFiles

[ATHR_DEV_OS61_1054.ndi.NTamd64.Services]
AddService = athr, 2, atheros.Service, atheros.EventLog
Include    = netvwifibus.inf
Needs      = VWiFiBus.Services

[ATHR_DEV_OS61_1054.ndi.NTamd64.HW]
Include = netvwifibus.inf
Needs   = VWiFiBus.PnPFilterRegistration

[ATHR_DEV_OS61_2054.ndi.NTamd64]
Characteristics = 0x84
BusType         = 5
AddReg          = atheros_os61.reg, atheros.reg, cfpignore.reg
DelReg          = atheros.DelReg
CopyFiles       = atheros.CopyFiles
*IfType         = 71        ; IF_TYPE_IEEE80211
*MediaType      = 16        ; NdisMediumNative802_11
*PhysicalMediaType = 9      ; NdisPhysicalMediumNative802_11
Include         = netvwifibus.inf, machine.inf
Needs           = VWiFiBus.CopyFiles

[ATHR_DEV_OS61_2054.ndi.NTamd64.Services]
AddService = athr, 2, atheros.Service, atheros.EventLog
Include    = netvwifibus.inf
Needs      = VWiFiBus.Services

[ATHR_DEV_OS61_2054.ndi.NTamd64.HW]
Include = netvwifibus.inf
Needs   = VWiFiBus.PnPFilterRegistration

[ATHR_DEV_OS61_1062.ndi.NTamd64]
Characteristics = 0x84
BusType         = 5
AddReg          = atheros_os61.reg, atheros.reg
DelReg          = atheros.DelReg
CopyFiles       = atheros.CopyFiles
*IfType         = 71        ; IF_TYPE_IEEE80211
*MediaType      = 16        ; NdisMediumNative802_11
*PhysicalMediaType = 9      ; NdisPhysicalMediumNative802_11
Include         = netvwifibus.inf, machine.inf
Needs           = VWiFiBus.CopyFiles

[ATHR_DEV_OS61_1062.ndi.NTamd64.Services]
AddService = athr, 2, atheros.Service, atheros.EventLog
Include    = netvwifibus.inf
Needs      = VWiFiBus.Services

[ATHR_DEV_OS61_1062.ndi.NTamd64.HW]
Include = netvwifibus.inf
Needs   = VWiFiBus.PnPFilterRegistration

[ATHR_DEV_OS61_2062.ndi.NTamd64]
Characteristics = 0x84
BusType         = 5
AddReg          = atheros_os61.reg, atheros.reg
DelReg          = atheros.DelReg
CopyFiles       = atheros.CopyFiles
*IfType         = 71        ; IF_TYPE_IEEE80211
*MediaType      = 16        ; NdisMediumNative802_11
*PhysicalMediaType = 9      ; NdisPhysicalMediumNative802_11
Include         = netvwifibus.inf, machine.inf
Needs           = VWiFiBus.CopyFiles

[ATHR_DEV_OS61_2062.ndi.NTamd64.Services]
AddService = athr, 2, atheros.Service, atheros.EventLog
Include    = netvwifibus.inf
Needs      = VWiFiBus.Services

[ATHR_DEV_OS61_2062.ndi.NTamd64.HW]
Include = netvwifibus.inf
Needs   = VWiFiBus.PnPFilterRegistration

[ATHR_DEV_OS61_1063.ndi.NTamd64]
Characteristics = 0x84
BusType         = 5
AddReg          = atheros_os61.reg, atheros.reg
DelReg          = atheros.DelReg
CopyFiles       = atheros.CopyFiles
*IfType         = 71        ; IF_TYPE_IEEE80211
*MediaType      = 16        ; NdisMediumNative802_11
*PhysicalMediaType = 9      ; NdisPhysicalMediumNative802_11
Include         = netvwifibus.inf, machine.inf
Needs           = VWiFiBus.CopyFiles

[ATHR_DEV_OS61_1063.ndi.NTamd64.Services]
AddService = athr, 2, atheros.Service, atheros.EventLog
Include    = netvwifibus.inf
Needs      = VWiFiBus.Services

[ATHR_DEV_OS61_1063.ndi.NTamd64.HW]
Include = netvwifibus.inf
Needs   = VWiFiBus.PnPFilterRegistration

[ATHR_DEV_OS61_2063.ndi.NTamd64]
Characteristics = 0x84
BusType         = 5
AddReg          = atheros_os61.reg, atheros.reg, cfpignore.reg
DelReg          = atheros.DelReg
CopyFiles       = atheros.CopyFiles
*IfType         = 71        ; IF_TYPE_IEEE80211
*MediaType      = 16        ; NdisMediumNative802_11
*PhysicalMediaType = 9      ; NdisPhysicalMediumNative802_11
Include         = netvwifibus.inf, machine.inf
Needs           = VWiFiBus.CopyFiles

[ATHR_DEV_OS61_2063.ndi.NTamd64.Services]
AddService = athr, 2, atheros.Service, atheros.EventLog
Include    = netvwifibus.inf
Needs      = VWiFiBus.Services

[ATHR_DEV_OS61_2063.ndi.NTamd64.HW]
Include = netvwifibus.inf
Needs   = VWiFiBus.PnPFilterRegistration

[ATHR_DEV_OS61_1071.ndi.NTamd64]
Characteristics = 0x84
BusType         = 5
AddReg          = atheros_os61.reg, atheros11n.reg, htAdhoc.reg
DelReg          = atheros.DelReg
CopyFiles       = atheros.CopyFiles
*IfType         = 71            ; IF_TYPE_IEEE80211
*MediaType      = 16            ; NdisMediumNative802_11
*PhysicalMediaType = 9          ; NdisPhysicalMediumNative802_11
Include         = netvwifibus.inf, machine.inf
Needs           = VWiFiBus.CopyFiles

[ATHR_DEV_OS61_1071.ndi.NTamd64.Services]
AddService = athr, 2, atheros.Service, atheros.EventLog
Include    = netvwifibus.inf
Needs      = VWiFiBus.Services

[ATHR_DEV_OS61_1071.ndi.NTamd64.HW]
Include = netvwifibus.inf
Needs   = VWiFiBus.PnPFilterRegistration

[ATHR_DEV_OS61_90001385.ndi.NTamd64]
Characteristics = 0x84
BusType         = 5
AddReg          = atheros_os61.reg, atheros11n.reg, expresscardaspmoff.reg, htAdhoc.reg
DelReg          = atheros.DelReg
CopyFiles       = atheros.CopyFiles
*IfType         = 71            ; IF_TYPE_IEEE80211
*MediaType      = 16            ; NdisMediumNative802_11
*PhysicalMediaType = 9          ; NdisPhysicalMediumNative802_11
Include         = netvwifibus.inf, machine.inf
Needs           = VWiFiBus.CopyFiles

[ATHR_DEV_OS61_90001385.ndi.NTamd64.Services]
AddService = athr, 2, atheros.Service, atheros.EventLog
Include    = netvwifibus.inf
Needs      = VWiFiBus.Services

[ATHR_DEV_OS61_90001385.ndi.NTamd64.HW]
Include = netvwifibus.inf
Needs   = VWiFiBus.PnPFilterRegistration

[ATHR_DEV_OS61_2A5F103C.ndi.NTamd64]
Characteristics = 0x84
BusType         = 5
AddReg          = atheros_os61.reg, atheros11n.reg, customer2.11n.reg, htAdhoc.reg
DelReg          = atheros.DelReg
CopyFiles       = atheros.CopyFiles
*IfType         = 71            ; IF_TYPE_IEEE80211
*MediaType      = 16            ; NdisMediumNative802_11
*PhysicalMediaType = 9          ; NdisPhysicalMediumNative802_11
Include         = netvwifibus.inf, machine.inf
Needs           = VWiFiBus.CopyFiles

[ATHR_DEV_OS61_2A5F103C.ndi.NTamd64.Services]
AddService = athr, 2, atheros.Service, atheros.EventLog
Include    = netvwifibus.inf
Needs      = VWiFiBus.Services

[ATHR_DEV_OS61_2A5F103C.ndi.NTamd64.HW]
Include = netvwifibus.inf
Needs   = VWiFiBus.PnPFilterRegistration

[ATHR_DEV_OS61_11AD.ndi.NTamd64]
Characteristics = 0x84
BusType         = 5
AddReg          = atheros_os61.reg, atheros.reg, customer2.reg
DelReg          = atheros.DelReg
CopyFiles       = atheros.CopyFiles
*IfType         = 71        ; IF_TYPE_IEEE80211
*MediaType      = 16        ; NdisMediumNative802_11
*PhysicalMediaType = 9      ; NdisPhysicalMediumNative802_11
Include         = netvwifibus.inf, machine.inf
Needs           = VWiFiBus.CopyFiles

[ATHR_DEV_OS61_11AD.ndi.NTamd64.Services]
AddService = athr, 2, atheros.Service, atheros.EventLog
Include    = netvwifibus.inf
Needs      = VWiFiBus.Services

[ATHR_DEV_OS61_11AD.ndi.NTamd64.HW]
Include = netvwifibus.inf
Needs   = VWiFiBus.PnPFilterRegistration

[ATHR_DEV_OS61_3072.ndi.NTamd64]
Characteristics = 0x84
BusType         = 5
AddReg          = atheros_os61.reg, atheros11n.reg, htAdhoc.reg
DelReg          = atheros.DelReg
CopyFiles       = atheros.CopyFiles
*IfType         = 71            ; IF_TYPE_IEEE80211
*MediaType      = 16            ; NdisMediumNative802_11
*PhysicalMediaType = 9          ; NdisPhysicalMediumNative802_11
Include         = netvwifibus.inf, machine.inf
Needs           = VWiFiBus.CopyFiles

[ATHR_DEV_OS61_3072.ndi.NTamd64.Services]
AddService = athr, 2, atheros.Service, atheros.EventLog
Include    = netvwifibus.inf
Needs      = VWiFiBus.Services

[ATHR_DEV_OS61_3072.ndi.NTamd64.HW]
Include = netvwifibus.inf
Needs   = VWiFiBus.PnPFilterRegistration

[ATHR_DEV_OS61_10671A3B.ndi.NTamd64]
Characteristics = 0x84
BusType         = 5
AddReg          = atheros_os61.reg, atheros11n.reg, cemspecled_func1_1.reg, smpsDynamic.reg, htWepTkipOpt.reg, htAdhoc.reg, indicaterxlinkspeed.reg
DelReg          = atheros.DelReg
CopyFiles       = atheros.CopyFiles
*IfType         = 71            ; IF_TYPE_IEEE80211
*MediaType      = 16            ; NdisMediumNative802_11
*PhysicalMediaType = 9          ; NdisPhysicalMediumNative802_11
Include         = netvwifibus.inf, machine.inf
Needs           = VWiFiBus.CopyFiles

[ATHR_DEV_OS61_10671A3B.ndi.NTamd64.Services]
AddService = athr, 2, atheros.Service, atheros.EventLog
Include    = netvwifibus.inf
Needs      = VWiFiBus.Services

[ATHR_DEV_OS61_10671A3B.ndi.NTamd64.HW]
Include = netvwifibus.inf
Needs   = VWiFiBus.PnPFilterRegistration

[ATHR_DEV_OS61_1A671A3B.ndi.NTamd64]
Characteristics = 0x84
BusType         = 5
AddReg          = atheros_os61.reg, atheros11n.reg, cemspecled_func1_1.reg
DelReg          = atheros.DelReg
CopyFiles       = atheros.CopyFiles
*IfType         = 71            ; IF_TYPE_IEEE80211
*MediaType      = 16            ; NdisMediumNative802_11
*PhysicalMediaType = 9          ; NdisPhysicalMediumNative802_11
Include         = netvwifibus.inf, machine.inf
Needs           = VWiFiBus.CopyFiles

[ATHR_DEV_OS61_1A671A3B.ndi.NTamd64.Services]
AddService = athr, 2, atheros.Service, atheros.EventLog
Include    = netvwifibus.inf
Needs      = VWiFiBus.Services

[ATHR_DEV_OS61_1A671A3B.ndi.NTamd64.HW]
Include = netvwifibus.inf
Needs   = VWiFiBus.PnPFilterRegistration

[ATHR_DEV_OS61_10711A3B.ndi.NTamd64]
Characteristics = 0x84
BusType         = 5
AddReg          = atheros_os61.reg, atheros11n.reg, cemspecled_func1_1.reg, smpsDynamic.reg, htEnableWepTkip.reg, htAdhoc.reg
DelReg          = atheros.DelReg
CopyFiles       = atheros.CopyFiles
*IfType         = 71            ; IF_TYPE_IEEE80211
*MediaType      = 16            ; NdisMediumNative802_11
*PhysicalMediaType = 9          ; NdisPhysicalMediumNative802_11
Include         = netvwifibus.inf, machine.inf
Needs           = VWiFiBus.CopyFiles

[ATHR_DEV_OS61_10711A3B.ndi.NTamd64.Services]
AddService = athr, 2, atheros.Service, atheros.EventLog
Include    = netvwifibus.inf
Needs      = VWiFiBus.Services

[ATHR_DEV_OS61_10711A3B.ndi.NTamd64.HW]
Include = netvwifibus.inf
Needs   = VWiFiBus.PnPFilterRegistration

[ATHR_DEV_OS61_1C711A3B.ndi.NTamd64]
Characteristics = 0x84
BusType         = 5
AddReg          = atheros_os61.reg, atheros11n.reg, cemspecled_func1_1.reg, smpsDynamic.reg, 5416.bandselect.reg, htEnableWepTkip.reg, htAdhoc.reg, d3forcel1disable.reg
DelReg          = atheros.DelReg
CopyFiles       = atheros.CopyFiles
*IfType         = 71            ; IF_TYPE_IEEE80211
*MediaType      = 16            ; NdisMediumNative802_11
*PhysicalMediaType = 9          ; NdisPhysicalMediumNative802_11
Include         = netvwifibus.inf, machine.inf
Needs           = VWiFiBus.CopyFiles

[ATHR_DEV_OS61_1C711A3B.ndi.NTamd64.Services]
AddService = athr, 2, atheros.Service, atheros.EventLog
Include    = netvwifibus.inf
Needs      = VWiFiBus.Services

[ATHR_DEV_OS61_1C711A3B.ndi.NTamd64.HW]
Include = netvwifibus.inf
Needs   = VWiFiBus.PnPFilterRegistration

[ATHR_DEV_OS61_03011A32.ndi.NTamd64]
Characteristics = 0x84
BusType         = 5
AddReg          = atheros_os61.reg, atheros11n.reg, cemspecled_func1_1.reg, smpsDynamic.reg, htAdhoc.reg
DelReg          = atheros.DelReg
CopyFiles       = atheros.CopyFiles
*IfType         = 71            ; IF_TYPE_IEEE80211
*MediaType      = 16            ; NdisMediumNative802_11
*PhysicalMediaType = 9          ; NdisPhysicalMediumNative802_11
Include         = netvwifibus.inf, machine.inf
Needs           = VWiFiBus.CopyFiles

[ATHR_DEV_OS61_03011A32.ndi.NTamd64.Services]
AddService = athr, 2, atheros.Service, atheros.EventLog
Include    = netvwifibus.inf
Needs      = VWiFiBus.Services

[ATHR_DEV_OS61_03011A32.ndi.NTamd64.HW]
Include = netvwifibus.inf
Needs   = VWiFiBus.PnPFilterRegistration

[ATHR_DEV_OS61_3091.ndi.NTamd64]
Characteristics = 0x84
BusType         = 5
AddReg          = atheros_os61.reg, atheros11n.reg, smpsDynamic.reg, htAdhoc.reg
DelReg          = atheros.DelReg
CopyFiles       = atheros.CopyFiles
*IfType         = 71            ; IF_TYPE_IEEE80211
*MediaType      = 16            ; NdisMediumNative802_11
*PhysicalMediaType = 9          ; NdisPhysicalMediumNative802_11
Include         = netvwifibus.inf, machine.inf
Needs           = VWiFiBus.CopyFiles

[ATHR_DEV_OS61_3091.ndi.NTamd64.Services]
AddService = athr, 2, atheros.Service, atheros.EventLog
Include    = netvwifibus.inf
Needs      = VWiFiBus.Services

[ATHR_DEV_OS61_3091.ndi.NTamd64.HW]
Include = netvwifibus.inf
Needs   = VWiFiBus.PnPFilterRegistration

[ATHR_DEV_OS61_20001071.ndi.NTamd64]
Characteristics = 0x84
BusType         = 5
AddReg          = atheros_os61.reg, atheros11n.reg, smpsDynamic.reg, htAdhoc.reg, roamPolicy2.reg, wirelessmodeselectCompex.reg, TxPowerSelect.reg, wowenable.reg
DelReg          = atheros.DelReg
CopyFiles       = atheros.CopyFiles
*IfType         = 71            ; IF_TYPE_IEEE80211
*MediaType      = 16            ; NdisMediumNative802_11
*PhysicalMediaType = 9          ; NdisPhysicalMediumNative802_11
Include         = netvwifibus.inf, machine.inf
Needs           = VWiFiBus.CopyFiles

[ATHR_DEV_OS61_20001071.ndi.NTamd64.Services]
AddService = athr, 2, atheros.Service, atheros.EventLog
Include    = netvwifibus.inf
Needs      = VWiFiBus.Services

[ATHR_DEV_OS61_20001071.ndi.NTamd64.HW]
Include = netvwifibus.inf
Needs   = VWiFiBus.PnPFilterRegistration

[ATHR_DEV_OS61_309D168C.ndi.NTamd64]
Characteristics = 0x84
BusType         = 5
AddReg          = atheros_os61.reg, atheros11n.reg, smpsDynamic.reg, htAdhoc.reg, customer1roamPolicy.reg, wirelessmodeselectkite.reg
DelReg          = atheros.DelReg
CopyFiles       = atheros.CopyFiles
*IfType         = 71            ; IF_TYPE_IEEE80211
*MediaType      = 16            ; NdisMediumNative802_11
*PhysicalMediaType = 9          ; NdisPhysicalMediumNative802_11
Include         = netvwifibus.inf, machine.inf
Needs           = VWiFiBus.CopyFiles

[ATHR_DEV_OS61_309D168C.ndi.NTamd64.Services]
AddService = athr, 2, atheros.Service, atheros.EventLog
Include    = netvwifibus.inf
Needs      = VWiFiBus.Services

[ATHR_DEV_OS61_309D168C.ndi.NTamd64.HW]
Include = netvwifibus.inf
Needs   = VWiFiBus.PnPFilterRegistration

[ATHR_DEV_OS61_3091amd.ndi.NTamd64]
Characteristics = 0x84
BusType         = 5
AddReg          = atheros_os61.reg, atheros11n.reg, smpsDynamic.reg, htAdhoc.reg, cemspecled_func1_1.reg
DelReg          = atheros.DelReg
CopyFiles       = atheros.CopyFiles
*IfType         = 71            ; IF_TYPE_IEEE80211
*MediaType      = 16            ; NdisMediumNative802_11
*PhysicalMediaType = 9          ; NdisPhysicalMediumNative802_11
Include         = netvwifibus.inf, machine.inf
Needs           = VWiFiBus.CopyFiles

[ATHR_DEV_OS61_3091amd.ndi.NTamd64.Services]
AddService = athr, 2, atheros.Service, atheros.EventLog
Include    = netvwifibus.inf
Needs      = VWiFiBus.Services

[ATHR_DEV_OS61_3091amd.ndi.NTamd64.HW]
Include = netvwifibus.inf
Needs   = VWiFiBus.PnPFilterRegistration

[ATHR_DEV_OS61_008F106B.ndi.NTamd64]
Characteristics = 0x84
BusType         = 5
AddReg          = atheros_os61.reg, atheros11n.reg, smpsDynamic.reg, htAdhoc.reg, wowenable.reg, merlinshiftdelay.reg
DelReg          = atheros.DelReg
CopyFiles       = atheros.CopyFiles
*IfType         = 71            ; IF_TYPE_IEEE80211
*MediaType      = 16            ; NdisMediumNative802_11
*PhysicalMediaType = 9          ; NdisPhysicalMediumNative802_11
Include         = netvwifibus.inf, machine.inf
Needs           = VWiFiBus.CopyFiles

[ATHR_DEV_OS61_008F106B.ndi.NTamd64.Services]
AddService = athr, 2, atheros.Service, atheros.EventLog
Include    = netvwifibus.inf
Needs      = VWiFiBus.Services

[ATHR_DEV_OS61_008F106B.ndi.NTamd64.HW]
Include = netvwifibus.inf
Needs   = VWiFiBus.PnPFilterRegistration

[ATHR_DEV_OS61_309D17AA.ndi.NTamd64]
Characteristics = 0x84
BusType         = 5
AddReg          = atheros_os61.reg, atheros11n.reg, smpsDynamic.reg, htAdhoc.reg, Customer15a.led.reg
DelReg          = atheros.DelReg
CopyFiles       = atheros.CopyFiles
*IfType         = 71            ; IF_TYPE_IEEE80211
*MediaType      = 16            ; NdisMediumNative802_11
*PhysicalMediaType = 9          ; NdisPhysicalMediumNative802_11
Include         = netvwifibus.inf, machine.inf
Needs           = VWiFiBus.CopyFiles

[ATHR_DEV_OS61_309D17AA.ndi.NTamd64.Services]
AddService = athr, 2, atheros.Service, atheros.EventLog
Include    = netvwifibus.inf
Needs      = VWiFiBus.Services

[ATHR_DEV_OS61_309D17AA.ndi.NTamd64.HW]
Include = netvwifibus.inf
Needs   = VWiFiBus.PnPFilterRegistration

[ATHR_DEV_OS61_30A117AA.ndi.NTamd64]
Characteristics = 0x84
BusType         = 5
AddReg          = atheros_os61.reg, atheros11n.reg, smpsDynamic.reg, htAdhoc.reg, Customer15a.led.reg, triggerlevelkiteonly.reg, c3war.reg, sharegpio.reg
DelReg          = atheros.DelReg
CopyFiles       = atheros.CopyFiles
*IfType         = 71            ; IF_TYPE_IEEE80211
*MediaType      = 16            ; NdisMediumNative802_11
*PhysicalMediaType = 9          ; NdisPhysicalMediumNative802_11
Include         = netvwifibus.inf, machine.inf
Needs           = VWiFiBus.CopyFiles

[ATHR_DEV_OS61_30A117AA.ndi.NTamd64.Services]
AddService = athr, 2, atheros.Service, atheros.EventLog
Include    = netvwifibus.inf
Needs      = VWiFiBus.Services

[ATHR_DEV_OS61_30A117AA.ndi.NTamd64.HW]
Include = netvwifibus.inf
Needs   = VWiFiBus.PnPFilterRegistration

[ATHR_DEV_OS61_30A117AAw.ndi.NTamd64]
Characteristics = 0x84
BusType         = 5
AddReg          = atheros_os61.reg, atheros11n.reg, smpsDynamic.reg, htAdhoc.reg, Customer15a.led.reg, triggerlevelkiteonly.reg, c3war.reg, sharegpio.reg, janusda.reg
DelReg          = atheros.DelReg
CopyFiles       = atheros.CopyFiles
*IfType         = 71            ; IF_TYPE_IEEE80211
*MediaType      = 16            ; NdisMediumNative802_11
*PhysicalMediaType = 9          ; NdisPhysicalMediumNative802_11
Include         = netvwifibus.inf, machine.inf
Needs           = VWiFiBus.CopyFiles

[ATHR_DEV_OS61_30A117AAw.ndi.NTamd64.Services]
AddService = athr, 2, atheros.Service, atheros.EventLog
Include    = netvwifibus.inf
Needs      = VWiFiBus.Services

[ATHR_DEV_OS61_30A117AAw.ndi.NTamd64.HW]
Include = netvwifibus.inf
Needs   = VWiFiBus.PnPFilterRegistration

[ATHR_DEV_OS61_311817AA.ndi.NTamd64]
Characteristics = 0x84
BusType         = 5
AddReg          = atheros_os61.reg, atheros11n.reg, htAdhoc.reg, paprdenable.reg, customer2GreenTx.reg, cemspecled_func2_6.reg, wowenable.reg, power_management.reg
DelReg          = atheros.DelReg
CopyFiles       = atheros.CopyFiles
*IfType         = 71        ; IF_TYPE_IEEE80211
*MediaType      = 16        ; NdisMediumNative802_11
*PhysicalMediaType = 9      ; NdisPhysicalMediumNative802_11
Include         = netvwifibus.inf, machine.inf
Needs           = VWiFiBus.CopyFiles

[ATHR_DEV_OS61_311817AA.ndi.NTamd64.Services]
AddService = athr, 2, atheros.Service, atheros.EventLog
Include    = netvwifibus.inf
Needs      = VWiFiBus.Services

[ATHR_DEV_OS61_311817AA.ndi.NTamd64.HW]
Include = netvwifibus.inf
Needs   = PciASPMOptIn, VWiFiBus.PnPFilterRegistration

[ATHR_DEV_OS61_321817AA.ndi.NTamd64]
Characteristics = 0x84
BusType         = 5
AddReg          = atheros_os61.reg, atheros11n.reg, htAdhoc.reg, 9485BTcoex.reg, customer2GreenTx.reg, paprdenable.reg, 9485LnaDivUseBtAntEnable.reg, cemspecled_func2_6.reg, wowenable.reg
DelReg          = atheros.DelReg
CopyFiles       = atheros.CopyFiles
*IfType         = 71        ; IF_TYPE_IEEE80211
*MediaType      = 16        ; NdisMediumNative802_11
*PhysicalMediaType = 9      ; NdisPhysicalMediumNative802_11
Include         = netvwifibus.inf, machine.inf
Needs           = VWiFiBus.CopyFiles

[ATHR_DEV_OS61_321817AA.ndi.NTamd64.Services]
AddService = athr, 2, atheros.Service, atheros.EventLog
Include    = netvwifibus.inf
Needs      = VWiFiBus.Services

[ATHR_DEV_OS61_321817AA.ndi.NTamd64.HW]
Include = netvwifibus.inf
Needs   = PciASPMOptIn, VWiFiBus.PnPFilterRegistration

[ATHR_DEV_OS61_321917AA.ndi.NTamd64]
Characteristics = 0x84
BusType         = 5
AddReg          = atheros_os61.reg, atheros11n.reg, htAdhoc.reg, 9485BTcoex.reg, customer2GreenTx.reg, paprdenable.reg, 9485LnaDivUseBtAntEnable.reg, cemspecled_func2_6.reg
DelReg          = atheros.DelReg
CopyFiles       = atheros.CopyFiles
*IfType         = 71        ; IF_TYPE_IEEE80211
*MediaType      = 16        ; NdisMediumNative802_11
*PhysicalMediaType = 9      ; NdisPhysicalMediumNative802_11
Include         = netvwifibus.inf, machine.inf
Needs           = VWiFiBus.CopyFiles

[ATHR_DEV_OS61_321917AA.ndi.NTamd64.Services]
AddService = athr, 2, atheros.Service, atheros.EventLog
Include    = netvwifibus.inf
Needs      = VWiFiBus.Services

[ATHR_DEV_OS61_321917AA.ndi.NTamd64.HW]
AddReg  = MSI.reg
Include = netvwifibus.inf
Needs   = PciASPMOptIn, VWiFiBus.PnPFilterRegistration

[ATHR_DEV_OS61_311417AA.ndi.NTamd64]
Characteristics = 0x84
BusType         = 5
AddReg          = atheros_os61.reg, atheros11n.reg, smpsDynamic.reg, htAdhoc.reg, jupiter2ant.reg, customer2GreenTx.reg, customer3h.reg
DelReg          = atheros.DelReg
CopyFiles       = atheros.CopyFiles
*IfType         = 71        ; IF_TYPE_IEEE80211
*MediaType      = 16        ; NdisMediumNative802_11
*PhysicalMediaType = 9      ; NdisPhysicalMediumNative802_11
Include         = netvwifibus.inf, machine.inf
Needs           = VWiFiBus.CopyFiles

[ATHR_DEV_OS61_311417AA.ndi.NTamd64.Services]
AddService = athr, 2, atheros.Service, atheros.EventLog
Include    = netvwifibus.inf
Needs      = VWiFiBus.Services

[ATHR_DEV_OS61_311417AA.ndi.NTamd64.HW]
Include = netvwifibus.inf
Needs   = PciASPMOptIn, VWiFiBus.PnPFilterRegistration

[ATHR_DEV_OS61_321417AA.ndi.NTamd64]
Characteristics = 0x84
BusType         = 5
AddReg          = atheros_os61.reg, atheros11n.reg, smpsDynamic.reg, htAdhoc.reg, jupiter2ant.reg, customer2GreenTx.reg, customer3h.reg, wowenable.reg
DelReg          = atheros.DelReg
CopyFiles       = atheros.CopyFiles
*IfType         = 71        ; IF_TYPE_IEEE80211
*MediaType      = 16        ; NdisMediumNative802_11
*PhysicalMediaType = 9      ; NdisPhysicalMediumNative802_11
Include         = netvwifibus.inf, machine.inf
Needs           = VWiFiBus.CopyFiles

[ATHR_DEV_OS61_321417AA.ndi.NTamd64.Services]
AddService = athr, 2, atheros.Service, atheros.EventLog
Include    = netvwifibus.inf
Needs      = VWiFiBus.Services

[ATHR_DEV_OS61_321417AA.ndi.NTamd64.HW]
Include = netvwifibus.inf
Needs   = PciASPMOptIn, VWiFiBus.PnPFilterRegistration

[ATHR_DEV_OS61_00911969.ndi.NTamd64]
Characteristics = 0x84
BusType         = 5
AddReg          = atheros_os61.reg, atheros11n.reg, smpsDynamic.reg, htAdhoc.reg, jupiter2ant.reg, customer2GreenTx.reg, customer3h.reg, wowenable.reg
DelReg          = atheros.DelReg
CopyFiles       = atheros.CopyFiles
*IfType         = 71        ; IF_TYPE_IEEE80211
*MediaType      = 16        ; NdisMediumNative802_11
*PhysicalMediaType = 9      ; NdisPhysicalMediumNative802_11
Include         = netvwifibus.inf, machine.inf
Needs           = VWiFiBus.CopyFiles

[ATHR_DEV_OS61_00911969.ndi.NTamd64.Services]
AddService = athr, 2, atheros.Service, atheros.EventLog
Include    = netvwifibus.inf
Needs      = VWiFiBus.Services

[ATHR_DEV_OS61_00911969.ndi.NTamd64.HW]
Include = netvwifibus.inf
Needs   = PciASPMOptIn, VWiFiBus.PnPFilterRegistration

;Liteon
[ATHR_DEV_OS61_321417AAA.ndi.NTamd64]
Characteristics = 0x84
BusType         = 5
AddReg          = atheros_os61.reg, atheros11n.reg, smpsDynamic.reg, htAdhoc.reg, jupiter2ant.reg, customer2GreenTx.reg, customer3h.reg, wowenable.reg, bandselect.reg
DelReg          = atheros.DelReg
CopyFiles       = atheros.CopyFiles
*IfType         = 71        ; IF_TYPE_IEEE80211
*MediaType      = 16        ; NdisMediumNative802_11
*PhysicalMediaType = 9      ; NdisPhysicalMediumNative802_11
Include         = netvwifibus.inf, machine.inf
Needs           = VWiFiBus.CopyFiles

[ATHR_DEV_OS61_321417AAA.ndi.NTamd64.Services]
AddService = athr, 2, atheros.Service, atheros.EventLog
Include    = netvwifibus.inf
Needs      = VWiFiBus.Services

[ATHR_DEV_OS61_321417AAA.ndi.NTamd64.HW]
Include = netvwifibus.inf
Needs   = PciASPMOptIn, VWiFiBus.PnPFilterRegistration

[ATHR_DEV_OS61_30A417AA.ndi.NTamd64]
Characteristics = 0x84
BusType         = 5
AddReg          = atheros_os61.reg, atheros11n.reg, smpsDynamic.reg, htAdhoc.reg, cemspecled_func2_8.reg, c3war.reg, sharegpio.reg
DelReg          = atheros.DelReg
CopyFiles       = atheros.CopyFiles
*IfType         = 71            ; IF_TYPE_IEEE80211
*MediaType      = 16            ; NdisMediumNative802_11
*PhysicalMediaType = 9          ; NdisPhysicalMediumNative802_11
Include         = netvwifibus.inf, machine.inf
Needs           = VWiFiBus.CopyFiles

[ATHR_DEV_OS61_30A417AA.ndi.NTamd64.Services]
AddService = athr, 2, atheros.Service, atheros.EventLog
Include    = netvwifibus.inf
Needs      = VWiFiBus.Services

[ATHR_DEV_OS61_30A417AA.ndi.NTamd64.HW]
Include = netvwifibus.inf
Needs   = VWiFiBus.PnPFilterRegistration

[ATHR_DEV_OS61_30A417AAw.ndi.NTamd64]
Characteristics = 0x84
BusType         = 5
AddReg          = atheros_os61.reg, atheros11n.reg, smpsDynamic.reg, htAdhoc.reg, cemspecled_func2_8.reg, c3war.reg, sharegpio.reg, WB197da.reg
DelReg          = atheros.DelReg
CopyFiles       = atheros.CopyFiles
*IfType         = 71            ; IF_TYPE_IEEE80211
*MediaType      = 16            ; NdisMediumNative802_11
*PhysicalMediaType = 9          ; NdisPhysicalMediumNative802_11
Include         = netvwifibus.inf, machine.inf
Needs           = VWiFiBus.CopyFiles

[ATHR_DEV_OS61_30A417AAw.ndi.NTamd64.Services]
AddService = athr, 2, atheros.Service, atheros.EventLog
Include    = netvwifibus.inf
Needs      = VWiFiBus.Services

[ATHR_DEV_OS61_30A417AAw.ndi.NTamd64.HW]
Include = netvwifibus.inf
Needs   = VWiFiBus.PnPFilterRegistration

[ATHR_DEV_OS61_316417AA.ndi.NTamd64]
Characteristics = 0x84
BusType         = 5
AddReg          = atheros_os61.reg, atheros.reg, Customer15b.led.reg
DelReg          = atheros.DelReg
CopyFiles       = atheros.CopyFiles
*IfType         = 71        ; IF_TYPE_IEEE80211
*MediaType      = 16        ; NdisMediumNative802_11
*PhysicalMediaType = 9      ; NdisPhysicalMediumNative802_11
Include         = netvwifibus.inf, machine.inf
Needs           = VWiFiBus.CopyFiles

[ATHR_DEV_OS61_316417AA.ndi.NTamd64.Services]
AddService = athr, 2, atheros.Service, atheros.EventLog
Include    = netvwifibus.inf
Needs      = VWiFiBus.Services

[ATHR_DEV_OS61_316417AA.ndi.NTamd64.HW]
Include = netvwifibus.inf
Needs   = VWiFiBus.PnPFilterRegistration

[ATHR_DEV_OS61_7136144F.ndi.NTamd64]
Characteristics = 0x84
BusType         = 5
AddReg          = atheros_os61.reg, atheros11n.reg, smpsDynamic.reg, htAdhoc.reg, merlinshiftdelay.reg, cfpignore.reg
DelReg          = atheros.DelReg
CopyFiles       = atheros.CopyFiles
*IfType         = 71            ; IF_TYPE_IEEE80211
*MediaType      = 16            ; NdisMediumNative802_11
*PhysicalMediaType = 9          ; NdisPhysicalMediumNative802_11
Include         = netvwifibus.inf, machine.inf
Needs           = VWiFiBus.CopyFiles

[ATHR_DEV_OS61_7136144F.ndi.NTamd64.Services]
AddService = athr, 2, atheros.Service, atheros.EventLog
Include    = netvwifibus.inf
Needs      = VWiFiBus.Services

[ATHR_DEV_OS61_7136144F.ndi.NTamd64.HW]
Include = netvwifibus.inf
Needs   = VWiFiBus.PnPFilterRegistration

[ATHR_DEV_OS61_7163144F.ndi.NTamd64]
Characteristics = 0x84
BusType         = 5
AddReg          = atheros_os61.reg, atheros11n.reg, smpsDynamic.reg, htAdhoc.reg, merlinshiftdelay.reg, fullhwresethb93.reg, cfpignore.reg
DelReg          = atheros.DelReg
CopyFiles       = atheros.CopyFiles
*IfType         = 71            ; IF_TYPE_IEEE80211
*MediaType      = 16            ; NdisMediumNative802_11
*PhysicalMediaType = 9          ; NdisPhysicalMediumNative802_11
Include         = netvwifibus.inf, machine.inf
Needs           = VWiFiBus.CopyFiles

[ATHR_DEV_OS61_7163144F.ndi.NTamd64.Services]
AddService = athr, 2, atheros.Service, atheros.EventLog
Include    = netvwifibus.inf
Needs      = VWiFiBus.Services

[ATHR_DEV_OS61_7163144F.ndi.NTamd64.HW]
Include = netvwifibus.inf
Needs   = VWiFiBus.PnPFilterRegistration

[ATHR_DEV_OS61_D05B10FC.ndi.NTamd64]
Characteristics = 0x84
BusType         = 5
AddReg          = atheros_os61.reg, atheros11n.reg, smpsDynamic.reg, htAdhoc.reg, customer_IODATA.reg
DelReg          = atheros.DelReg
CopyFiles       = atheros.CopyFiles
*IfType         = 71            ; IF_TYPE_IEEE80211
*MediaType      = 16            ; NdisMediumNative802_11
*PhysicalMediaType = 9          ; NdisPhysicalMediumNative802_11
Include         = netvwifibus.inf, machine.inf
Needs           = VWiFiBus.CopyFiles

[ATHR_DEV_OS61_D05B10FC.ndi.NTamd64.Services]
AddService = athr, 2, atheros.Service, atheros.EventLog
Include    = netvwifibus.inf
Needs      = VWiFiBus.Services

[ATHR_DEV_OS61_D05B10FC.ndi.NTamd64.HW]
Include = netvwifibus.inf
Needs   = VWiFiBus.PnPFilterRegistration

[ATHR_DEV_OS61_T3091.ndi.NTamd64]
Characteristics = 0x84
BusType         = 5
AddReg          = atheros_os61.reg, atheros11n.reg, smpsDynamic.reg, pcibusconfig.reg, htAdhoc.reg
DelReg          = atheros.DelReg
CopyFiles       = atheros.CopyFiles
*IfType         = 71            ; IF_TYPE_IEEE80211
*MediaType      = 16            ; NdisMediumNative802_11
*PhysicalMediaType = 9          ; NdisPhysicalMediumNative802_11
Include         = netvwifibus.inf, machine.inf
Needs           = VWiFiBus.CopyFiles

[ATHR_DEV_OS61_T3091.ndi.NTamd64.Services]
AddService = athr, 2, atheros.Service, atheros.EventLog
Include    = netvwifibus.inf
Needs      = VWiFiBus.Services

[ATHR_DEV_OS61_T3091.ndi.NTamd64.HW]
Include = netvwifibus.inf
Needs   = VWiFiBus.PnPFilterRegistration

[ATHR_DEV_OS61_309917AA.ndi.NTamd64]
Characteristics = 0x84
BusType         = 5
AddReg          = atheros_os61.reg, atheros11n.reg, cemspecled_func1_1.reg, smpsDynamic.reg, htAdhoc.reg
DelReg          = atheros.DelReg
CopyFiles       = atheros.CopyFiles
*IfType         = 71            ; IF_TYPE_IEEE80211
*MediaType      = 16            ; NdisMediumNative802_11
*PhysicalMediaType = 9          ; NdisPhysicalMediumNative802_11
Include         = netvwifibus.inf, machine.inf
Needs           = VWiFiBus.CopyFiles

[ATHR_DEV_OS61_309917AA.ndi.NTamd64.Services]
AddService = athr, 2, atheros.Service, atheros.EventLog
Include    = netvwifibus.inf
Needs      = VWiFiBus.Services

[ATHR_DEV_OS61_309917AA.ndi.NTamd64.HW]
Include = netvwifibus.inf
Needs   = VWiFiBus.PnPFilterRegistration

[ATHR_DEV_OS61_30A1.ndi.NTamd64]
Characteristics = 0x84
BusType         = 5
AddReg          = atheros_os61.reg, atheros11n.reg, htAdhoc.reg, triggerlevelkiteonly.reg, c3war.reg
DelReg          = atheros.DelReg
CopyFiles       = atheros.CopyFiles
*IfType         = 71            ; IF_TYPE_IEEE80211
*MediaType      = 16            ; NdisMediumNative802_11
*PhysicalMediaType = 9          ; NdisPhysicalMediumNative802_11
Include         = netvwifibus.inf, machine.inf
Needs           = VWiFiBus.CopyFiles

[ATHR_DEV_OS61_30A1.ndi.NTamd64.Services]
AddService = athr, 2, atheros.Service, atheros.EventLog
Include    = netvwifibus.inf
Needs      = VWiFiBus.Services

[ATHR_DEV_OS61_30A1.ndi.NTamd64.HW]
Include = netvwifibus.inf
Needs   = VWiFiBus.PnPFilterRegistration

[ATHR_DEV_OS61_30A1op.ndi.NTamd64]
Characteristics = 0x84
BusType         = 5
AddReg          = atheros_os61.reg, atheros11n.reg, htAdhoc.reg, triggerlevelkiteonly.reg, c3war.reg, customerop.reg, regdmn.reg, cmdRegister.reg, rxLatencyWar.reg, ignore11denable.reg
DelReg          = atheros.DelReg
CopyFiles       = atheros.CopyFiles
*IfType         = 71            ; IF_TYPE_IEEE80211
*MediaType      = 16            ; NdisMediumNative802_11
*PhysicalMediaType = 9          ; NdisPhysicalMediumNative802_11
Include         = netvwifibus.inf, machine.inf
Needs           = VWiFiBus.CopyFiles

[ATHR_DEV_OS61_30A1op.ndi.NTamd64.Services]
AddService = athr, 2, atheros.Service, atheros.EventLog
Include    = netvwifibus.inf
Needs      = VWiFiBus.Services

[ATHR_DEV_OS61_30A1op.ndi.NTamd64.HW]
Include = netvwifibus.inf
Needs   = VWiFiBus.PnPFilterRegistration

[ATHR_DEV_OS61_30A4.ndi.NTamd64]
Characteristics = 0x84
BusType         = 5
AddReg          = atheros_os61.reg, atheros11n.reg, htAdhoc.reg
DelReg          = atheros.DelReg
CopyFiles       = atheros.CopyFiles
*IfType         = 71            ; IF_TYPE_IEEE80211
*MediaType      = 16            ; NdisMediumNative802_11
*PhysicalMediaType = 9          ; NdisPhysicalMediumNative802_11
Include         = netvwifibus.inf, machine.inf
Needs           = VWiFiBus.CopyFiles

[ATHR_DEV_OS61_30A4.ndi.NTamd64.Services]
AddService = athr, 2, atheros.Service, atheros.EventLog
Include    = netvwifibus.inf
Needs      = VWiFiBus.Services

[ATHR_DEV_OS61_30A4.ndi.NTamd64.HW]
Include = netvwifibus.inf
Needs   = VWiFiBus.PnPFilterRegistration

[ATHR_DEV_OS61_30A4TP.ndi.NTamd64]
Characteristics = 0x84
BusType         = 5
AddReg          = atheros_os61.reg, atheros11n.reg, htAdhoc.reg, tpshiftdelay.reg
DelReg          = atheros.DelReg
CopyFiles       = atheros.CopyFiles
*IfType         = 71            ; IF_TYPE_IEEE80211
*MediaType      = 16            ; NdisMediumNative802_11
*PhysicalMediaType = 9          ; NdisPhysicalMediumNative802_11
Include         = netvwifibus.inf, machine.inf
Needs           = VWiFiBus.CopyFiles

[ATHR_DEV_OS61_30A4TP.ndi.NTamd64.Services]
AddService = athr, 2, atheros.Service, atheros.EventLog
Include    = netvwifibus.inf
Needs      = VWiFiBus.Services

[ATHR_DEV_OS61_30A4TP.ndi.NTamd64.HW]
Include = netvwifibus.inf
Needs   = VWiFiBus.PnPFilterRegistration

[ATHR_DEV_OS61_T30A1.ndi.NTamd64]
Characteristics = 0x84
BusType         = 5
AddReg          = atheros_os61.reg, atheros11n.reg, htAdhoc.reg, triggerlevelkiteonly.reg, c3war.reg, cfpignore.reg
DelReg          = atheros.DelReg
CopyFiles       = atheros.CopyFiles
*IfType         = 71            ; IF_TYPE_IEEE80211
*MediaType      = 16            ; NdisMediumNative802_11
*PhysicalMediaType = 9          ; NdisPhysicalMediumNative802_11
Include         = netvwifibus.inf, machine.inf
Needs           = VWiFiBus.CopyFiles

[ATHR_DEV_OS61_T30A1.ndi.NTamd64.Services]
AddService = athr, 2, atheros.Service, atheros.EventLog
Include    = netvwifibus.inf
Needs      = VWiFiBus.Services

[ATHR_DEV_OS61_T30A1.ndi.NTamd64.HW]
Include = netvwifibus.inf
Needs   = VWiFiBus.PnPFilterRegistration

[ATHR_DEV_OS61_T30A4.ndi.NTamd64]
Characteristics = 0x84
BusType         = 5
AddReg          = atheros_os61.reg, atheros11n.reg, htAdhoc.reg, cfpignore.reg
DelReg          = atheros.DelReg
CopyFiles       = atheros.CopyFiles
*IfType         = 71            ; IF_TYPE_IEEE80211
*MediaType      = 16            ; NdisMediumNative802_11
*PhysicalMediaType = 9          ; NdisPhysicalMediumNative802_11
Include         = netvwifibus.inf, machine.inf
Needs           = VWiFiBus.CopyFiles

[ATHR_DEV_OS61_T30A4.ndi.NTamd64.Services]
AddService = athr, 2, atheros.Service, atheros.EventLog
Include    = netvwifibus.inf
Needs      = VWiFiBus.Services

[ATHR_DEV_OS61_T30A4.ndi.NTamd64.HW]
Include = netvwifibus.inf
Needs   = VWiFiBus.PnPFilterRegistration

[ATHR_DEV_OS61_660311AD.ndi.NTamd64]
Characteristics = 0x84
BusType         = 5
AddReg          = atheros_os61.reg, atheros11n.reg, htAdhoc.reg, customer3f.reg, amp.reg, ampFilter.reg, c3war.reg, roamPolicy2.reg, smpsDynamic.reg, maxpowersave.reg, customer1GreenTx.reg, wowenable.reg, hb97ChainMask.reg
DelReg          = atheros.DelReg
CopyFiles       = atheros.CopyFiles
*IfType         = 71            ; IF_TYPE_IEEE80211
*MediaType      = 16            ; NdisMediumNative802_11
*PhysicalMediaType = 9          ; NdisPhysicalMediumNative802_11
Include         = netvwifibus.inf, machine.inf
Needs           = VWiFiBus.CopyFiles

[ATHR_DEV_OS61_660311AD.ndi.NTamd64.Services]
AddService = athr, 2, atheros.Service, atheros.EventLog
Include    = netvwifibus.inf
Needs      = VWiFiBus.Services

[ATHR_DEV_OS61_660311AD.ndi.NTamd64.HW]
Include = netvwifibus.inf
Needs   = VWiFiBus.PnPFilterRegistration

[ATHR_DEV_OS61_03091A32.ndi.NTamd64]
Characteristics = 0x84
BusType         = 5
AddReg          = atheros_os61.reg, atheros11n.reg, htAdhoc.reg, cemspecled_func1_8.reg
DelReg          = atheros.DelReg
CopyFiles       = atheros.CopyFiles
*IfType         = 71            ; IF_TYPE_IEEE80211
*MediaType      = 16            ; NdisMediumNative802_11
*PhysicalMediaType = 9          ; NdisPhysicalMediumNative802_11
Include         = netvwifibus.inf, machine.inf
Needs           = VWiFiBus.CopyFiles

[ATHR_DEV_OS61_03091A32.ndi.NTamd64.Services]
AddService = athr, 2, atheros.Service, atheros.EventLog
Include    = netvwifibus.inf
Needs      = VWiFiBus.Services

[ATHR_DEV_OS61_03091A32.ndi.NTamd64.HW]
Include = netvwifibus.inf
Needs   = VWiFiBus.PnPFilterRegistration

[ATHR_DEV_OS61_30AA.ndi.NTamd64]
Characteristics = 0x84
BusType         = 5
AddReg          = atheros_os61.reg, atheros11n.reg, htAdhoc.reg, triggerlevelkiteonly.reg, c3war.reg, Customer15a.led.reg
DelReg          = atheros.DelReg
CopyFiles       = atheros.CopyFiles
*IfType         = 71            ; IF_TYPE_IEEE80211
*MediaType      = 16            ; NdisMediumNative802_11
*PhysicalMediaType = 9          ; NdisPhysicalMediumNative802_11
Include         = netvwifibus.inf, machine.inf
Needs           = VWiFiBus.CopyFiles

[ATHR_DEV_OS61_30AA.ndi.NTamd64.Services]
AddService = athr, 2, atheros.Service, atheros.EventLog
Include    = netvwifibus.inf
Needs      = VWiFiBus.Services

[ATHR_DEV_OS61_30AA.ndi.NTamd64.HW]
Include = netvwifibus.inf
Needs   = VWiFiBus.PnPFilterRegistration

[ATHR_DEV_OS61_30AB.ndi.NTamd64]
Characteristics = 0x84
BusType         = 5
AddReg          = atheros_os61.reg, atheros11n.reg, htAdhoc.reg, janusda.reg, triggerlevelkiteonly.reg, c3war.reg, Customer15a.led.reg, wirelessmode.2g.reg
DelReg          = atheros.DelReg
CopyFiles       = atheros.CopyFiles
*IfType         = 71            ; IF_TYPE_IEEE80211
*MediaType      = 16            ; NdisMediumNative802_11
*PhysicalMediaType = 9          ; NdisPhysicalMediumNative802_11
Include         = netvwifibus.inf, machine.inf
Needs           = VWiFiBus.CopyFiles

[ATHR_DEV_OS61_30AB.ndi.NTamd64.Services]
AddService = athr, 2, atheros.Service, atheros.EventLog
Include    = netvwifibus.inf
Needs      = VWiFiBus.Services

[ATHR_DEV_OS61_30AB.ndi.NTamd64.HW]
Include = netvwifibus.inf
Needs   = VWiFiBus.PnPFilterRegistration

[ATHR_DEV_OS61_30AB2C37.ndi.NTamd64]
Characteristics = 0x84
BusType         = 5
AddReg          = atheros_os61.reg, atheros11n.reg, htAdhoc.reg, janusda.reg, triggerlevelkiteonly.reg, c3war.reg, Customer15a.led.reg, amp.reg, ampFilter.reg, htWepTkipOpt.reg, wirelessmodeselectkite.reg
DelReg          = atheros.DelReg
CopyFiles       = atheros.CopyFiles
*IfType         = 71            ; IF_TYPE_IEEE80211
*MediaType      = 16            ; NdisMediumNative802_11
*PhysicalMediaType = 9          ; NdisPhysicalMediumNative802_11
Include         = netvwifibus.inf, machine.inf
Needs           = VWiFiBus.CopyFiles

[ATHR_DEV_OS61_30AB2C37.ndi.NTamd64.Services]
AddService = athr, 2, atheros.Service, atheros.EventLog
Include    = netvwifibus.inf
Needs      = VWiFiBus.Services

[ATHR_DEV_OS61_30AB2C37.ndi.NTamd64.HW]
Include = netvwifibus.inf
Needs   = VWiFiBus.PnPFilterRegistration

; 2C371A3B
[ATHR_DEV_OS61_2C371A3B.ndi.NTamd64]
Characteristics = 0x84
BusType         = 5
AddReg          = atheros_os61.reg, atheros11n.reg, htAdhoc.reg, janusda.reg, triggerlevelkiteonly.reg, c3war.reg, Customer15a.led.reg, bt30_high_speed.reg, ampFilter.reg, htWepTkipOpt.reg, wirelessmodeselectkite.reg
DelReg          = atheros.DelReg
CopyFiles       = atheros.CopyFiles
*IfType         = 71            ; IF_TYPE_IEEE80211
*MediaType      = 16            ; NdisMediumNative802_11
*PhysicalMediaType = 9          ; NdisPhysicalMediumNative802_11
Include         = netvwifibus.inf, machine.inf
Needs           = VWiFiBus.CopyFiles

[ATHR_DEV_OS61_2C371A3B.ndi.NTamd64.Services]
AddService = athr, 2, atheros.Service, atheros.EventLog
Include    = netvwifibus.inf
Needs      = VWiFiBus.Services

[ATHR_DEV_OS61_2C371A3B.ndi.NTamd64.HW]
Include = netvwifibus.inf
Needs   = VWiFiBus.PnPFilterRegistration

[ATHR_DEV_OS61_30B0.ndi.NTamd64]
Characteristics = 0x84
BusType         = 5
AddReg          = atheros_os61.reg, atheros11n.reg, htAdhoc.reg, heliusda.reg
DelReg          = atheros.DelReg
CopyFiles       = atheros.CopyFiles
*IfType         = 71            ; IF_TYPE_IEEE80211
*MediaType      = 16            ; NdisMediumNative802_11
*PhysicalMediaType = 9          ; NdisPhysicalMediumNative802_11
Include         = netvwifibus.inf, machine.inf
Needs           = VWiFiBus.CopyFiles

[ATHR_DEV_OS61_30B0.ndi.NTamd64.Services]
AddService = athr, 2, atheros.Service, atheros.EventLog
Include    = netvwifibus.inf
Needs      = VWiFiBus.Services

[ATHR_DEV_OS61_30B0.ndi.NTamd64.HW]
Include = netvwifibus.inf
Needs   = VWiFiBus.PnPFilterRegistration

[ATHR_DEV_OS61_30B07189.ndi.NTamd64]
Characteristics = 0x84
BusType         = 5
AddReg          = atheros_os61.reg, atheros11n.reg, htAdhoc.reg, heliusda.reg, btcoexa2dp99.reg, cmdRegister.reg, ignore11denable.reg
DelReg          = atheros.DelReg
CopyFiles       = atheros.CopyFiles
*IfType         = 71            ; IF_TYPE_IEEE80211
*MediaType      = 16            ; NdisMediumNative802_11
*PhysicalMediaType = 9          ; NdisPhysicalMediumNative802_11
Include         = netvwifibus.inf, machine.inf
Needs           = VWiFiBus.CopyFiles

[ATHR_DEV_OS61_30B07189.ndi.NTamd64.Services]
AddService = athr, 2, atheros.Service, atheros.EventLog
Include    = netvwifibus.inf
Needs      = VWiFiBus.Services

[ATHR_DEV_OS61_30B07189.ndi.NTamd64.HW]
Include = netvwifibus.inf
Needs   = VWiFiBus.PnPFilterRegistration

[ATHR_DEV_OS61_30ABLT.ndi.NTamd64]
Characteristics = 0x84
BusType         = 5
AddReg          = atheros_os61.reg, atheros11n.reg, htAdhoc.reg, janusda.reg, cemspecled_func0_1.reg, triggerlevelkiteonly.reg, c3war.reg
DelReg          = atheros.DelReg
CopyFiles       = atheros.CopyFiles
*IfType         = 71            ; IF_TYPE_IEEE80211
*MediaType      = 16            ; NdisMediumNative802_11
*PhysicalMediaType = 9          ; NdisPhysicalMediumNative802_11
Include         = netvwifibus.inf, machine.inf
Needs           = VWiFiBus.CopyFiles

[ATHR_DEV_OS61_30ABLT.ndi.NTamd64.Services]
AddService = athr, 2, atheros.Service, atheros.EventLog
Include    = netvwifibus.inf
Needs      = VWiFiBus.Services

[ATHR_DEV_OS61_30ABLT.ndi.NTamd64.HW]
Include = netvwifibus.inf
Needs   = VWiFiBus.PnPFilterRegistration

[ATHR_DEV_OS61_30A1LT.ndi.NTamd64]
Characteristics = 0x84
BusType         = 5
AddReg          = atheros_os61.reg, atheros11n.reg, htAdhoc.reg, cemspecled_func0_1.reg, triggerlevelkiteonly.reg, c3war.reg
DelReg          = atheros.DelReg
CopyFiles       = atheros.CopyFiles
*IfType         = 71            ; IF_TYPE_IEEE80211
*MediaType      = 16            ; NdisMediumNative802_11
*PhysicalMediaType = 9          ; NdisPhysicalMediumNative802_11
Include         = netvwifibus.inf, machine.inf
Needs           = VWiFiBus.CopyFiles

[ATHR_DEV_OS61_30A1LT.ndi.NTamd64.Services]
AddService = athr, 2, atheros.Service, atheros.EventLog
Include    = netvwifibus.inf
Needs      = VWiFiBus.Services

[ATHR_DEV_OS61_30A1LT.ndi.NTamd64.HW]
Include = netvwifibus.inf
Needs   = VWiFiBus.PnPFilterRegistration

[ATHR_DEV_OS61_BA91167D.ndi.NTamd64]
Characteristics = 0x84
BusType         = 5
AddReg          = atheros_os61.reg, atheros11n.reg, htAdhoc.reg, janusda.reg, cemspecled_func1_1.reg, triggerlevelkiteonly.reg, c3war.reg
DelReg          = atheros.DelReg
CopyFiles       = atheros.CopyFiles
*IfType         = 71            ; IF_TYPE_IEEE80211
*MediaType      = 16            ; NdisMediumNative802_11
*PhysicalMediaType = 9          ; NdisPhysicalMediumNative802_11
Include         = netvwifibus.inf, machine.inf
Needs           = VWiFiBus.CopyFiles

[ATHR_DEV_OS61_BA91167D.ndi.NTamd64.Services]
AddService = athr, 2, atheros.Service, atheros.EventLog
Include    = netvwifibus.inf
Needs      = VWiFiBus.Services

[ATHR_DEV_OS61_BA91167D.ndi.NTamd64.HW]
Include = netvwifibus.inf
Needs   = VWiFiBus.PnPFilterRegistration

[ATHR_DEV_OS61_7173144Fw.ndi.NTamd64]
Characteristics = 0x84
BusType         = 5
AddReg          = atheros_os61.reg, atheros11n.reg, htAdhoc.reg, janusda_CoexAgent0.reg, triggerlevelkiteonly.reg, c3war.reg, roamPolicy.reg, ampGuid.reg, cfpignore.reg
DelReg          = atheros.DelReg
CopyFiles       = atheros.CopyFiles
*IfType         = 71            ; IF_TYPE_IEEE80211
*MediaType      = 16            ; NdisMediumNative802_11
*PhysicalMediaType = 9          ; NdisPhysicalMediumNative802_11
Include         = netvwifibus.inf, machine.inf
Needs           = VWiFiBus.CopyFiles

[ATHR_DEV_OS61_7173144Fw.ndi.NTamd64.Services]
AddService = athr, 2, atheros.Service, atheros.EventLog
Include    = netvwifibus.inf
Needs      = VWiFiBus.Services

[ATHR_DEV_OS61_7173144Fw.ndi.NTamd64.HW]
Include = netvwifibus.inf
Needs   = VWiFiBus.PnPFilterRegistration

[ATHR_DEV_OS61_30A1a.ndi.NTamd64]
Characteristics = 0x84
BusType         = 5
AddReg          = atheros_os61.reg, atheros11n.reg, htAdhoc.reg, cmdRegister.reg, triggerlevelkiteonly.reg, c3war.reg, rxLatencyWar.reg, ignore11denable.reg
DelReg          = atheros.DelReg
CopyFiles       = atheros.CopyFiles
*IfType         = 71            ; IF_TYPE_IEEE80211
*MediaType      = 16            ; NdisMediumNative802_11
*PhysicalMediaType = 9          ; NdisPhysicalMediumNative802_11
Include         = netvwifibus.inf, machine.inf
Needs           = VWiFiBus.CopyFiles

[ATHR_DEV_OS61_30A1a.ndi.NTamd64.Services]
AddService = athr, 2, atheros.Service, atheros.EventLog
Include    = netvwifibus.inf
Needs      = VWiFiBus.Services

[ATHR_DEV_OS61_30A1a.ndi.NTamd64.HW]
Include = netvwifibus.inf
Needs   = VWiFiBus.PnPFilterRegistration

[ATHR_DEV_OS61_30A1w.ndi.NTamd64]
Characteristics = 0x84
BusType         = 5
AddReg          = atheros_os61.reg, atheros11n.reg, htAdhoc.reg, cmdRegister.reg, janusda_coexPTA_40_21.reg, triggerlevelkiteonly.reg, c3war.reg, rxLatencyWar.reg, ignore11denable.reg
DelReg          = atheros.DelReg
CopyFiles       = atheros.CopyFiles
*IfType         = 71            ; IF_TYPE_IEEE80211
*MediaType      = 16            ; NdisMediumNative802_11
*PhysicalMediaType = 9          ; NdisPhysicalMediumNative802_11
Include         = netvwifibus.inf, machine.inf
Needs           = VWiFiBus.CopyFiles

[ATHR_DEV_OS61_30A1w.ndi.NTamd64.Services]
AddService = athr, 2, atheros.Service, atheros.EventLog
Include    = netvwifibus.inf
Needs      = VWiFiBus.Services

[ATHR_DEV_OS61_30A1w.ndi.NTamd64.HW]
Include = netvwifibus.inf
Needs   = VWiFiBus.PnPFilterRegistration

[ATHR_DEV_OS61_E023105B.ndi.NTamd64]
Characteristics = 0x84
BusType         = 5
AddReg          = atheros_os61.reg, atheros11n.reg, htAdhoc.reg, cemspecled_func1_1.reg, triggerlevelkiteonly.reg, c3war.reg
DelReg          = atheros.DelReg
CopyFiles       = atheros.CopyFiles
*IfType         = 71            ; IF_TYPE_IEEE80211
*MediaType      = 16            ; NdisMediumNative802_11
*PhysicalMediaType = 9          ; NdisPhysicalMediumNative802_11
Include         = netvwifibus.inf, machine.inf
Needs           = VWiFiBus.CopyFiles

[ATHR_DEV_OS61_E023105B.ndi.NTamd64.Services]
AddService = athr, 2, atheros.Service, atheros.EventLog
Include    = netvwifibus.inf
Needs      = VWiFiBus.Services

[ATHR_DEV_OS61_E023105B.ndi.NTamd64.HW]
Include = netvwifibus.inf
Needs   = VWiFiBus.PnPFilterRegistration

[ATHR_DEV_OS61_E036105B.ndi.NTamd64]
Characteristics = 0x84
BusType         = 5
AddReg          = atheros_os61.reg, atheros11n.reg, htAdhoc.reg, cemspecled_func2_1.reg, triggerlevelkiteonly.reg, c3war.reg
DelReg          = atheros.DelReg
CopyFiles       = atheros.CopyFiles
*IfType         = 71            ; IF_TYPE_IEEE80211
*MediaType      = 16            ; NdisMediumNative802_11
*PhysicalMediaType = 9          ; NdisPhysicalMediumNative802_11
Include         = netvwifibus.inf, machine.inf
Needs           = VWiFiBus.CopyFiles

[ATHR_DEV_OS61_E036105B.ndi.NTamd64.Services]
AddService = athr, 2, atheros.Service, atheros.EventLog
Include    = netvwifibus.inf
Needs      = VWiFiBus.Services

[ATHR_DEV_OS61_E036105B.ndi.NTamd64.HW]
Include = netvwifibus.inf
Needs   = VWiFiBus.PnPFilterRegistration

[ATHR_DEV_OS61_E033105Bw.ndi.NTamd64]
Characteristics = 0x84
BusType         = 5
AddReg          = atheros_os61.reg, atheros11n.reg, htAdhoc.reg, cemspecled_func1_1.reg, janusda.reg, triggerlevelkiteonly.reg, c3war.reg
DelReg          = atheros.DelReg
CopyFiles       = atheros.CopyFiles
*IfType         = 71            ; IF_TYPE_IEEE80211
*MediaType      = 16            ; NdisMediumNative802_11
*PhysicalMediaType = 9          ; NdisPhysicalMediumNative802_11
Include         = netvwifibus.inf, machine.inf
Needs           = VWiFiBus.CopyFiles

[ATHR_DEV_OS61_E033105Bw.ndi.NTamd64.Services]
AddService = athr, 2, atheros.Service, atheros.EventLog
Include    = netvwifibus.inf
Needs      = VWiFiBus.Services

[ATHR_DEV_OS61_E033105Bw.ndi.NTamd64.HW]
Include = netvwifibus.inf
Needs   = VWiFiBus.PnPFilterRegistration

[ATHR_DEV_OS61_E029105B.ndi.NTamd64]
Characteristics = 0x84
BusType         = 5
AddReg          = atheros_os61.reg, atheros.reg, cemspecled_func1_1.reg
DelReg          = atheros.DelReg
CopyFiles       = atheros.CopyFiles
*IfType         = 71            ; IF_TYPE_IEEE80211
*MediaType      = 16            ; NdisMediumNative802_11
*PhysicalMediaType = 9          ; NdisPhysicalMediumNative802_11
Include         = netvwifibus.inf, machine.inf
Needs           = VWiFiBus.CopyFiles

[ATHR_DEV_OS61_E029105B.ndi.NTamd64.Services]
AddService = athr, 2, atheros.Service, atheros.EventLog
Include    = netvwifibus.inf
Needs      = VWiFiBus.Services

[ATHR_DEV_OS61_E029105B.ndi.NTamd64.HW]
Include = netvwifibus.inf
Needs   = VWiFiBus.PnPFilterRegistration

[ATHR_DEV_OS61_11121A3B.ndi.NTamd64]
Characteristics = 0x84
BusType         = 5
AddReg          = atheros_os61.reg, atheros.reg, cemspecled_func1_1.reg
DelReg          = atheros.DelReg
CopyFiles       = atheros.CopyFiles
*IfType         = 71            ; IF_TYPE_IEEE80211
*MediaType      = 16            ; NdisMediumNative802_11
*PhysicalMediaType = 9          ; NdisPhysicalMediumNative802_11
Include         = netvwifibus.inf, machine.inf
Needs           = VWiFiBus.CopyFiles

[ATHR_DEV_OS61_11121A3B.ndi.NTamd64.Services]
AddService = athr, 2, atheros.Service, atheros.EventLog
Include    = netvwifibus.inf
Needs      = VWiFiBus.Services

[ATHR_DEV_OS61_11121A3B.ndi.NTamd64.HW]
Include = netvwifibus.inf
Needs   = VWiFiBus.PnPFilterRegistration

[ATHR_DEV_OS61_662111AD.ndi.NTamd64]
Characteristics = 0x84
BusType         = 5
AddReg          = atheros_os61.reg, atheros11n.reg, cemspecled_func1_1.reg, htAdhoc.reg, triggerlevelkiteonly.reg, c3war.reg, MCCStaTputAdjust.reg
DelReg          = atheros.DelReg
CopyFiles       = atheros.CopyFiles
*IfType         = 71            ; IF_TYPE_IEEE80211
*MediaType      = 16            ; NdisMediumNative802_11
*PhysicalMediaType = 9          ; NdisPhysicalMediumNative802_11
Include         = netvwifibus.inf, machine.inf
Needs           = VWiFiBus.CopyFiles

[ATHR_DEV_OS61_662111AD.ndi.NTamd64.Services]
AddService = athr, 2, atheros.Service, atheros.EventLog
Include    = netvwifibus.inf
Needs      = VWiFiBus.Services

[ATHR_DEV_OS61_662111AD.ndi.NTamd64.HW]
Include = netvwifibus.inf
Needs   = VWiFiBus.PnPFilterRegistration

[ATHR_DEV_OS61_662211AD.ndi.NTamd64]
Characteristics = 0x84
BusType         = 5
AddReg          = atheros_os61.reg, atheros11n.reg, cemspecled_func1_1.reg, htAdhoc.reg
DelReg          = atheros.DelReg
CopyFiles       = atheros.CopyFiles
*IfType         = 71            ; IF_TYPE_IEEE80211
*MediaType      = 16            ; NdisMediumNative802_11
*PhysicalMediaType = 9          ; NdisPhysicalMediumNative802_11
Include         = netvwifibus.inf, machine.inf
Needs           = VWiFiBus.CopyFiles

[ATHR_DEV_OS61_662211AD.ndi.NTamd64.Services]
AddService = athr, 2, atheros.Service, atheros.EventLog
Include    = netvwifibus.inf
Needs      = VWiFiBus.Services

[ATHR_DEV_OS61_662211AD.ndi.NTamd64.HW]
Include = netvwifibus.inf
Needs   = VWiFiBus.PnPFilterRegistration

[ATHR_DEV_OS61_3091PB.ndi.NTamd64]
Characteristics = 0x84
BusType         = 5
AddReg          = atheros_os61.reg, atheros11n.reg, pushbutton.reg, smpsDynamic.reg, htAdhoc.reg
DelReg          = atheros.DelReg
CopyFiles       = atheros.CopyFiles
*IfType         = 71            ; IF_TYPE_IEEE80211
*MediaType      = 16            ; NdisMediumNative802_11
*PhysicalMediaType = 9          ; NdisPhysicalMediumNative802_11
Include         = netvwifibus.inf, machine.inf
Needs           = VWiFiBus.CopyFiles

[ATHR_DEV_OS61_3091PB.ndi.NTamd64.Services]
AddService = athr, 2, atheros.Service, atheros.EventLog
Include    = netvwifibus.inf
Needs      = VWiFiBus.Services

[ATHR_DEV_OS61_3091PB.ndi.NTamd64.HW]
Include = netvwifibus.inf
Needs   = VWiFiBus.PnPFilterRegistration

[ATHR_DEV_OS61_1000168C.ndi.NTamd64]
Characteristics = 0x84
BusType         = 5
AddReg          = atheros_os61.reg, atheros11n.reg, customer2merlin.reg, smpsDynamic.reg, htAdhoc.reg, fastclockdisable.reg
DelReg          = atheros.DelReg
CopyFiles       = atheros.CopyFiles
*IfType         = 71            ; IF_TYPE_IEEE80211
*MediaType      = 16            ; NdisMediumNative802_11
*PhysicalMediaType = 9          ; NdisPhysicalMediumNative802_11
Include         = netvwifibus.inf, machine.inf
Needs           = VWiFiBus.CopyFiles

[ATHR_DEV_OS61_1000168C.ndi.NTamd64.Services]
AddService = athr, 2, atheros.Service, atheros.EventLog
Include    = netvwifibus.inf
Needs      = VWiFiBus.Services

[ATHR_DEV_OS61_1000168C.ndi.NTamd64.HW]
Include = netvwifibus.inf
Needs   = VWiFiBus.PnPFilterRegistration

[ATHR_DEV_OS61_1001168C.ndi.NTamd64]
Characteristics = 0x84
BusType         = 5
AddReg          = atheros_os61.reg, atheros11n.reg, customer2.11n.reg, smpsDynamic.reg, htAdhoc.reg, fastclockdisable.reg
DelReg          = atheros.DelReg
CopyFiles       = atheros.CopyFiles
*IfType         = 71            ; IF_TYPE_IEEE80211
*MediaType      = 16            ; NdisMediumNative802_11
*PhysicalMediaType = 9          ; NdisPhysicalMediumNative802_11
Include         = netvwifibus.inf, machine.inf
Needs           = VWiFiBus.CopyFiles

[ATHR_DEV_OS61_1001168C.ndi.NTamd64.Services]
AddService = athr, 2, atheros.Service, atheros.EventLog
Include    = netvwifibus.inf
Needs      = VWiFiBus.Services

[ATHR_DEV_OS61_1001168C.ndi.NTamd64.HW]
Include = netvwifibus.inf
Needs   = VWiFiBus.PnPFilterRegistration

[ATHR_DEV_OS61_3091SF.ndi.NTamd64]
Characteristics = 0x84
BusType         = 5
AddReg          = atheros_os61.reg, atheros11n.reg, customer_Samsung.reg, smpsDynamic.reg, htAdhoc.reg, cmdRegister.reg, ignore11denable.reg
DelReg          = atheros.DelReg
CopyFiles       = atheros.CopyFiles
*IfType         = 71            ; IF_TYPE_IEEE80211
*MediaType      = 16            ; NdisMediumNative802_11
*PhysicalMediaType = 9          ; NdisPhysicalMediumNative802_11
Include         = netvwifibus.inf, machine.inf
Needs           = VWiFiBus.CopyFiles

[ATHR_DEV_OS61_3091SF.ndi.NTamd64.Services]
AddService = athr, 2, atheros.Service, atheros.EventLog
Include    = netvwifibus.inf
Needs      = VWiFiBus.Services

[ATHR_DEV_OS61_3091SF.ndi.NTamd64.HW]
Include = netvwifibus.inf
Needs   = VWiFiBus.PnPFilterRegistration

[ATHR_DEV_OS61_03051A32.ndi.NTamd64]
Characteristics = 0x84
BusType         = 5
AddReg          = atheros_os61.reg, atheros11n.reg, cemspecled_func1_1.reg, htAdhoc.reg, triggerlevelkiteonly.reg, c3war.reg
DelReg          = atheros.DelReg
CopyFiles       = atheros.CopyFiles
*IfType         = 71            ; IF_TYPE_IEEE80211
*MediaType      = 16            ; NdisMediumNative802_11
*PhysicalMediaType = 9          ; NdisPhysicalMediumNative802_11
Include         = netvwifibus.inf, machine.inf
Needs           = VWiFiBus.CopyFiles

[ATHR_DEV_OS61_03051A32.ndi.NTamd64.Services]
AddService = athr, 2, atheros.Service, atheros.EventLog
Include    = netvwifibus.inf
Needs      = VWiFiBus.Services

[ATHR_DEV_OS61_03051A32.ndi.NTamd64.HW]
Include = netvwifibus.inf
Needs   = VWiFiBus.PnPFilterRegistration

[ATHR_DEV_OS61_03051A32w.ndi.NTamd64]
Characteristics = 0x84
BusType         = 5
AddReg          = atheros_os61.reg, atheros11n.reg, cemspecled_func1_1.reg, htAdhoc.reg, janusda.reg, triggerlevelkiteonly.reg, c3war.reg
DelReg          = atheros.DelReg
CopyFiles       = atheros.CopyFiles
*IfType         = 71            ; IF_TYPE_IEEE80211
*MediaType      = 16            ; NdisMediumNative802_11
*PhysicalMediaType = 9          ; NdisPhysicalMediumNative802_11
Include         = netvwifibus.inf, machine.inf
Needs           = VWiFiBus.CopyFiles

[ATHR_DEV_OS61_03051A32w.ndi.NTamd64.Services]
AddService = athr, 2, atheros.Service, atheros.EventLog
Include    = netvwifibus.inf
Needs      = VWiFiBus.Services

[ATHR_DEV_OS61_03051A32w.ndi.NTamd64.HW]
Include = netvwifibus.inf
Needs   = VWiFiBus.PnPFilterRegistration

[ATHR_DEV_OS61_D8111113.ndi.NTamd64]
Characteristics = 0x84
BusType         = 5
AddReg          = atheros_os61.reg, atheros11n.reg, cemspecled_func1_1.reg, htAdhoc.reg, triggerlevelkiteonly.reg, c3war.reg
DelReg          = atheros.DelReg
CopyFiles       = atheros.CopyFiles
*IfType         = 71            ; IF_TYPE_IEEE80211
*MediaType      = 16            ; NdisMediumNative802_11
*PhysicalMediaType = 9          ; NdisPhysicalMediumNative802_11
Include         = netvwifibus.inf, machine.inf
Needs           = VWiFiBus.CopyFiles

[ATHR_DEV_OS61_D8111113.ndi.NTamd64.Services]
AddService = athr, 2, atheros.Service, atheros.EventLog
Include    = netvwifibus.inf
Needs      = VWiFiBus.Services

[ATHR_DEV_OS61_D8111113.ndi.NTamd64.HW]
Include = netvwifibus.inf
Needs   = VWiFiBus.PnPFilterRegistration

[ATHR_DEV_OS61_10891A3B.ndi.NTamd64]
Characteristics = 0x84
BusType         = 5
AddReg          = atheros_os61.reg, atheros11n.reg, cemspecled_func1_1.reg, htWepTkipOpt.reg, htAdhoc.reg, wirelessmodeselectkite.reg, triggerlevelkiteonly.reg, c3war.reg
DelReg          = atheros.DelReg
CopyFiles       = atheros.CopyFiles
*IfType         = 71            ; IF_TYPE_IEEE80211
*MediaType      = 16            ; NdisMediumNative802_11
*PhysicalMediaType = 9          ; NdisPhysicalMediumNative802_11
Include         = netvwifibus.inf, machine.inf
Needs           = VWiFiBus.CopyFiles

[ATHR_DEV_OS61_10891A3B.ndi.NTamd64.Services]
AddService = athr, 2, atheros.Service, atheros.EventLog
Include    = netvwifibus.inf
Needs      = VWiFiBus.Services

[ATHR_DEV_OS61_10891A3B.ndi.NTamd64.HW]
Include = netvwifibus.inf
Needs   = VWiFiBus.PnPFilterRegistration

[ATHR_DEV_OS61_1D891A3B.ndi.NTamd64]
Characteristics = 0x84
BusType         = 5
AddReg          = atheros_os61.reg, atheros11n.reg, cemspecled_func1_1.reg, htWepTkipOpt.reg, htAdhoc.reg, wirelessmodeselectkite.reg, triggerlevelkiteonly.reg, c3war.reg, amp.reg, ampFilter.reg
DelReg          = atheros.DelReg
CopyFiles       = atheros.CopyFiles
*IfType         = 71            ; IF_TYPE_IEEE80211
*MediaType      = 16            ; NdisMediumNative802_11
*PhysicalMediaType = 9          ; NdisPhysicalMediumNative802_11
Include         = netvwifibus.inf, machine.inf
Needs           = VWiFiBus.CopyFiles

[ATHR_DEV_OS61_1D891A3B.ndi.NTamd64.Services]
AddService = athr, 2, atheros.Service, atheros.EventLog
Include    = netvwifibus.inf
Needs      = VWiFiBus.Services

[ATHR_DEV_OS61_1D891A3B.ndi.NTamd64.HW]
Include = netvwifibus.inf
Needs   = VWiFiBus.PnPFilterRegistration

[ATHR_DEV_OS61_11211A3B.ndi.NTamd64]
Characteristics = 0x84
BusType         = 5
AddReg          = atheros_os61.reg, atheros11n.reg, cemspecled_func2_8.reg, htWepTkipOpt.reg, htAdhoc.reg, wirelessmodeselectkite.reg
DelReg          = atheros.DelReg
CopyFiles       = atheros.CopyFiles
*IfType         = 71            ; IF_TYPE_IEEE80211
*MediaType      = 16            ; NdisMediumNative802_11
*PhysicalMediaType = 9          ; NdisPhysicalMediumNative802_11
Include         = netvwifibus.inf, machine.inf
Needs           = VWiFiBus.CopyFiles

[ATHR_DEV_OS61_11211A3B.ndi.NTamd64.Services]
AddService = athr, 2, atheros.Service, atheros.EventLog
Include    = netvwifibus.inf
Needs      = VWiFiBus.Services

[ATHR_DEV_OS61_11211A3B.ndi.NTamd64.HW]
Include = netvwifibus.inf
Needs   = VWiFiBus.PnPFilterRegistration

[ATHR_DEV_OS61_1A211A3B.ndi.NTamd64]
Characteristics = 0x84
BusType         = 5
AddReg          = atheros_os61.reg, atheros.reg, cemspecled_func2_8.reg, htWepTkipOpt.reg, htAdhoc.reg, wirelessmodeselectkite.reg
DelReg          = atheros.DelReg
CopyFiles       = atheros.CopyFiles
*IfType         = 71            ; IF_TYPE_IEEE80211
*MediaType      = 16            ; NdisMediumNative802_11
*PhysicalMediaType = 9          ; NdisPhysicalMediumNative802_11
Include         = netvwifibus.inf, machine.inf
Needs           = VWiFiBus.CopyFiles

[ATHR_DEV_OS61_1A211A3B.ndi.NTamd64.Services]
AddService = athr, 2, atheros.Service, atheros.EventLog
Include    = netvwifibus.inf
Needs      = VWiFiBus.Services

[ATHR_DEV_OS61_1A211A3B.ndi.NTamd64.HW]
Include = netvwifibus.inf
Needs   = VWiFiBus.PnPFilterRegistration

[ATHR_DEV_OS61_20371A3B.ndi.NTamd64]
Characteristics = 0x84
BusType         = 5
AddReg          = atheros_os61.reg, atheros11n.reg, cemspecled_func1_1.reg, htEnableWepTkip.reg, htAdhoc.reg, wirelessmodeselectkite.reg, triggerlevelkiteonly.reg, c3war.reg
DelReg          = atheros.DelReg
CopyFiles       = atheros.CopyFiles
*IfType         = 71            ; IF_TYPE_IEEE80211
*MediaType      = 16            ; NdisMediumNative802_11
*PhysicalMediaType = 9          ; NdisPhysicalMediumNative802_11
Include         = netvwifibus.inf, machine.inf
Needs           = VWiFiBus.CopyFiles

[ATHR_DEV_OS61_20371A3B.ndi.NTamd64.Services]
AddService = athr, 2, atheros.Service, atheros.EventLog
Include    = netvwifibus.inf
Needs      = VWiFiBus.Services

[ATHR_DEV_OS61_20371A3B.ndi.NTamd64.HW]
Include = netvwifibus.inf
Needs   = VWiFiBus.PnPFilterRegistration

[ATHR_DEV_OS61_1A891A3B.ndi.NTamd64]
Characteristics = 0x84
BusType         = 5
AddReg          = atheros_os61.reg, atheros11n.reg, cemspecled_func1_1.reg, triggerlevelkiteonly.reg, c3war.reg
DelReg          = atheros.DelReg
CopyFiles       = atheros.CopyFiles
*IfType         = 71            ; IF_TYPE_IEEE80211
*MediaType      = 16            ; NdisMediumNative802_11
*PhysicalMediaType = 9          ; NdisPhysicalMediumNative802_11
Include         = netvwifibus.inf, machine.inf
Needs           = VWiFiBus.CopyFiles

[ATHR_DEV_OS61_1A891A3B.ndi.NTamd64.Services]
AddService = athr, 2, atheros.Service, atheros.EventLog
Include    = netvwifibus.inf
Needs      = VWiFiBus.Services

[ATHR_DEV_OS61_1A891A3B.ndi.NTamd64.HW]
Include = netvwifibus.inf
Needs   = VWiFiBus.PnPFilterRegistration

[ATHR_DEV_OS61_2A371A3B.ndi.NTamd64]
Characteristics = 0x84
BusType         = 5
AddReg          = atheros_os61.reg, atheros11n.reg, Customer15a.led.reg, triggerlevelkiteonly.reg, c3war.reg, janusda.reg
DelReg          = atheros.DelReg
CopyFiles       = atheros.CopyFiles
*IfType         = 71            ; IF_TYPE_IEEE80211
*MediaType      = 16            ; NdisMediumNative802_11
*PhysicalMediaType = 9          ; NdisPhysicalMediumNative802_11
Include         = netvwifibus.inf, machine.inf
Needs           = VWiFiBus.CopyFiles

[ATHR_DEV_OS61_2A371A3B.ndi.NTamd64.Services]
AddService = athr, 2, atheros.Service, atheros.EventLog
Include    = netvwifibus.inf
Needs      = VWiFiBus.Services

[ATHR_DEV_OS61_2A371A3B.ndi.NTamd64.HW]
Include = netvwifibus.inf
Needs   = VWiFiBus.PnPFilterRegistration

[ATHR_DEV_OS61_2C971A3B.ndi.NTamd64]
Characteristics = 0x84
BusType         = 5
AddReg          = atheros_os61.reg, atheros11n.reg, htAdhoc.reg, 9485BTcoex.reg, customer2GreenTx.reg, paprdenable.reg, cemspecled_func2_6.reg
DelReg          = atheros.DelReg
CopyFiles       = atheros.CopyFiles
*IfType         = 71        ; IF_TYPE_IEEE80211
*MediaType      = 16        ; NdisMediumNative802_11
*PhysicalMediaType = 9      ; NdisPhysicalMediumNative802_11
Include         = netvwifibus.inf, machine.inf
Needs           = VWiFiBus.CopyFiles

[ATHR_DEV_OS61_2C971A3B.ndi.NTamd64.Services]
AddService = athr, 2, atheros.Service, atheros.EventLog
Include    = netvwifibus.inf
Needs      = VWiFiBus.Services

[ATHR_DEV_OS61_2C971A3B.ndi.NTamd64.HW]
Include = netvwifibus.inf
Needs   = PciASPMOptIn, VWiFiBus.PnPFilterRegistration

[ATHR_DEV_OS61_2C971A3B_1.ndi.NTamd64]
Characteristics = 0x84
BusType         = 5
AddReg          = atheros_os61.reg, atheros11n.reg, htAdhoc.reg, 9485BTcoex.reg, customer2GreenTx.reg, paprdenable.reg, cemspecled_func2_6.reg
DelReg          = atheros.DelReg
CopyFiles       = atheros.CopyFiles
*IfType         = 71        ; IF_TYPE_IEEE80211
*MediaType      = 16        ; NdisMediumNative802_11
*PhysicalMediaType = 9      ; NdisPhysicalMediumNative802_11
Include         = netvwifibus.inf, machine.inf
Needs           = VWiFiBus.CopyFiles

[ATHR_DEV_OS61_2C971A3B_1.ndi.NTamd64.Services]
AddService = athr, 2, atheros.Service, atheros.EventLog
Include    = netvwifibus.inf
Needs      = VWiFiBus.Services

[ATHR_DEV_OS61_2C971A3B_1.ndi.NTamd64.HW]
Include = netvwifibus.inf
Needs   = PciASPMOptIn, VWiFiBus.PnPFilterRegistration

; 662811AD
[ATHR_DEV_OS61_662811AD.ndi.NTamd64]
Characteristics = 0x84
BusType         = 5
AddReg          = atheros_os61.reg, atheros11n.reg, htAdhoc.reg, 9485BTcoexPTA.reg, customer2GreenTx.reg, paprdenable.reg, cemspecled_func2_6.reg, bt30_high_speed.reg
DelReg          = atheros.DelReg
CopyFiles       = atheros.CopyFiles
*IfType         = 71        ; IF_TYPE_IEEE80211
*MediaType      = 16        ; NdisMediumNative802_11
*PhysicalMediaType = 9      ; NdisPhysicalMediumNative802_11
Include         = netvwifibus.inf, machine.inf
Needs           = VWiFiBus.CopyFiles

[ATHR_DEV_OS61_662811AD.ndi.NTamd64.Services]
AddService = athr, 2, atheros.Service, atheros.EventLog
Include    = netvwifibus.inf
Needs      = VWiFiBus.Services

[ATHR_DEV_OS61_662811AD.ndi.NTamd64.HW]
Include = netvwifibus.inf
Needs   = PciASPMOptIn, VWiFiBus.PnPFilterRegistration

; 2C971A3B
[ATHR_DEV_OS61_2C971A3B_3.ndi.NTamd64]
Characteristics = 0x84
BusType         = 5
AddReg          = atheros_os61.reg, atheros11n.reg, htAdhoc.reg, 9485BTcoexPTA.reg, customer2GreenTx.reg, paprdenable.reg, cemspecled_func2_6.reg, bt30_high_speed.reg
DelReg          = atheros.DelReg
CopyFiles       = atheros.CopyFiles
*IfType         = 71        ; IF_TYPE_IEEE80211
*MediaType      = 16        ; NdisMediumNative802_11
*PhysicalMediaType = 9      ; NdisPhysicalMediumNative802_11
Include         = netvwifibus.inf, machine.inf
Needs           = VWiFiBus.CopyFiles

[ATHR_DEV_OS61_2C971A3B_3.ndi.NTamd64.Services]
AddService = athr, 2, atheros.Service, atheros.EventLog
Include    = netvwifibus.inf
Needs      = VWiFiBus.Services

[ATHR_DEV_OS61_2C971A3B_3.ndi.NTamd64.HW]
Include = netvwifibus.inf
Needs   = PciASPMOptIn, VWiFiBus.PnPFilterRegistration

[ATHR_DEV_OS61_20971A3B.ndi.NTamd64]
Characteristics = 0x84
BusType         = 5
AddReg          = atheros_os61.reg, atheros11n.reg, htAdhoc.reg, 9485BTcoex.reg, customer2GreenTx.reg, paprdenable.reg, cemspecled_func2_6.reg, S5wow.reg
DelReg          = atheros.DelReg
CopyFiles       = atheros.CopyFiles
*IfType         = 71        ; IF_TYPE_IEEE80211
*MediaType      = 16        ; NdisMediumNative802_11
*PhysicalMediaType = 9      ; NdisPhysicalMediumNative802_11
Include         = netvwifibus.inf, machine.inf
Needs           = VWiFiBus.CopyFiles

[ATHR_DEV_OS61_20971A3B.ndi.NTamd64.Services]
AddService = athr, 2, atheros.Service, atheros.EventLog
Include    = netvwifibus.inf
Needs      = VWiFiBus.Services

[ATHR_DEV_OS61_20971A3B.ndi.NTamd64.HW]
Include = netvwifibus.inf
Needs   = PciASPMOptIn, VWiFiBus.PnPFilterRegistration

[ATHR_DEV_OS61_209C1A3B.ndi.NTamd64]
Characteristics = 0x84
BusType         = 5
AddReg          = atheros_os61.reg, atheros11n.reg, htAdhoc.reg, 9485BTcoex.reg, customer2GreenTx.reg, paprdenable.reg, cemspecled_func2_6.reg, wowenable.reg
DelReg          = atheros.DelReg
CopyFiles       = atheros.CopyFiles
*IfType         = 71        ; IF_TYPE_IEEE80211
*MediaType      = 16        ; NdisMediumNative802_11
*PhysicalMediaType = 9      ; NdisPhysicalMediumNative802_11
Include         = netvwifibus.inf, machine.inf
Needs           = VWiFiBus.CopyFiles

[ATHR_DEV_OS61_209C1A3B.ndi.NTamd64.Services]
AddService = athr, 2, atheros.Service, atheros.EventLog
Include    = netvwifibus.inf
Needs      = VWiFiBus.Services

[ATHR_DEV_OS61_209C1A3B.ndi.NTamd64.HW]
Include = netvwifibus.inf
Needs   = PciASPMOptIn, VWiFiBus.PnPFilterRegistration

; 20861A3B
[ATHR_DEV_OS61_20861A3B.ndi.NTamd64]
Characteristics = 0x84
BusType         = 5
AddReg          = atheros_os61.reg, atheros11n.reg, htAdhoc.reg, 9485BTcoexDivEn.reg, customer2GreenTx.reg, paprdenable.reg, cemspecled_func2_6.reg, 9485LnaDivUseBtAntEnable.reg, CUS198_xLnaGpioCfg.reg, antCtrlComm2gSwitchEnable.reg, rateCtrlTxFastDrop.reg, IdleConfiguration.reg, bt30_high_speed.reg, ampFilter.reg
DelReg          = atheros.DelReg
CopyFiles       = atheros.CopyFiles
*IfType         = 71        ; IF_TYPE_IEEE80211
*MediaType      = 16        ; NdisMediumNative802_11
*PhysicalMediaType = 9      ; NdisPhysicalMediumNative802_11
Include         = netvwifibus.inf, machine.inf
Needs           = VWiFiBus.CopyFiles

[ATHR_DEV_OS61_20861A3B.ndi.NTamd64.Services]
AddService = athr, 2, atheros.Service, atheros.EventLog
Include    = netvwifibus.inf
Needs      = VWiFiBus.Services

[ATHR_DEV_OS61_20861A3B.ndi.NTamd64.HW]
Include = netvwifibus.inf
Needs   = PciASPMOptIn, VWiFiBus.PnPFilterRegistration

[ATHR_DEV_OS61_CUS198_1.ndi.NTamd64]
Characteristics = 0x84
BusType         = 5
AddReg          = atheros_os61.reg, atheros11n.reg, htAdhoc.reg, 9485BTcoexDivEn_1.reg, customer2GreenTx.reg, paprdenable.reg, customer3h.reg, 9485LnaDivUseBtAntEnable.reg, CUS198_xLnaGpioCfg.reg, antCtrlComm2gSwitchEnable.reg, rateCtrlTxFastDrop.reg, IdleConfiguration.reg
DelReg          = atheros.DelReg
CopyFiles       = atheros.CopyFiles
*IfType         = 71        ; IF_TYPE_IEEE80211
*MediaType      = 16        ; NdisMediumNative802_11
*PhysicalMediaType = 9      ; NdisPhysicalMediumNative802_11
Include         = netvwifibus.inf, machine.inf
Needs           = VWiFiBus.CopyFiles

[ATHR_DEV_OS61_CUS198_1.ndi.NTamd64.Services]
AddService = athr, 2, atheros.Service, atheros.EventLog
Include    = netvwifibus.inf
Needs      = VWiFiBus.Services

[ATHR_DEV_OS61_CUS198_1.ndi.NTamd64.HW]
Include = netvwifibus.inf
Needs   = PciASPMOptIn, VWiFiBus.PnPFilterRegistration

; 21261A3B
[ATHR_DEV_OS61_21261A3B.ndi.NTamd64]
Characteristics = 0x84
BusType         = 5
AddReg          = atheros_os61.reg, atheros11n.reg, htAdhoc.reg, 9485BTcoexDivEn_1.reg, customer2GreenTx.reg, paprdenable.reg, customer3h.reg, 9485LnaDivUseBtAntEnable.reg, CUS198_xLnaGpioCfg.reg, antCtrlComm2gSwitchEnable.reg, rateCtrlTxFastDrop.reg, IdleConfiguration.reg, bt30_high_speed.reg
DelReg          = atheros.DelReg
CopyFiles       = atheros.CopyFiles
*IfType         = 71        ; IF_TYPE_IEEE80211
*MediaType      = 16        ; NdisMediumNative802_11
*PhysicalMediaType = 9      ; NdisPhysicalMediumNative802_11
Include         = netvwifibus.inf, machine.inf
Needs           = VWiFiBus.CopyFiles

[ATHR_DEV_OS61_21261A3B.ndi.NTamd64.Services]
AddService = athr, 2, atheros.Service, atheros.EventLog
Include    = netvwifibus.inf
Needs      = VWiFiBus.Services

[ATHR_DEV_OS61_21261A3B.ndi.NTamd64.HW]
Include = netvwifibus.inf
Needs   = PciASPMOptIn, VWiFiBus.PnPFilterRegistration

[ATHR_DEV_OS61_CUS198_2.ndi.NTamd64]
Characteristics = 0x84
BusType         = 5
AddReg          = atheros_os61.reg, atheros11n.reg, htAdhoc.reg, 9485BTcoexDivEn_1.reg, customer2GreenTx.reg, paprdenable.reg, customer3h.reg, 9485LnaDivUseBtAntEnable.reg, CUS198_xLnaGpioCfg.reg, antCtrlComm2gSwitchEnable.reg, rateCtrlTxFastDrop.reg, IdleConfiguration.reg, wowenable.reg, bt30_high_speed.reg
DelReg          = atheros.DelReg
CopyFiles       = atheros.CopyFiles
*IfType         = 71        ; IF_TYPE_IEEE80211
*MediaType      = 16        ; NdisMediumNative802_11
*PhysicalMediaType = 9      ; NdisPhysicalMediumNative802_11
Include         = netvwifibus.inf, machine.inf
Needs           = VWiFiBus.CopyFiles

[ATHR_DEV_OS61_CUS198_2.ndi.NTamd64.Services]
AddService = athr, 2, atheros.Service, atheros.EventLog
Include    = netvwifibus.inf
Needs      = VWiFiBus.Services

[ATHR_DEV_OS61_CUS198_2.ndi.NTamd64.HW]
Include = netvwifibus.inf
Needs   = PciASPMOptIn, VWiFiBus.PnPFilterRegistration

[ATHR_DEV_OS61_11861A3B.ndi.NTamd64]
Characteristics = 0x84
BusType         = 5
AddReg          = atheros_os61.reg, atheros11n.reg, htAdhoc.reg, customer2GreenTx.reg, paprdenable.reg, cemspecled_func2_6.reg
DelReg          = atheros.DelReg
CopyFiles       = atheros.CopyFiles
*IfType         = 71        ; IF_TYPE_IEEE80211
*MediaType      = 16        ; NdisMediumNative802_11
*PhysicalMediaType = 9      ; NdisPhysicalMediumNative802_11
Include         = netvwifibus.inf, machine.inf
Needs           = VWiFiBus.CopyFiles

[ATHR_DEV_OS61_11861A3B.ndi.NTamd64.Services]
AddService = athr, 2, atheros.Service, atheros.EventLog
Include    = netvwifibus.inf
Needs      = VWiFiBus.Services

[ATHR_DEV_OS61_11861A3B.ndi.NTamd64.HW]
Include = netvwifibus.inf
Needs   = PciASPMOptIn, VWiFiBus.PnPFilterRegistration

[ATHR_DEV_OS61_11861A3B_1.ndi.NTamd64]
Characteristics = 0x84
BusType         = 5
AddReg          = atheros_os61.reg, atheros11n.reg, htAdhoc.reg, customer2GreenTx.reg, paprdenable.reg, cemspecled_func2_6.reg
DelReg          = atheros.DelReg
CopyFiles       = atheros.CopyFiles
*IfType         = 71        ; IF_TYPE_IEEE80211
*MediaType      = 16        ; NdisMediumNative802_11
*PhysicalMediaType = 9      ; NdisPhysicalMediumNative802_11
Include         = netvwifibus.inf, machine.inf
Needs           = VWiFiBus.CopyFiles

[ATHR_DEV_OS61_11861A3B_1.ndi.NTamd64.Services]
AddService = athr, 2, atheros.Service, atheros.EventLog
Include    = netvwifibus.inf
Needs      = VWiFiBus.Services

[ATHR_DEV_OS61_11861A3B_1.ndi.NTamd64.HW]
Include = netvwifibus.inf
Needs   = PciASPMOptIn, VWiFiBus.PnPFilterRegistration

[ATHR_DEV_OS61_118C1A3B1.ndi.NTamd64]
Characteristics = 0x84
BusType         = 5
AddReg          = atheros_os61.reg, atheros11n.reg, htAdhoc.reg, customer2GreenTx.reg, paprdenable.reg, cemspecled_func2_6.reg, wowenable.reg, customer1roamPolicy.reg, wirelessmodeselectkite.reg
DelReg          = atheros.DelReg
CopyFiles       = atheros.CopyFiles
*IfType         = 71        ; IF_TYPE_IEEE80211
*MediaType      = 16        ; NdisMediumNative802_11
*PhysicalMediaType = 9      ; NdisPhysicalMediumNative802_11
Include         = netvwifibus.inf, machine.inf
Needs           = VWiFiBus.CopyFiles

[ATHR_DEV_OS61_118C1A3B1.ndi.NTamd64.Services]
AddService = athr, 2, atheros.Service, atheros.EventLog
Include    = netvwifibus.inf
Needs      = VWiFiBus.Services

[ATHR_DEV_OS61_118C1A3B1.ndi.NTamd64.HW]
Include = netvwifibus.inf
Needs   = VWiFiBus.PnPFilterRegistration

[ATHR_DEV_OS61_850D1043.ndi.NTamd64]
Characteristics = 0x84
BusType         = 5
AddReg          = atheros_os61.reg, atheros11n.reg, htAdhoc.reg, customer2GreenTx.reg, paprdenable.reg, cemspecled_func2_6.reg, S5wow.reg
DelReg          = atheros.DelReg
CopyFiles       = atheros.CopyFiles
*IfType         = 71        ; IF_TYPE_IEEE80211
*MediaType      = 16        ; NdisMediumNative802_11
*PhysicalMediaType = 9      ; NdisPhysicalMediumNative802_11
Include         = netvwifibus.inf, machine.inf
Needs           = VWiFiBus.CopyFiles

[ATHR_DEV_OS61_850D1043.ndi.NTamd64.Services]
AddService = athr, 2, atheros.Service, atheros.EventLog
Include    = netvwifibus.inf
Needs      = VWiFiBus.Services

[ATHR_DEV_OS61_850D1043.ndi.NTamd64.HW]
Include = netvwifibus.inf
Needs   = PciASPMOptIn, VWiFiBus.PnPFilterRegistration

[ATHR_DEV_OS61_E006105B.ndi.NTamd64]
Characteristics = 0x84
BusType         = 5
AddReg          = atheros_os61.reg, atheros11n.reg, customer3c.reg, smpsDynamic.reg, htAdhoc.reg, roamPolicy2.reg
DelReg          = atheros.DelReg
CopyFiles       = atheros.CopyFiles
*IfType         = 71            ; IF_TYPE_IEEE80211
*MediaType      = 16            ; NdisMediumNative802_11
*PhysicalMediaType = 9          ; NdisPhysicalMediumNative802_11
Include         = netvwifibus.inf, machine.inf
Needs           = VWiFiBus.CopyFiles

[ATHR_DEV_OS61_E006105B.ndi.NTamd64.Services]
AddService = athr, 2, atheros.Service, atheros.EventLog
Include    = netvwifibus.inf
Needs      = VWiFiBus.Services

[ATHR_DEV_OS61_E006105B.ndi.NTamd64.HW]
Include = netvwifibus.inf
Needs   = VWiFiBus.PnPFilterRegistration

[ATHR_DEV_OS61_655211AD.ndi.NTamd64]
Characteristics = 0x84
BusType         = 5
AddReg          = atheros_os61.reg, atheros11n.reg, customer3c.reg, smpsDynamic.reg, htAdhoc.reg, 5416.bandselect.reg, roamPolicy2.reg
DelReg          = atheros.DelReg
CopyFiles       = atheros.CopyFiles
*IfType         = 71            ; IF_TYPE_IEEE80211
*MediaType      = 16            ; NdisMediumNative802_11
*PhysicalMediaType = 9          ; NdisPhysicalMediumNative802_11
Include         = netvwifibus.inf, machine.inf
Needs           = VWiFiBus.CopyFiles

[ATHR_DEV_OS61_655211AD.ndi.NTamd64.Services]
AddService = athr, 2, atheros.Service, atheros.EventLog
Include    = netvwifibus.inf
Needs      = VWiFiBus.Services

[ATHR_DEV_OS61_655211AD.ndi.NTamd64.HW]
Include = netvwifibus.inf
Needs   = VWiFiBus.PnPFilterRegistration

[ATHR_DEV_OS61_661711AD.ndi.NTamd64]
Characteristics = 0x84
BusType         = 5
AddReg          = atheros_os61.reg, atheros11n.reg, htAdhoc.reg, paprdenable.reg, customer3g.reg, maxpowersave.reg, serializing.reg, roamPolicy2.reg, customer1GreenTx.reg, wowenable.reg
DelReg          = atheros.DelReg
CopyFiles       = atheros.CopyFiles
*IfType         = 71        ; IF_TYPE_IEEE80211
*MediaType      = 16        ; NdisMediumNative802_11
*PhysicalMediaType = 9      ; NdisPhysicalMediumNative802_11
Include         = netvwifibus.inf, machine.inf
Needs           = VWiFiBus.CopyFiles

[ATHR_DEV_OS61_661711AD.ndi.NTamd64.Services]
AddService = athr, 2, atheros.Service, atheros.EventLog
Include    = netvwifibus.inf
Needs      = VWiFiBus.Services

[ATHR_DEV_OS61_661711AD.ndi.NTamd64.HW]
Include = netvwifibus.inf
Needs   = PciASPMOptIn, VWiFiBus.PnPFilterRegistration

;add by alan liu for liteon PCIE 1.1
[ATHR_DEV_OS61_661711ADPCIE_1_1.ndi.NTamd64]
Characteristics = 0x84
BusType         = 5
AddReg          = atheros_os61.reg, atheros11n.reg, htAdhoc.reg, paprdenable.reg, customer3gpcie11.reg, maxpowersave.reg, serializing.reg, roamPolicy2.reg, customer1GreenTx.reg, wowenable.reg
DelReg          = atheros.DelReg
CopyFiles       = atheros.CopyFiles
*IfType         = 71        ; IF_TYPE_IEEE80211
*MediaType      = 16        ; NdisMediumNative802_11
*PhysicalMediaType = 9      ; NdisPhysicalMediumNative802_11
Include         = netvwifibus.inf, machine.inf
Needs           = VWiFiBus.CopyFiles

[ATHR_DEV_OS61_661711ADPCIE_1_1.ndi.NTamd64.Services]
AddService = athr, 2, atheros.Service, atheros.EventLog
Include    = netvwifibus.inf
Needs      = VWiFiBus.Services

[ATHR_DEV_OS61_661711ADPCIE_1_1.ndi.NTamd64.HW]
Include = netvwifibus.inf
Needs   = PciASPMOptIn, VWiFiBus.PnPFilterRegistration

;----------------------------------------------------------------------------------------------------

[ATHR_DEV_OS61_E04A105B.ndi.NTamd64]
Characteristics = 0x84
BusType         = 5
AddReg          = atheros_os61.reg, atheros11n.reg, smpsDynamic.reg, htAdhoc.reg, cemspecled_func2_10.reg, serializing.reg, maxpowersave.reg, roamPolicy2.reg, customer1GreenTx.reg
DelReg          = atheros.DelReg
CopyFiles       = atheros.CopyFiles
*IfType         = 71        ; IF_TYPE_IEEE80211
*MediaType      = 16        ; NdisMediumNative802_11
*PhysicalMediaType = 9      ; NdisPhysicalMediumNative802_11
Include         = netvwifibus.inf, machine.inf
Needs           = VWiFiBus.CopyFiles

[ATHR_DEV_OS61_E04A105B.ndi.NTamd64.Services]
AddService = athr, 2, atheros.Service, atheros.EventLog
Include    = netvwifibus.inf
Needs      = VWiFiBus.Services

[ATHR_DEV_OS61_E04A105B.ndi.NTamd64.HW]
AddReg  = MSI.reg
Include = netvwifibus.inf
Needs   = PciASPMOptIn, VWiFiBus.PnPFilterRegistration

[ATHR_DEV_OS61_E01F105B.ndi.NTamd64]
Characteristics = 0x84
BusType         = 5
AddReg          = atheros_os61.reg, atheros11n.reg, customer3c.reg, smpsDynamic.reg, htAdhoc.reg, maxpowersave.reg, serializing.reg, d3forcel1disable1.reg, cmdRegister.reg, amp.reg, ampFilter.reg, c3war.reg, roamPolicy2.reg
DelReg          = atheros.DelReg
CopyFiles       = atheros.CopyFiles
*IfType         = 71            ; IF_TYPE_IEEE80211
*MediaType      = 16            ; NdisMediumNative802_11
*PhysicalMediaType = 9          ; NdisPhysicalMediumNative802_11
Include         = netvwifibus.inf, machine.inf
Needs           = VWiFiBus.CopyFiles

[ATHR_DEV_OS61_E01F105B.ndi.NTamd64.Services]
AddService = athr, 2, atheros.Service, atheros.EventLog
Include    = netvwifibus.inf
Needs      = VWiFiBus.Services

[ATHR_DEV_OS61_E01F105B.ndi.NTamd64.HW]
Include = netvwifibus.inf
Needs   = VWiFiBus.PnPFilterRegistration

[ATHR_DEV_OS61_664211AD.ndi.NTamd64]
Characteristics = 0x84
BusType         = 5
AddReg          = atheros_os61.reg, atheros11n.reg, customer3c.reg, smpsDynamic.reg, maxpowersave.reg, serializing.reg, d3forcel1disable1.reg, cmdRegister.reg, amp.reg, ampFilter.reg, roamPolicy2.reg
DelReg          = atheros.DelReg
CopyFiles       = atheros.CopyFiles
*IfType         = 71            ; IF_TYPE_IEEE80211
*MediaType      = 16            ; NdisMediumNative802_11
*PhysicalMediaType = 9          ; NdisPhysicalMediumNative802_11
Include         = netvwifibus.inf, machine.inf
Needs           = VWiFiBus.CopyFiles

[ATHR_DEV_OS61_664211AD.ndi.NTamd64.Services]
AddService = athr, 2, atheros.Service, atheros.EventLog
Include    = netvwifibus.inf
Needs      = VWiFiBus.Services

[ATHR_DEV_OS61_664211AD.ndi.NTamd64.HW]
Include = netvwifibus.inf
Needs   = VWiFiBus.PnPFilterRegistration

[ATHR_DEV_OS61_663111AD.ndi.NTamd64]
Characteristics = 0x84
BusType         = 5
AddReg          = atheros_os61.reg, atheros11n.reg, customer3c.reg, smpsDynamic.reg, htAdhoc.reg, maxpowersave.reg, serializing.reg, triggerlevelkiteonly.reg, c3war.reg
DelReg          = atheros.DelReg
CopyFiles       = atheros.CopyFiles
*IfType         = 71            ; IF_TYPE_IEEE80211
*MediaType      = 16            ; NdisMediumNative802_11
*PhysicalMediaType = 9          ; NdisPhysicalMediumNative802_11
Include         = netvwifibus.inf, machine.inf
Needs           = VWiFiBus.CopyFiles

[ATHR_DEV_OS61_663111AD.ndi.NTamd64.Services]
AddService = athr, 2, atheros.Service, atheros.EventLog
Include    = netvwifibus.inf
Needs      = VWiFiBus.Services

[ATHR_DEV_OS61_663111AD.ndi.NTamd64.HW]
Include = netvwifibus.inf
Needs   = VWiFiBus.PnPFilterRegistration

[ATHR_DEV_OS61_E016105B.ndi.NTamd64]
Characteristics = 0x84
BusType         = 5
AddReg          = atheros_os61.reg, atheros11n.reg, customer3c.reg, htAdhoc.reg, maxpowersave.reg, serializing.reg, triggerlevelkiteonly.reg, c3war.reg, cmdRegister.reg, amp.reg, ampFilter.reg, roamPolicy2.reg, customer1GreenTx.reg
DelReg          = atheros.DelReg
CopyFiles       = atheros.CopyFiles
*IfType         = 71            ; IF_TYPE_IEEE80211
*MediaType      = 16            ; NdisMediumNative802_11
*PhysicalMediaType = 9          ; NdisPhysicalMediumNative802_11
Include         = netvwifibus.inf, machine.inf
Needs           = VWiFiBus.CopyFiles

[ATHR_DEV_OS61_E016105B.ndi.NTamd64.Services]
AddService = athr, 2, atheros.Service, atheros.EventLog
Include    = netvwifibus.inf
Needs      = VWiFiBus.Services

[ATHR_DEV_OS61_E016105B.ndi.NTamd64.HW]
Include = netvwifibus.inf
Needs   = VWiFiBus.PnPFilterRegistration

[ATHR_DEV_OS61_E035105B.ndi.NTamd64]
Characteristics = 0x84
BusType         = 5
AddReg          = atheros_os61.reg, atheros11n.reg, customer3c.reg, maxpowersave.reg, serializing.reg, cmdRegister.reg, amp.reg, ampFilter.reg, triggerlevelkiteonly.reg, c3war.reg, roamPolicy2.reg, customer1GreenTx.reg
DelReg          = atheros.DelReg
CopyFiles       = atheros.CopyFiles
*IfType         = 71            ; IF_TYPE_IEEE80211
*MediaType      = 16            ; NdisMediumNative802_11
*PhysicalMediaType = 9          ; NdisPhysicalMediumNative802_11
Include         = netvwifibus.inf, machine.inf
Needs           = VWiFiBus.CopyFiles

[ATHR_DEV_OS61_E035105B.ndi.NTamd64.Services]
AddService = athr, 2, atheros.Service, atheros.EventLog
Include    = netvwifibus.inf
Needs      = VWiFiBus.Services

[ATHR_DEV_OS61_E035105B.ndi.NTamd64.HW]
Include = netvwifibus.inf
Needs   = VWiFiBus.PnPFilterRegistration

[ATHR_DEV_OS61_E031105Bw.ndi.NTamd64]
Characteristics = 0x84
BusType         = 5
AddReg          = atheros_os61.reg, atheros11n.reg, customer3c.reg, htAdhoc.reg, maxpowersave.reg, serializing.reg, janusda.reg, triggerlevelkiteonly.reg, c3war.reg, amp.reg, ampFilter.reg, roamPolicy2.reg, customer1GreenTx.reg, wirelessmode.2g.reg
DelReg          = atheros.DelReg
CopyFiles       = atheros.CopyFiles
*IfType         = 71            ; IF_TYPE_IEEE80211
*MediaType      = 16            ; NdisMediumNative802_11
*PhysicalMediaType = 9          ; NdisPhysicalMediumNative802_11
Include         = netvwifibus.inf, machine.inf
Needs           = VWiFiBus.CopyFiles

[ATHR_DEV_OS61_E031105Bw.ndi.NTamd64.Services]
AddService = athr, 2, atheros.Service, atheros.EventLog
Include    = netvwifibus.inf
Needs      = VWiFiBus.Services

[ATHR_DEV_OS61_E031105Bw.ndi.NTamd64.HW]
Include = netvwifibus.inf
Needs   = VWiFiBus.PnPFilterRegistration

[ATHR_DEV_OS61_1013.ndi.NTamd64]
Characteristics = 0x84
BusType         = 5
AddReg          = atheros_os61.reg, atheros.reg, customer0LED.reg, customer0.reg, roamthreshA.reg, ignore11d.reg
DelReg          = atheros.DelReg
CopyFiles       = atheros.CopyFiles
*IfType         = 71        ; IF_TYPE_IEEE80211
*MediaType      = 16        ; NdisMediumNative802_11
*PhysicalMediaType = 9      ; NdisPhysicalMediumNative802_11
Include         = netvwifibus.inf, machine.inf
Needs           = VWiFiBus.CopyFiles

[ATHR_DEV_OS61_1013.ndi.NTamd64.Services]
AddService = athr, 2, atheros.Service, atheros.EventLog
Include    = netvwifibus.inf
Needs      = VWiFiBus.Services

[ATHR_DEV_OS61_1013.ndi.NTamd64.HW]
Include = netvwifibus.inf
Needs   = VWiFiBus.PnPFilterRegistration

[ATHR_DEV_OS61_2013.ndi.NTamd64]
Characteristics = 0x84
BusType         = 5
AddReg          = atheros_os61.reg, atheros.reg, customer0LED.reg, customer0.reg, roamthreshA.reg, ignore11d.reg, bandselect.reg
DelReg          = atheros.DelReg
CopyFiles       = atheros.CopyFiles
*IfType         = 71        ; IF_TYPE_IEEE80211
*MediaType      = 16        ; NdisMediumNative802_11
*PhysicalMediaType = 9      ; NdisPhysicalMediumNative802_11
Include         = netvwifibus.inf, machine.inf
Needs           = VWiFiBus.CopyFiles

[ATHR_DEV_OS61_2013.ndi.NTamd64.Services]
AddService = athr, 2, atheros.Service, atheros.EventLog
Include    = netvwifibus.inf
Needs      = VWiFiBus.Services

[ATHR_DEV_OS61_2013.ndi.NTamd64.HW]
Include = netvwifibus.inf
Needs   = VWiFiBus.PnPFilterRegistration

[ATHR_DEV_OS61_3013.ndi.NTamd64]
Characteristics = 0x84
BusType         = 5
AddReg          = atheros_os61.reg, atheros.reg, customer0LED1.reg, customer0.reg, roamthreshA.reg, ignore11d.reg
DelReg          = atheros.DelReg
CopyFiles       = atheros.CopyFiles
*IfType         = 71        ; IF_TYPE_IEEE80211
*MediaType      = 16        ; NdisMediumNative802_11
*PhysicalMediaType = 9      ; NdisPhysicalMediumNative802_11
Include         = netvwifibus.inf, machine.inf
Needs           = VWiFiBus.CopyFiles

[ATHR_DEV_OS61_3013.ndi.NTamd64.Services]
AddService = athr, 2, atheros.Service, atheros.EventLog
Include    = netvwifibus.inf
Needs      = VWiFiBus.Services

[ATHR_DEV_OS61_3013.ndi.NTamd64.HW]
Include = netvwifibus.inf
Needs   = VWiFiBus.PnPFilterRegistration

[ATHR_DEV_OS61_4013.ndi.NTamd64]
Characteristics = 0x84
BusType         = 5
AddReg          = atheros_os61.reg, atheros.reg, customer0LED1.reg, customer0.reg, roamthreshA.reg, ignore11d.reg, bandselect.reg
DelReg          = atheros.DelReg
CopyFiles       = atheros.CopyFiles
*IfType         = 71        ; IF_TYPE_IEEE80211
*MediaType      = 16        ; NdisMediumNative802_11
*PhysicalMediaType = 9      ; NdisPhysicalMediumNative802_11
Include         = netvwifibus.inf, machine.inf
Needs           = VWiFiBus.CopyFiles

[ATHR_DEV_OS61_4013.ndi.NTamd64.Services]
AddService = athr, 2, atheros.Service, atheros.EventLog
Include    = netvwifibus.inf
Needs      = VWiFiBus.Services

[ATHR_DEV_OS61_4013.ndi.NTamd64.HW]
Include = netvwifibus.inf
Needs   = VWiFiBus.PnPFilterRegistration

[ATHR_DEV_OS61_5013.ndi.NTamd64]
Characteristics = 0x84
BusType         = 5
AddReg          = atheros_os61.reg, atheros.reg, customer0LED2.reg, customer0.reg, roamthreshA.reg, ignore11d.reg
DelReg          = atheros.DelReg
CopyFiles       = atheros.CopyFiles
*IfType         = 71        ; IF_TYPE_IEEE80211
*MediaType      = 16        ; NdisMediumNative802_11
*PhysicalMediaType = 9      ; NdisPhysicalMediumNative802_11
Include         = netvwifibus.inf, machine.inf
Needs           = VWiFiBus.CopyFiles

[ATHR_DEV_OS61_5013.ndi.NTamd64.Services]
AddService = athr, 2, atheros.Service, atheros.EventLog
Include    = netvwifibus.inf
Needs      = VWiFiBus.Services

[ATHR_DEV_OS61_5013.ndi.NTamd64.HW]
Include = netvwifibus.inf
Needs   = VWiFiBus.PnPFilterRegistration

[ATHR_DEV_OS61_6013.ndi.NTamd64]
Characteristics = 0x84
BusType         = 5
AddReg          = atheros_os61.reg, atheros.reg, customer0LED2.reg, customer0.reg, roamthreshA.reg, ignore11d.reg, d3hot.reg
DelReg          = atheros.DelReg
CopyFiles       = atheros.CopyFiles
*IfType         = 71        ; IF_TYPE_IEEE80211
*MediaType      = 16        ; NdisMediumNative802_11
*PhysicalMediaType = 9      ; NdisPhysicalMediumNative802_11
Include         = netvwifibus.inf, machine.inf
Needs           = VWiFiBus.CopyFiles

[ATHR_DEV_OS61_6013.ndi.NTamd64.Services]
AddService = athr, 2, atheros.Service, atheros.EventLog
Include    = netvwifibus.inf
Needs      = VWiFiBus.Services

[ATHR_DEV_OS61_6013.ndi.NTamd64.HW]
Include = netvwifibus.inf
Needs   = VWiFiBus.PnPFilterRegistration

[ATHR_DEV_OS61_0036.ndi.NTamd64]
Characteristics = 0x84
BusType         = 5
AddReg          = atheros_os61.reg, atheros11n.reg, customer0LED1.reg, customer0_HB93.reg, roamthreshA.reg, ignore11d.reg, smpsDynamic.reg, htAdhoc.reg
DelReg          = atheros.DelReg
CopyFiles       = atheros.CopyFiles
*IfType         = 71        ; IF_TYPE_IEEE80211
*MediaType      = 16        ; NdisMediumNative802_11
*PhysicalMediaType = 9      ; NdisPhysicalMediumNative802_11
Include         = netvwifibus.inf, machine.inf
Needs           = VWiFiBus.CopyFiles

[ATHR_DEV_OS61_0036.ndi.NTamd64.Services]
AddService = athr, 2, atheros.Service, atheros.EventLog
Include    = netvwifibus.inf
Needs      = VWiFiBus.Services

[ATHR_DEV_OS61_0036.ndi.NTamd64.HW]
Include = netvwifibus.inf
Needs   = VWiFiBus.PnPFilterRegistration

[ATHR_DEV_OS61_0037.ndi.NTamd64]
Characteristics = 0x84
BusType         = 5
AddReg          = atheros_os61.reg, atheros11n.reg, customer0LED1.reg, customer0_HB95.reg, roamthreshA.reg, ignore11d.reg, htAdhoc.reg, triggerlevelkiteonly.reg, c3war.reg
DelReg          = atheros.DelReg
CopyFiles       = atheros.CopyFiles
*IfType         = 71        ; IF_TYPE_IEEE80211
*MediaType      = 16        ; NdisMediumNative802_11
*PhysicalMediaType = 9      ; NdisPhysicalMediumNative802_11
Include         = netvwifibus.inf, machine.inf
Needs           = VWiFiBus.CopyFiles

[ATHR_DEV_OS61_0037.ndi.NTamd64.Services]
AddService = athr, 2, atheros.Service, atheros.EventLog
Include    = netvwifibus.inf
Needs      = VWiFiBus.Services

[ATHR_DEV_OS61_0037.ndi.NTamd64.HW]
Include = netvwifibus.inf
Needs   = VWiFiBus.PnPFilterRegistration

[ATHR_DEV_OS61_F013.ndi.NTamd64]
Characteristics = 0x84
BusType         = 5
AddReg          = atheros_os61.reg, atheros.reg, customer1ani.reg, bandselect.reg, adhocchannelselect.reg, enableswretry, customer1roamPolicy.reg
DelReg          = atheros.DelReg
CopyFiles       = atheros.CopyFiles
*IfType         = 71        ; IF_TYPE_IEEE80211
*MediaType      = 16        ; NdisMediumNative802_11
*PhysicalMediaType = 9      ; NdisPhysicalMediumNative802_11
Include         = netvwifibus.inf, machine.inf
Needs           = VWiFiBus.CopyFiles

[ATHR_DEV_OS61_F013.ndi.NTamd64.Services]
AddService = athr, 2, atheros.Service, atheros.EventLog
Include    = netvwifibus.inf
Needs      = VWiFiBus.Services

[ATHR_DEV_OS61_F013.ndi.NTamd64.HW]
Include = netvwifibus.inf
Needs   = VWiFiBus.PnPFilterRegistration

[ATHR_DEV_OS61_F013C.ndi.NTamd64]
Characteristics = 0x84
BusType         = 5
AddReg          = atheros_os61.reg, atheros.reg, customer1ani.reg, bandselect.reg, adhocchannelselect.reg, enableswretry, customer1roamPolicy.reg, minpower.reg
DelReg          = atheros.DelReg
CopyFiles       = atheros.CopyFiles
*IfType         = 71        ; IF_TYPE_IEEE80211
*MediaType      = 16        ; NdisMediumNative802_11
*PhysicalMediaType = 9      ; NdisPhysicalMediumNative802_11
Include         = netvwifibus.inf, machine.inf
Needs           = VWiFiBus.CopyFiles

[ATHR_DEV_OS61_F013C.ndi.NTamd64.Services]
AddService = athr, 2, atheros.Service, atheros.EventLog
Include    = netvwifibus.inf
Needs      = VWiFiBus.Services

[ATHR_DEV_OS61_F013C.ndi.NTamd64.HW]
Include = netvwifibus.inf
Needs   = VWiFiBus.PnPFilterRegistration

[ATHR_DEV_OS61_F01C.ndi.NTamd64]
Characteristics = 0x84
BusType         = 5
AddReg          = atheros_os61.reg, atheros.reg, customer1ani.reg, adhocchannelselect.reg, enableswretry, customer1roamPolicy.reg
DelReg          = atheros.DelReg
CopyFiles       = atheros.CopyFiles
*IfType         = 71        ; IF_TYPE_IEEE80211
*MediaType      = 16        ; NdisMediumNative802_11
*PhysicalMediaType = 9      ; NdisPhysicalMediumNative802_11
Include         = netvwifibus.inf, machine.inf
Needs           = VWiFiBus.CopyFiles

[ATHR_DEV_OS61_F01C.ndi.NTamd64.Services]
AddService = athr, 2, atheros.Service, atheros.EventLog
Include    = netvwifibus.inf
Needs      = VWiFiBus.Services

[ATHR_DEV_OS61_F01C.ndi.NTamd64.HW]
Include = netvwifibus.inf
Needs   = VWiFiBus.PnPFilterRegistration

[ATHR_DEV_OS61_04221468.ndi.NTamd64]
Characteristics = 0x84
BusType         = 5
AddReg          = atheros_os61.reg, atheros.reg, customer3.reg
DelReg          = atheros.DelReg
CopyFiles       = atheros.CopyFiles
*IfType         = 71        ; IF_TYPE_IEEE80211
*MediaType      = 16        ; NdisMediumNative802_11
*PhysicalMediaType = 9      ; NdisPhysicalMediumNative802_11
Include         = netvwifibus.inf, machine.inf
Needs           = VWiFiBus.CopyFiles

[ATHR_DEV_OS61_04221468.ndi.NTamd64.Services]
AddService = athr, 2, atheros.Service, atheros.EventLog
Include    = netvwifibus.inf
Needs      = VWiFiBus.Services

[ATHR_DEV_OS61_04221468.ndi.NTamd64.HW]
Include = netvwifibus.inf
Needs   = VWiFiBus.PnPFilterRegistration

[ATHR_DEV_OS61_E000105B.ndi.NTamd64]
Characteristics = 0x84
BusType         = 5
AddReg          = atheros_os61.reg, atheros.reg, customer4b.reg, customer4a_ASPM.reg, d3hot.reg
DelReg          = atheros.DelReg
CopyFiles       = atheros.CopyFiles
*IfType         = 71        ; IF_TYPE_IEEE80211
*MediaType      = 16        ; NdisMediumNative802_11
*PhysicalMediaType = 9      ; NdisPhysicalMediumNative802_11
Include         = netvwifibus.inf, machine.inf
Needs           = VWiFiBus.CopyFiles, PciASPMOptIn

[ATHR_DEV_OS61_E000105B.ndi.NTamd64.Services]
AddService = athr, 2, atheros.Service, atheros.EventLog
Include    = netvwifibus.inf
Needs      = VWiFiBus.Services

[ATHR_DEV_OS61_E000105B.ndi.NTamd64.HW]
Include = netvwifibus.inf
Needs   = VWiFiBus.PnPFilterRegistration

[ATHR_DEV_OS61_E002105B.ndi.NTamd64]
Characteristics = 0x84
BusType         = 5
AddReg          = atheros_os61.reg, atheros.reg, customer4b.reg, customer4a_ASPM.reg, d3hot.reg
DelReg          = atheros.DelReg
CopyFiles       = atheros.CopyFiles
*IfType         = 71        ; IF_TYPE_IEEE80211
*MediaType      = 16        ; NdisMediumNative802_11
*PhysicalMediaType = 9      ; NdisPhysicalMediumNative802_11
Include         = netvwifibus.inf, machine.inf
Needs           = VWiFiBus.CopyFiles, PciASPMOptIn

[ATHR_DEV_OS61_E002105B.ndi.NTamd64.Services]
AddService = athr, 2, atheros.Service, atheros.EventLog
Include    = netvwifibus.inf
Needs      = VWiFiBus.Services

[ATHR_DEV_OS61_E002105B.ndi.NTamd64.HW]
Include = netvwifibus.inf
Needs   = VWiFiBus.PnPFilterRegistration

[ATHR_DEV_OS61_04281468.ndi.NTamd64]
Characteristics = 0x84
BusType         = 5
AddReg          = atheros_os61.reg, atheros.reg, customer3e.reg, interruptpolling.reg, customer3_legacybgwmode.reg, adhocchannelselect.reg, d3hot.reg, roamPolicy2.reg
DelReg          = atheros.DelReg
CopyFiles       = atheros.CopyFiles
*IfType         = 71        ; IF_TYPE_IEEE80211
*MediaType      = 16        ; NdisMediumNative802_11
*PhysicalMediaType = 9      ; NdisPhysicalMediumNative802_11
Include         = netvwifibus.inf, machine.inf
Needs           = VWiFiBus.CopyFiles

[ATHR_DEV_OS61_04281468.ndi.NTamd64.Services]
AddService = athr, 2, atheros.Service, atheros.EventLog
Include    = netvwifibus.inf
Needs      = VWiFiBus.Services

[ATHR_DEV_OS61_04281468.ndi.NTamd64.HW]
Include = netvwifibus.inf
Needs   = VWiFiBus.PnPFilterRegistration

[ATHR_DEV_OS61_01051A32.ndi.NTamd64]
Characteristics = 0x84
BusType         = 5
AddReg          = atheros_os61.reg, atheros.reg, customer3a.reg, d3hot.reg
DelReg          = atheros.DelReg
CopyFiles       = atheros.CopyFiles
*IfType         = 71        ; IF_TYPE_IEEE80211
*MediaType      = 16        ; NdisMediumNative802_11
*PhysicalMediaType = 9      ; NdisPhysicalMediumNative802_11
Include         = netvwifibus.inf, machine.inf
Needs           = VWiFiBus.CopyFiles

[ATHR_DEV_OS61_01051A32.ndi.NTamd64.Services]
AddService = athr, 2, atheros.Service, atheros.EventLog
Include    = netvwifibus.inf
Needs      = VWiFiBus.Services

[ATHR_DEV_OS61_01051A32.ndi.NTamd64.HW]
Include = netvwifibus.inf
Needs   = VWiFiBus.PnPFilterRegistration

[ATHR_DEV_OS61_01121A32.ndi.NTamd64]
Characteristics = 0x84
BusType         = 5
AddReg          = atheros_os61.reg, atheros.reg, customer3d.reg, d3hot.reg, adhocchannelselect.reg
DelReg          = atheros.DelReg
CopyFiles       = atheros.CopyFiles
*IfType         = 71        ; IF_TYPE_IEEE80211
*MediaType      = 16        ; NdisMediumNative802_11
*PhysicalMediaType = 9      ; NdisPhysicalMediumNative802_11
Include         = netvwifibus.inf, machine.inf
Needs           = VWiFiBus.CopyFiles

[ATHR_DEV_OS61_01121A32.ndi.NTamd64.Services]
AddService = athr, 2, atheros.Service, atheros.EventLog
Include    = netvwifibus.inf
Needs      = VWiFiBus.Services

[ATHR_DEV_OS61_01121A32.ndi.NTamd64.HW]
Include = netvwifibus.inf
Needs   = VWiFiBus.PnPFilterRegistration

[ATHR_DEV_OS61_04061468.ndi.NTamd64]
Characteristics = 0x84
BusType         = 5
AddReg          = atheros_os61.reg, atheros.reg, customer4.reg
DelReg          = atheros.DelReg
CopyFiles       = atheros.CopyFiles
*IfType         = 71        ; IF_TYPE_IEEE80211
*MediaType      = 16        ; NdisMediumNative802_11
*PhysicalMediaType = 9      ; NdisPhysicalMediumNative802_11
Include         = netvwifibus.inf, machine.inf
Needs           = VWiFiBus.CopyFiles

[ATHR_DEV_OS61_04061468.ndi.NTamd64.Services]
AddService = athr, 2, atheros.Service, atheros.EventLog
Include    = netvwifibus.inf
Needs      = VWiFiBus.Services

[ATHR_DEV_OS61_04061468.ndi.NTamd64.HW]
Include = netvwifibus.inf
Needs   = VWiFiBus.PnPFilterRegistration

[ATHR_DEV_OS61_04231468.ndi.NTamd64]
Characteristics = 0x84
BusType         = 5
AddReg          = atheros_os61.reg, atheros.reg, customer4a.reg
DelReg          = atheros.DelReg
CopyFiles       = atheros.CopyFiles
*IfType         = 71        ; IF_TYPE_IEEE80211
*MediaType      = 16        ; NdisMediumNative802_11
*PhysicalMediaType = 9      ; NdisPhysicalMediumNative802_11
Include         = netvwifibus.inf, machine.inf
Needs           = VWiFiBus.CopyFiles, PciASPMOptIn

[ATHR_DEV_OS61_04231468.ndi.NTamd64.Services]
AddService = athr, 2, atheros.Service, atheros.EventLog
Include    = netvwifibus.inf
Needs      = VWiFiBus.Services

[ATHR_DEV_OS61_04231468.ndi.NTamd64.HW]
Include = netvwifibus.inf
Needs   = VWiFiBus.PnPFilterRegistration

[ATHR_DEV_OS61_E007105B.ndi.NTamd64]
Characteristics = 0x84
BusType         = 5
AddReg          = atheros_os61.reg, atheros11n.reg, customer4a.reg, customer4adhoc.reg, smpsDynamic.reg, htAdhoc.reg
DelReg          = atheros.DelReg
CopyFiles       = atheros.CopyFiles
*IfType         = 71        ; IF_TYPE_IEEE80211
*MediaType      = 16        ; NdisMediumNative802_11
*PhysicalMediaType = 9      ; NdisPhysicalMediumNative802_11
Include         = netvwifibus.inf, machine.inf
Needs           = VWiFiBus.CopyFiles, PciASPMOptIn

[ATHR_DEV_OS61_E007105B.ndi.NTamd64.Services]
AddService = athr, 2, atheros.Service, atheros.EventLog
Include    = netvwifibus.inf
Needs      = VWiFiBus.Services

[ATHR_DEV_OS61_E007105B.ndi.NTamd64.HW]
Include = netvwifibus.inf
Needs   = VWiFiBus.PnPFilterRegistration

[ATHR_DEV_OS61_S30A1.ndi.NTamd64]
Characteristics = 0x84
BusType         = 5
AddReg          = atheros_os61.reg, atheros11n.reg, htAdhoc.reg, customer4adhoc.reg, customer4a.reg, ratecap.reg, triggerlevelkiteonly.reg, c3war.reg, cmdRegister.reg, ocsEnable.reg
DelReg          = atheros.DelReg
CopyFiles       = atheros.CopyFiles
*IfType         = 71            ; IF_TYPE_IEEE80211
*MediaType      = 16            ; NdisMediumNative802_11
*PhysicalMediaType = 9          ; NdisPhysicalMediumNative802_11
Include         = netvwifibus.inf, machine.inf
Needs           = VWiFiBus.CopyFiles, PciASPMOptIn

[ATHR_DEV_OS61_S30A1.ndi.NTamd64.Services]
AddService = athr, 2, atheros.Service, atheros.EventLog
Include    = netvwifibus.inf
Needs      = VWiFiBus.Services

[ATHR_DEV_OS61_S30A1.ndi.NTamd64.HW]
Include = netvwifibus.inf
Needs   = VWiFiBus.PnPFilterRegistration

[ATHR_DEV_OS61_S30A1w.ndi.NTamd64]
Characteristics = 0x84
BusType         = 5
AddReg          = atheros_os61.reg, atheros11n.reg, htAdhoc.reg, customer4adhoc.reg, customer4a.reg, ratecap.reg, triggerlevelkiteonly.reg, c3war.reg, cmdRegister.reg, janusda.reg, amp.reg, ampFilter.reg, cemspecled_func0_6.reg, customer2GreenTx.reg, ocsEnable.reg
DelReg          = atheros.DelReg
CopyFiles       = atheros.CopyFiles
*IfType         = 71            ; IF_TYPE_IEEE80211
*MediaType      = 16            ; NdisMediumNative802_11
*PhysicalMediaType = 9          ; NdisPhysicalMediumNative802_11
Include         = netvwifibus.inf, machine.inf
Needs           = VWiFiBus.CopyFiles, PciASPMOptIn

[ATHR_DEV_OS61_S30A1w.ndi.NTamd64.Services]
AddService = athr, 2, atheros.Service, atheros.EventLog
Include    = netvwifibus.inf
Needs      = VWiFiBus.Services

[ATHR_DEV_OS61_S30A1w.ndi.NTamd64.HW]
Include = netvwifibus.inf
Needs   = VWiFiBus.PnPFilterRegistration

[ATHR_DEV_OS61_S3119.ndi.NTamd64]
Characteristics = 0x84
BusType         = 5
AddReg          = atheros_os61.reg, atheros11n.reg, htAdhoc.reg, 9485BTcoex.reg, cemspecled_func0_6.reg, customer2GreenTx.reg, customer4c.reg, customer4adhoc.reg, paprdenable.reg, amp.reg, ampFilter.reg, ocsEnable.reg
DelReg          = atheros.DelReg
CopyFiles       = atheros.CopyFiles
*IfType         = 71        ; IF_TYPE_IEEE80211
*MediaType      = 16        ; NdisMediumNative802_11
*PhysicalMediaType = 9      ; NdisPhysicalMediumNative802_11
Include         = netvwifibus.inf, machine.inf
Needs           = VWiFiBus.CopyFiles

[ATHR_DEV_OS61_S3119.ndi.NTamd64.Services]
AddService = athr, 2, atheros.Service, atheros.EventLog
Include    = netvwifibus.inf
Needs      = VWiFiBus.Services

[ATHR_DEV_OS61_S3119.ndi.NTamd64.HW]
Include = netvwifibus.inf
Needs   = PciASPMOptIn, VWiFiBus.PnPFilterRegistration

[ATHR_DEV_OS61_661811AD.ndi.NTamd64]
Characteristics = 0x84
BusType         = 5
AddReg          = atheros_os61.reg, atheros11n.reg, htAdhoc.reg, 9485BTcoex.reg, paprdenable.reg, customer3g.reg, roamPolicy2.reg, maxpowersave2.reg, AdjustRSSI.reg, wirelessmode.2g.reg
DelReg          = atheros.DelReg
CopyFiles       = atheros.CopyFiles
*IfType         = 71        ; IF_TYPE_IEEE80211
*MediaType      = 16        ; NdisMediumNative802_11
*PhysicalMediaType = 9      ; NdisPhysicalMediumNative802_11
Include         = netvwifibus.inf, machine.inf
Needs           = VWiFiBus.CopyFiles

[ATHR_DEV_OS61_661811AD.ndi.NTamd64.Services]
AddService = athr, 2, atheros.Service, atheros.EventLog
Include    = netvwifibus.inf
Needs      = VWiFiBus.Services

[ATHR_DEV_OS61_661811AD.ndi.NTamd64.HW]
Include = netvwifibus.inf
Needs   = PciASPMOptIn, VWiFiBus.PnPFilterRegistration

[ATHR_DEV_OS61_SS30A1.ndi.NTamd64]
Characteristics = 0x84
BusType         = 5
AddReg          = atheros_os61.reg, atheros11n.reg, htAdhoc.reg, customer4adhoc.reg, customer4as.reg, ratecap.reg, c3war.reg, amp.reg, ampBFilter.reg, ocsEnable.reg
DelReg          = atheros.DelReg
CopyFiles       = atheros.CopyFiles
*IfType         = 71            ; IF_TYPE_IEEE80211
*MediaType      = 16            ; NdisMediumNative802_11
*PhysicalMediaType = 9          ; NdisPhysicalMediumNative802_11
Include         = netvwifibus.inf, machine.inf
Needs           = VWiFiBus.CopyFiles, PciASPMOptIn

[ATHR_DEV_OS61_SS30A1.ndi.NTamd64.Services]
AddService = athr, 2, atheros.Service, atheros.EventLog
Include    = netvwifibus.inf
Needs      = VWiFiBus.Services

[ATHR_DEV_OS61_SS30A1.ndi.NTamd64.HW]
Include = netvwifibus.inf
Needs   = VWiFiBus.PnPFilterRegistration

[ATHR_DEV_OS61_0032168c.ndi.NTamd64]
Characteristics = 0x84
BusType         = 5
AddReg          = atheros_os61.reg, atheros11n.reg, customer0_11n.reg, 5416.antennacontrols.reg, 5416.bgnxb.reg, htAdhoc.reg
DelReg          = atheros.DelReg
CopyFiles       = atheros.CopyFiles
*IfType         = 71            ; IF_TYPE_IEEE80211
*MediaType      = 16            ; NdisMediumNative802_11
*PhysicalMediaType = 9          ; NdisPhysicalMediumNative802_11
Include         = netvwifibus.inf, machine.inf
Needs           = VWiFiBus.CopyFiles

[ATHR_DEV_OS61_0032168c.ndi.NTamd64.Services]
AddService = athr, 2, atheros.Service, atheros.EventLog
Include    = netvwifibus.inf
Needs      = VWiFiBus.Services

[ATHR_DEV_OS61_0032168c.ndi.NTamd64.HW]
Include = netvwifibus.inf
Needs   = VWiFiBus.PnPFilterRegistration

[ATHR_DEV_OS61_0033168c.ndi.NTamd64]
Characteristics = 0x84
BusType         = 5
AddReg          = atheros_os61.reg, atheros11n.reg, customer0_11n.reg, 5416.antennacontrols.reg, 5416.bandselect.reg, htAdhoc.reg
DelReg          = atheros.DelReg
CopyFiles       = atheros.CopyFiles
*IfType         = 71            ; IF_TYPE_IEEE80211
*MediaType      = 16            ; NdisMediumNative802_11
*PhysicalMediaType = 9          ; NdisPhysicalMediumNative802_11
Include         = netvwifibus.inf, machine.inf
Needs           = VWiFiBus.CopyFiles

[ATHR_DEV_OS61_0033168c.ndi.NTamd64.Services]
AddService = athr, 2, atheros.Service, atheros.EventLog
Include    = netvwifibus.inf
Needs      = VWiFiBus.Services

[ATHR_DEV_OS61_0033168c.ndi.NTamd64.HW]
Include = netvwifibus.inf
Needs   = VWiFiBus.PnPFilterRegistration

[ATHR_DEV_OS61_13C010CF.ndi.NTamd64]
Characteristics = 0x84
BusType         = 5
AddReg          = atheros_os61.reg, atheros11n.reg, 5416.bandselect.reg, 5416.antennacontrols.reg, customer1ani.reg, adhocchannelselect.reg, enableswretry, customer1roamPolicy.reg, htAdhocdisable.reg
DelReg          = atheros.DelReg
CopyFiles       = atheros.CopyFiles
*IfType         = 71            ; IF_TYPE_IEEE80211
*MediaType      = 16            ; NdisMediumNative802_11
*PhysicalMediaType = 9          ; NdisPhysicalMediumNative802_11
Include         = netvwifibus.inf, machine.inf
Needs           = VWiFiBus.CopyFiles

[ATHR_DEV_OS61_13C010CF.ndi.NTamd64.Services]
AddService = athr, 2, atheros.Service, atheros.EventLog
Include    = netvwifibus.inf
Needs      = VWiFiBus.Services

[ATHR_DEV_OS61_13C010CF.ndi.NTamd64.HW]
Include = netvwifibus.inf
Needs   = VWiFiBus.PnPFilterRegistration

[ATHR_DEV_OS61_147C10CF.ndi.NTamd64]
Characteristics = 0x84
BusType         = 5
AddReg          = atheros_os61.reg, atheros11n.reg, 5416.bandselect.reg, customer1ani.reg, adhocchannelselect.reg, enableswretry, overridetxok.reg, customer1roamPolicy.reg, smpsDynamic.reg, htAdhocdisable.reg, merlinshiftdelay.reg, d3forcel1disable.reg
DelReg          = atheros.DelReg
CopyFiles       = atheros.CopyFiles
*IfType         = 71            ; IF_TYPE_IEEE80211
*MediaType      = 16            ; NdisMediumNative802_11
*PhysicalMediaType = 9          ; NdisPhysicalMediumNative802_11
Include         = netvwifibus.inf, machine.inf
Needs           = VWiFiBus.CopyFiles

[ATHR_DEV_OS61_147C10CF.ndi.NTamd64.Services]
AddService = athr, 2, atheros.Service, atheros.EventLog
Include    = netvwifibus.inf
Needs      = VWiFiBus.Services

[ATHR_DEV_OS61_147C10CF.ndi.NTamd64.HW]
Include = netvwifibus.inf
Needs   = VWiFiBus.PnPFilterRegistration

[ATHR_DEV_OS61_147D10CF.ndi.NTamd64]
Characteristics = 0x84
BusType         = 5
AddReg          = atheros_os61.reg, atheros11n.reg, customer1ani.reg, adhocchannelselect.reg, enableswretry, overridetxok.reg, customer1roamPolicy.reg, htAdhocdisable.reg, merlinshiftdelay.reg, d3forcel1disable.reg
DelReg          = atheros.DelReg
CopyFiles       = atheros.CopyFiles
*IfType         = 71            ; IF_TYPE_IEEE80211
*MediaType      = 16            ; NdisMediumNative802_11
*PhysicalMediaType = 9          ; NdisPhysicalMediumNative802_11
Include         = netvwifibus.inf, machine.inf
Needs           = VWiFiBus.CopyFiles

[ATHR_DEV_OS61_147D10CF.ndi.NTamd64.Services]
AddService = athr, 2, atheros.Service, atheros.EventLog
Include    = netvwifibus.inf
Needs      = VWiFiBus.Services

[ATHR_DEV_OS61_147D10CF.ndi.NTamd64.HW]
Include = netvwifibus.inf
Needs   = VWiFiBus.PnPFilterRegistration

[ATHR_DEV_OS61_153710CF.ndi.NTamd64]
Characteristics = 0x84
BusType         = 5
AddReg          = atheros_os61.reg, atheros11n.reg, customer1ani.reg, adhocchannelselect.reg, enableswretry, overridetxok.reg, customer1roamPolicy.reg, htAdhocdisable.reg, triggerlevelkiteonly.reg, c3war.reg, customer1GreenTx.reg, SleepTimePwrSaveMax2000.reg
DelReg          = atheros.DelReg
CopyFiles       = atheros.CopyFiles
*IfType         = 71            ; IF_TYPE_IEEE80211
*MediaType      = 16            ; NdisMediumNative802_11
*PhysicalMediaType = 9          ; NdisPhysicalMediumNative802_11
Include         = netvwifibus.inf, machine.inf
Needs           = VWiFiBus.CopyFiles

[ATHR_DEV_OS61_153710CF.ndi.NTamd64.Services]
AddService = athr, 2, atheros.Service, atheros.EventLog
Include    = netvwifibus.inf
Needs      = VWiFiBus.Services

[ATHR_DEV_OS61_153710CF.ndi.NTamd64.HW]
Include = netvwifibus.inf
Needs   = VWiFiBus.PnPFilterRegistration

[ATHR_DEV_OS61_158F10CF.ndi.NTamd64]
Characteristics = 0x84
BusType         = 5
AddReg          = atheros_os61.reg, atheros11n.reg, customer1ani.reg, adhocchannelselect.reg, enableswretry, overridetxok.reg, customer1roamPolicy.reg, htAdhocdisable.reg, customer1GreenTx.reg, SleepTimePwrSaveMax2000.reg
DelReg          = atheros.DelReg
CopyFiles       = atheros.CopyFiles
*IfType         = 71            ; IF_TYPE_IEEE80211
*MediaType      = 16            ; NdisMediumNative802_11
*PhysicalMediaType = 9          ; NdisPhysicalMediumNative802_11
Include         = netvwifibus.inf, machine.inf
Needs           = VWiFiBus.CopyFiles

[ATHR_DEV_OS61_158F10CF.ndi.NTamd64.Services]
AddService = athr, 2, atheros.Service, atheros.EventLog
Include    = netvwifibus.inf
Needs      = VWiFiBus.Services

[ATHR_DEV_OS61_158F10CF.ndi.NTamd64.HW]
Include = netvwifibus.inf
Needs   = VWiFiBus.PnPFilterRegistration

[ATHR_DEV_OS61_161910CF.ndi.NTamd64]
Characteristics = 0x84
BusType         = 5
AddReg          = atheros_os61.reg, atheros11n.reg, customer1ani.reg, adhocchannelselect.reg, enableswretry, overridetxok.reg, customer1roamPolicy.reg, htAdhocdisable.reg, janusda.reg, triggerlevelkiteonly.reg, c3war.reg, customer1GreenTx.reg, SleepTimePwrSaveMax2000.reg
DelReg          = atheros.DelReg
CopyFiles       = atheros.CopyFiles
*IfType         = 71            ; IF_TYPE_IEEE80211
*MediaType      = 16            ; NdisMediumNative802_11
*PhysicalMediaType = 9          ; NdisPhysicalMediumNative802_11
Include         = netvwifibus.inf, machine.inf
Needs           = VWiFiBus.CopyFiles

[ATHR_DEV_OS61_161910CF.ndi.NTamd64.Services]
AddService = athr, 2, atheros.Service, atheros.EventLog
Include    = netvwifibus.inf
Needs      = VWiFiBus.Services

[ATHR_DEV_OS61_161910CF.ndi.NTamd64.HW]
Include = netvwifibus.inf
Needs   = VWiFiBus.PnPFilterRegistration

[ATHR_DEV_OS61_16A810CF.ndi.NTamd64]
Characteristics = 0x84
BusType         = 5
AddReg          = atheros_os61.reg, atheros11n.reg, 5416.bandselect.reg, customer1ani.reg, adhocchannelselect.reg, enableswretry, overridetxok.reg, customer1roamPolicy.reg, smpsDynamic.reg, htAdhocdisable.reg, customer1GreenTx.reg, SleepTimePwrSaveMax2000.reg, swBeaconProcess.reg
DelReg          = atheros.DelReg
CopyFiles       = atheros.CopyFiles
*IfType         = 71            ; IF_TYPE_IEEE80211
*MediaType      = 16            ; NdisMediumNative802_11
*PhysicalMediaType = 9          ; NdisPhysicalMediumNative802_11
Include         = netvwifibus.inf, machine.inf
Needs           = VWiFiBus.CopyFiles

[ATHR_DEV_OS61_16A810CF.ndi.NTamd64.Services]
AddService = athr, 2, atheros.Service, atheros.EventLog
Include    = netvwifibus.inf
Needs      = VWiFiBus.Services

[ATHR_DEV_OS61_16A810CF.ndi.NTamd64.HW]
Include = netvwifibus.inf
Needs   = VWiFiBus.PnPFilterRegistration

[ATHR_DEV_OS61_7125144F.ndi.NTamd64]
Characteristics = 0x84
BusType         = 5
AddReg          = atheros_os61.reg, atheros11n.reg, 5416.antennacontrols.reg, htAdhoc.reg, cfpignore.reg
DelReg          = atheros.DelReg
CopyFiles       = atheros.CopyFiles
*IfType         = 71            ; IF_TYPE_IEEE80211
*MediaType      = 16            ; NdisMediumNative802_11
*PhysicalMediaType = 9          ; NdisPhysicalMediumNative802_11
Include         = netvwifibus.inf, machine.inf
Needs           = VWiFiBus.CopyFiles

[ATHR_DEV_OS61_7125144F.ndi.NTamd64.Services]
AddService = athr, 2, atheros.Service, atheros.EventLog
Include    = netvwifibus.inf
Needs      = VWiFiBus.Services

[ATHR_DEV_OS61_7125144F.ndi.NTamd64.HW]
Include = netvwifibus.inf
Needs   = VWiFiBus.PnPFilterRegistration

[ATHR_DEV_OS61_03841014.ndi.NTamd64]
Characteristics = 0x84
BusType         = 5
AddReg          = atheros_os61.reg, atheros11n.reg, 5416.antennacontrols.reg, xb72.via.reg, htAdhoc.reg
DelReg          = atheros.DelReg
CopyFiles       = atheros.CopyFiles
*IfType         = 71            ; IF_TYPE_IEEE80211
*MediaType      = 16            ; NdisMediumNative802_11
*PhysicalMediaType = 9          ; NdisPhysicalMediumNative802_11
Include         = netvwifibus.inf, machine.inf
Needs           = VWiFiBus.CopyFiles

[ATHR_DEV_OS61_03841014.ndi.NTamd64.Services]
AddService = athr, 2, atheros.Service, atheros.EventLog
Include    = netvwifibus.inf
Needs      = VWiFiBus.Services

[ATHR_DEV_OS61_03841014.ndi.NTamd64.HW]
Include = netvwifibus.inf
Needs   = VWiFiBus.PnPFilterRegistration

[ATHR_DEV_OS61_3A171186.ndi.NTamd64]
Characteristics = 0x84
BusType         = 5
AddReg          = atheros_os61.reg, atheros.reg, customer5Led.reg
DelReg          = atheros.DelReg
CopyFiles       = atheros.CopyFiles
*IfType         = 71        ; IF_TYPE_IEEE80211
*MediaType      = 16        ; NdisMediumNative802_11
*PhysicalMediaType = 9      ; NdisPhysicalMediumNative802_11
Include         = netvwifibus.inf, machine.inf
Needs           = VWiFiBus.CopyFiles

[ATHR_DEV_OS61_3A171186.ndi.NTamd64.Services]
AddService = athr, 2, atheros.Service, atheros.EventLog
Include    = netvwifibus.inf
Needs      = VWiFiBus.Services

[ATHR_DEV_OS61_3A171186.ndi.NTamd64.HW]
Include = netvwifibus.inf
Needs   = VWiFiBus.PnPFilterRegistration

[ATHR_DEV_OS61_10261A3B.ndi.NTamd64]
Characteristics = 0x84
BusType         = 5
AddReg          = atheros_os61.reg, atheros.reg, cemspecled_func1_3.reg, d3hot.reg
DelReg          = atheros.DelReg
CopyFiles       = atheros.CopyFiles
*IfType         = 71        ; IF_TYPE_IEEE80211
*MediaType      = 16        ; NdisMediumNative802_11
*PhysicalMediaType = 9      ; NdisPhysicalMediumNative802_11
Include         = netvwifibus.inf, machine.inf
Needs           = VWiFiBus.CopyFiles

[ATHR_DEV_OS61_10261A3B.ndi.NTamd64.Services]
AddService = athr, 2, atheros.Service, atheros.EventLog
Include    = netvwifibus.inf
Needs      = VWiFiBus.Services

[ATHR_DEV_OS61_10261A3B.ndi.NTamd64.HW]
Include = netvwifibus.inf
Needs   = VWiFiBus.PnPFilterRegistration

[ATHR_DEV_OS61_80111799.ndi.NTamd64]
Characteristics = 0x84
BusType         = 5
AddReg          = atheros_os61.reg, atheros11n.reg, customer7Led.reg, ratecap.reg, htAdhoc.reg
DelReg          = atheros.DelReg
CopyFiles       = atheros.CopyFiles
*IfType         = 71            ; IF_TYPE_IEEE80211
*MediaType      = 16            ; NdisMediumNative802_11
*PhysicalMediaType = 9          ; NdisPhysicalMediumNative802_11
Include         = netvwifibus.inf, machine.inf
Needs           = VWiFiBus.CopyFiles

[ATHR_DEV_OS61_80111799.ndi.NTamd64.Services]
AddService = athr, 2, atheros.Service, atheros.EventLog
Include    = netvwifibus.inf
Needs      = VWiFiBus.Services

[ATHR_DEV_OS61_80111799.ndi.NTamd64.HW]
Include = netvwifibus.inf
Needs   = VWiFiBus.PnPFilterRegistration

[ATHR_DEV_OS61_1186.ndi.NTamd64]
Characteristics = 0x84
BusType         = 5
AddReg          = atheros_os61.reg, atheros11n.reg, customer5.11nLED.reg, ratecap.reg, htAdhoc.reg
DelReg          = atheros.DelReg
CopyFiles       = atheros.CopyFiles
*IfType         = 71            ; IF_TYPE_IEEE80211
*MediaType      = 16            ; NdisMediumNative802_11
*PhysicalMediaType = 9          ; NdisPhysicalMediumNative802_11
Include         = netvwifibus.inf, machine.inf
Needs           = VWiFiBus.CopyFiles

[ATHR_DEV_OS61_1186.ndi.NTamd64.Services]
AddService = athr, 2, atheros.Service, atheros.EventLog
Include    = netvwifibus.inf
Needs      = VWiFiBus.Services

[ATHR_DEV_OS61_1186.ndi.NTamd64.HW]
Include = netvwifibus.inf
Needs   = VWiFiBus.PnPFilterRegistration

[ATHR_DEV_OS61_3A691186.ndi.NTamd64]
Characteristics = 0x84
BusType         = 5
AddReg          = atheros_os61.reg, atheros11n.reg, pcibusconfig.reg, customer5.11nLED.reg, htAdhoc.reg
DelReg          = atheros.DelReg
CopyFiles       = atheros.CopyFiles
*IfType         = 71            ; IF_TYPE_IEEE80211
*MediaType      = 16            ; NdisMediumNative802_11
*PhysicalMediaType = 9          ; NdisPhysicalMediumNative802_11
Include         = netvwifibus.inf, machine.inf
Needs           = VWiFiBus.CopyFiles

[ATHR_DEV_OS61_3A691186.ndi.NTamd64.Services]
AddService = athr, 2, atheros.Service, atheros.EventLog
Include    = netvwifibus.inf
Needs      = VWiFiBus.Services

[ATHR_DEV_OS61_3A691186.ndi.NTamd64.HW]
Include = netvwifibus.inf
Needs   = VWiFiBus.PnPFilterRegistration

[ATHR_DEV_OS61_3A6D1186.ndi.NTamd64]
Characteristics = 0x84
BusType         = 5
AddReg          = atheros_os61.reg, atheros11n.reg, pcibusconfig.reg, customer5.3x3.reg, customer5.11nLED.reg, htAdhoc.reg
DelReg          = atheros.DelReg
CopyFiles       = atheros.CopyFiles
*IfType         = 71            ; IF_TYPE_IEEE80211
*MediaType      = 16            ; NdisMediumNative802_11
*PhysicalMediaType = 9          ; NdisPhysicalMediumNative802_11
Include         = netvwifibus.inf, machine.inf
Needs           = VWiFiBus.CopyFiles

[ATHR_DEV_OS61_3A6D1186.ndi.NTamd64.Services]
AddService = athr, 2, atheros.Service, atheros.EventLog
Include    = netvwifibus.inf
Needs      = VWiFiBus.Services

[ATHR_DEV_OS61_3A6D1186.ndi.NTamd64.HW]
Include = netvwifibus.inf
Needs   = VWiFiBus.PnPFilterRegistration

[ATHR_DEV_OS61_3A6F1186.ndi.NTamd64]
Characteristics = 0x84
BusType         = 5
AddReg          = atheros_os61.reg, atheros11n.reg, customer5.PCIe11nLed.reg, expresscardaspmoff.reg, htAdhoc.reg
DelReg          = atheros.DelReg
CopyFiles       = atheros.CopyFiles
*IfType         = 71            ; IF_TYPE_IEEE80211
*MediaType      = 16            ; NdisMediumNative802_11
*PhysicalMediaType = 9          ; NdisPhysicalMediumNative802_11
Include         = netvwifibus.inf, machine.inf
Needs           = VWiFiBus.CopyFiles

[ATHR_DEV_OS61_3A6F1186.ndi.NTamd64.Services]
AddService = athr, 2, atheros.Service, atheros.EventLog
Include    = netvwifibus.inf
Needs      = VWiFiBus.Services

[ATHR_DEV_OS61_3A6F1186.ndi.NTamd64.HW]
Include = netvwifibus.inf
Needs   = VWiFiBus.PnPFilterRegistration

[ATHR_DEV_OS61_3A701186.ndi.NTamd64]
Characteristics = 0x84
BusType         = 5
AddReg          = atheros_os61.reg, atheros11n.reg, customer5.3x3.reg, customer5.PCIe11nLed.reg, expresscardaspmoff.reg, htAdhoc.reg
DelReg          = atheros.DelReg
CopyFiles       = atheros.CopyFiles
*IfType         = 71            ; IF_TYPE_IEEE80211
*MediaType      = 16            ; NdisMediumNative802_11
*PhysicalMediaType = 9          ; NdisPhysicalMediumNative802_11
Include         = netvwifibus.inf, machine.inf
Needs           = VWiFiBus.CopyFiles

[ATHR_DEV_OS61_3A701186.ndi.NTamd64.Services]
AddService = athr, 2, atheros.Service, atheros.EventLog
Include    = netvwifibus.inf
Needs      = VWiFiBus.Services

[ATHR_DEV_OS61_3A701186.ndi.NTamd64.HW]
Include = netvwifibus.inf
Needs   = VWiFiBus.PnPFilterRegistration

[ATHR_DEV_OS61_3A7A1186.ndi.NTamd64]
Characteristics = 0x84
BusType         = 5
AddReg          = atheros_os61.reg, atheros11n.reg, pcibusconfig.reg, customer5.11nLED.reg, smpsDynamic.reg, htAdhoc.reg
DelReg          = atheros.DelReg
CopyFiles       = atheros.CopyFiles
*IfType         = 71            ; IF_TYPE_IEEE80211
*MediaType      = 16            ; NdisMediumNative802_11
*PhysicalMediaType = 9          ; NdisPhysicalMediumNative802_11
Include         = netvwifibus.inf, machine.inf
Needs           = VWiFiBus.CopyFiles

[ATHR_DEV_OS61_3A7A1186.ndi.NTamd64.Services]
AddService = athr, 2, atheros.Service, atheros.EventLog
Include    = netvwifibus.inf
Needs      = VWiFiBus.Services

[ATHR_DEV_OS61_3A7A1186.ndi.NTamd64.HW]
Include = netvwifibus.inf
Needs   = VWiFiBus.PnPFilterRegistration

[ATHR_DEV_OS61_3A7B1186.ndi.NTamd64]
Characteristics = 0x84
BusType         = 5
AddReg          = atheros_os61.reg, atheros11n.reg, customer5.11nLED.reg, ratecap.reg, smpsDynamic.reg, htAdhoc.reg
DelReg          = atheros.DelReg
CopyFiles       = atheros.CopyFiles
*IfType         = 71            ; IF_TYPE_IEEE80211
*MediaType      = 16            ; NdisMediumNative802_11
*PhysicalMediaType = 9          ; NdisPhysicalMediumNative802_11
Include         = netvwifibus.inf, machine.inf
Needs           = VWiFiBus.CopyFiles

[ATHR_DEV_OS61_3A7B1186.ndi.NTamd64.Services]
AddService = athr, 2, atheros.Service, atheros.EventLog
Include    = netvwifibus.inf
Needs      = VWiFiBus.Services

[ATHR_DEV_OS61_3A7B1186.ndi.NTamd64.HW]
Include = netvwifibus.inf
Needs   = VWiFiBus.PnPFilterRegistration

[ATHR_DEV_OS61_N2062.ndi.NTamd64]
Characteristics = 0x84
BusType         = 5
AddReg          = atheros_os61.reg, customer11.reg, customer11custom.reg, customer11_legacywmode.reg, cemspecled_func1_1.reg, customer11Ant.reg, rfKillDelayDetect.reg
DelReg          = atheros.DelReg
CopyFiles       = atheros.CopyFiles
*IfType         = 71        ; IF_TYPE_IEEE80211
*MediaType      = 16        ; NdisMediumNative802_11
*PhysicalMediaType = 9      ; NdisPhysicalMediumNative802_11
Include         = netvwifibus.inf, machine.inf
Needs           = VWiFiBus.CopyFiles

[ATHR_DEV_OS61_N2062.ndi.NTamd64.Services]
AddService = athr, 2, atheros.Service, atheros.EventLog
Include    = netvwifibus.inf
Needs      = VWiFiBus.Services

[ATHR_DEV_OS61_N2062.ndi.NTamd64.HW]
Include = netvwifibus.inf
Needs   = VWiFiBus.PnPFilterRegistration

[ATHR_DEV_OS61_N3072.ndi.NTamd64]
Characteristics = 0x84
BusType         = 5
AddReg          = atheros_os61.reg, customer11n.reg, customer11custom.reg, customer11_11nwmode.reg, cemspecled_func1_1.reg, htAdhoc.reg
DelReg          = atheros.DelReg
CopyFiles       = atheros.CopyFiles
*IfType         = 71            ; IF_TYPE_IEEE80211
*MediaType      = 16            ; NdisMediumNative802_11
*PhysicalMediaType = 9          ; NdisPhysicalMediumNative802_11
Include         = netvwifibus.inf, machine.inf
Needs           = VWiFiBus.CopyFiles

[ATHR_DEV_OS61_N3072.ndi.NTamd64.Services]
AddService = athr, 2, atheros.Service, atheros.EventLog
Include    = netvwifibus.inf
Needs      = VWiFiBus.Services

[ATHR_DEV_OS61_N3072.ndi.NTamd64.HW]
Include = netvwifibus.inf
Needs   = VWiFiBus.PnPFilterRegistration

[ATHR_DEV_OS61_N3073.ndi.NTamd64]
Characteristics = 0x84
BusType         = 5
AddReg          = atheros_os61.reg, customer11n.reg, customer11custom.reg, customer11_11n40wmode.reg, cemspecled_func1_1.reg, htAdhoc.reg
DelReg          = atheros.DelReg
CopyFiles       = atheros.CopyFiles
*IfType         = 71            ; IF_TYPE_IEEE80211
*MediaType      = 16            ; NdisMediumNative802_11
*PhysicalMediaType = 9          ; NdisPhysicalMediumNative802_11
Include         = netvwifibus.inf, machine.inf
Needs           = VWiFiBus.CopyFiles

[ATHR_DEV_OS61_N3073.ndi.NTamd64.Services]
AddService = athr, 2, atheros.Service, atheros.EventLog
Include    = netvwifibus.inf
Needs      = VWiFiBus.Services

[ATHR_DEV_OS61_N3073.ndi.NTamd64.HW]
Include = netvwifibus.inf
Needs   = VWiFiBus.PnPFilterRegistration

[ATHR_DEV_OS61_S001A.ndi.NTamd64]
Characteristics = 0x84
BusType         = 5
AddReg          = atheros_os61.reg, atheros.reg, customer_Samsung.reg, cmdRegister.reg, ignore11denable.reg
DelReg          = atheros.DelReg
CopyFiles       = atheros.CopyFiles
*IfType         = 71        ; IF_TYPE_IEEE80211
*MediaType      = 16        ; NdisMediumNative802_11
*PhysicalMediaType = 9      ; NdisPhysicalMediumNative802_11
Include         = netvwifibus.inf, machine.inf
Needs           = VWiFiBus.CopyFiles

[ATHR_DEV_OS61_S001A.ndi.NTamd64.Services]
AddService = athr, 2, atheros.Service, atheros.EventLog
Include    = netvwifibus.inf
Needs      = VWiFiBus.Services

[ATHR_DEV_OS61_S001A.ndi.NTamd64.HW]
Include = netvwifibus.inf
Needs   = VWiFiBus.PnPFilterRegistration

[ATHR_DEV_OS61_S001B.ndi.NTamd64]
Characteristics = 0x84
BusType         = 5
AddReg          = atheros_os61.reg, atheros.reg, customer_Samsung.reg, cmdRegister.reg, ignore11denable.reg
DelReg          = atheros.DelReg
CopyFiles       = atheros.CopyFiles
*IfType         = 71        ; IF_TYPE_IEEE80211
*MediaType      = 16        ; NdisMediumNative802_11
*PhysicalMediaType = 9      ; NdisPhysicalMediumNative802_11
Include         = netvwifibus.inf, machine.inf
Needs           = VWiFiBus.CopyFiles

[ATHR_DEV_OS61_S001B.ndi.NTamd64.Services]
AddService = athr, 2, atheros.Service, atheros.EventLog
Include    = netvwifibus.inf
Needs      = VWiFiBus.Services

[ATHR_DEV_OS61_S001B.ndi.NTamd64.HW]
Include = netvwifibus.inf
Needs   = VWiFiBus.PnPFilterRegistration

[ATHR_DEV_OS61_S3067.ndi.NTamd64]
Characteristics = 0x84
BusType         = 5
AddReg          = atheros_os61.reg, atheros.reg, customer_Samsung.reg, rssiAdjust.reg, cmdRegister.reg, ignore11denable.reg
DelReg          = atheros.DelReg
CopyFiles       = atheros.CopyFiles
*IfType         = 71        ; IF_TYPE_IEEE80211
*MediaType      = 16        ; NdisMediumNative802_11
*PhysicalMediaType = 9      ; NdisPhysicalMediumNative802_11
Include         = netvwifibus.inf, machine.inf
Needs           = VWiFiBus.CopyFiles

[ATHR_DEV_OS61_S3067.ndi.NTamd64.Services]
AddService = athr, 2, atheros.Service, atheros.EventLog
Include    = netvwifibus.inf
Needs      = VWiFiBus.Services

[ATHR_DEV_OS61_S3067.ndi.NTamd64.HW]
Include = netvwifibus.inf
Needs   = VWiFiBus.PnPFilterRegistration

[ATHR_DEV_OS61_S3067b.ndi.NTamd64]
Characteristics = 0x84
BusType         = 5
AddReg          = atheros_os61.reg, atheros.reg, customer_Samsung.reg, rssiAdjust.reg, cmdRegister.reg, cmdRegister.reg, ignore11denable.reg
DelReg          = atheros.DelReg
CopyFiles       = atheros.CopyFiles
*IfType         = 71        ; IF_TYPE_IEEE80211
*MediaType      = 16        ; NdisMediumNative802_11
*PhysicalMediaType = 9      ; NdisPhysicalMediumNative802_11
Include         = netvwifibus.inf, machine.inf
Needs           = VWiFiBus.CopyFiles

[ATHR_DEV_OS61_S3067b.ndi.NTamd64.Services]
AddService = athr, 2, atheros.Service, atheros.EventLog
Include    = netvwifibus.inf
Needs      = VWiFiBus.Services

[ATHR_DEV_OS61_S3067b.ndi.NTamd64.HW]
Include = netvwifibus.inf
Needs   = VWiFiBus.PnPFilterRegistration

[ATHR_DEV_OS61_10241A3B.ndi.NTamd64]
Characteristics = 0x84
BusType         = 5
AddReg          = atheros_os61.reg, atheros11n.reg, cemspecled_func1_1.reg, htEnableWepTkip.reg, htAdhoc.reg
DelReg          = atheros.DelReg
CopyFiles       = atheros.CopyFiles
*IfType         = 71            ; IF_TYPE_IEEE80211
*MediaType      = 16            ; NdisMediumNative802_11
*PhysicalMediaType = 9          ; NdisPhysicalMediumNative802_11
Include         = netvwifibus.inf, machine.inf
Needs           = VWiFiBus.CopyFiles

[ATHR_DEV_OS61_10241A3B.ndi.NTamd64.Services]
AddService = athr, 2, atheros.Service, atheros.EventLog
Include    = netvwifibus.inf
Needs      = VWiFiBus.Services

[ATHR_DEV_OS61_10241A3B.ndi.NTamd64.HW]
Include = netvwifibus.inf
Needs   = VWiFiBus.PnPFilterRegistration

[ATHR_DEV_OS61_02B0.ndi.NTamd64]
Characteristics = 0x84
BusType         = 5
AddReg          = atheros_os61.reg, atheros.reg, ledcontrol.reg, power.reg
DelReg          = atheros.DelReg
CopyFiles       = atheros.CopyFiles
*IfType         = 71        ; IF_TYPE_IEEE80211
*MediaType      = 16        ; NdisMediumNative802_11
*PhysicalMediaType = 9      ; NdisPhysicalMediumNative802_11
Include         = netvwifibus.inf, machine.inf
Needs           = VWiFiBus.CopyFiles

[ATHR_DEV_OS61_02B0.ndi.NTamd64.Services]
AddService = athr, 2, atheros.Service, atheros.EventLog
Include    = netvwifibus.inf
Needs      = VWiFiBus.Services

[ATHR_DEV_OS61_02B0.ndi.NTamd64.HW]
Include = netvwifibus.inf
Needs   = VWiFiBus.PnPFilterRegistration

[ATHR_DEV_OS61_D001C.ndi.NTamd64]
Characteristics = 0x84
BusType         = 5
AddReg          = atheros_os61.reg, atheros.reg, ledcontrol.reg, power.reg
DelReg          = atheros.DelReg
CopyFiles       = atheros.CopyFiles
*IfType         = 71        ; IF_TYPE_IEEE80211
*MediaType      = 16        ; NdisMediumNative802_11
*PhysicalMediaType = 9      ; NdisPhysicalMediumNative802_11
Include         = netvwifibus.inf, machine.inf
Needs           = VWiFiBus.CopyFiles

[ATHR_DEV_OS61_D001C.ndi.NTamd64.Services]
AddService = athr, 2, atheros.Service, atheros.EventLog
Include    = netvwifibus.inf
Needs      = VWiFiBus.Services

[ATHR_DEV_OS61_D001C.ndi.NTamd64.HW]
Include = netvwifibus.inf
Needs   = VWiFiBus.PnPFilterRegistration

[ATHR_DEV_OS61_D30ABHZ.ndi.NTamd64]
Characteristics = 0x84
BusType         = 5
AddReg          = atheros_os61.reg, atheros11n.reg, ledcontrol3.reg, kitec3.reg, djanusda.reg
DelReg          = atheros.DelReg
CopyFiles       = atheros.CopyFiles
*IfType         = 71        ; IF_TYPE_IEEE80211
*MediaType      = 16        ; NdisMediumNative802_11
*PhysicalMediaType = 9      ; NdisPhysicalMediumNative802_11
Include         = netvwifibus.inf, machine.inf
Needs           = VWiFiBus.CopyFiles

[ATHR_DEV_OS61_D30ABHZ.ndi.NTamd64.Services]
AddService = athr, 2, atheros.Service, atheros.EventLog
Include    = netvwifibus.inf
Needs      = VWiFiBus.Services

[ATHR_DEV_OS61_D30ABHZ.ndi.NTamd64.HW]
Include = netvwifibus.inf
Needs   = VWiFiBus.PnPFilterRegistration

[ATHR_DEV_OS61_D30A1.ndi.NTamd64]
Characteristics = 0x84
BusType         = 5
AddReg          = atheros_os61.reg, atheros11n.reg, ledcontrol2.reg, kitec3.reg
DelReg          = atheros.DelReg
CopyFiles       = atheros.CopyFiles
*IfType         = 71        ; IF_TYPE_IEEE80211
*MediaType      = 16        ; NdisMediumNative802_11
*PhysicalMediaType = 9      ; NdisPhysicalMediumNative802_11
Include         = netvwifibus.inf, machine.inf
Needs           = VWiFiBus.CopyFiles

[ATHR_DEV_OS61_D30A1.ndi.NTamd64.Services]
AddService = athr, 2, atheros.Service, atheros.EventLog
Include    = netvwifibus.inf
Needs      = VWiFiBus.Services

[ATHR_DEV_OS61_D30A1.ndi.NTamd64.HW]
Include = netvwifibus.inf
Needs   = VWiFiBus.PnPFilterRegistration

[ATHR_DEV_OS61_D30AB.ndi.NTamd64]
Characteristics = 0x84
BusType         = 5
AddReg          = atheros_os61.reg, atheros11n.reg, ledcontrol2.reg, kitec3.reg, djanusda2.reg
DelReg          = atheros.DelReg
CopyFiles       = atheros.CopyFiles
*IfType         = 71        ; IF_TYPE_IEEE80211
*MediaType      = 16        ; NdisMediumNative802_11
*PhysicalMediaType = 9      ; NdisPhysicalMediumNative802_11
Include         = netvwifibus.inf, machine.inf
Needs           = VWiFiBus.CopyFiles

[ATHR_DEV_OS61_D30AB.ndi.NTamd64.Services]
AddService = athr, 2, atheros.Service, atheros.EventLog
Include    = netvwifibus.inf
Needs      = VWiFiBus.Services

[ATHR_DEV_OS61_D30AB.ndi.NTamd64.HW]
Include = netvwifibus.inf
Needs   = VWiFiBus.PnPFilterRegistration

[ATHR_DEV_OS61_H001C.ndi.NTamd64]
Characteristics = 0x84
BusType         = 5
AddReg          = atheros_os61.reg, atheros.reg, ledcontrol.reg, AdhocModeSelect.reg
DelReg          = atheros.DelReg
CopyFiles       = atheros.CopyFiles
*IfType         = 71        ; IF_TYPE_IEEE80211
*MediaType      = 16        ; NdisMediumNative802_11
*PhysicalMediaType = 9      ; NdisPhysicalMediumNative802_11
Include         = netvwifibus.inf
Needs           = VWiFiBus.CopyFiles

[ATHR_DEV_OS61_H001C.ndi.NTamd64.Services]
AddService = athr, 2, atheros.Service, atheros.EventLog
Include    = netvwifibus.inf
Needs      = VWiFiBus.Services

[ATHR_DEV_OS61_H001C.ndi.NTamd64.HW]
Include = netvwifibus.inf
Needs   = VWiFiBus.PnPFilterRegistration

[ATHR_DEV_OS61_H2063.ndi.NTamd64]
Characteristics = 0x84
BusType         = 5
AddReg          = atheros_os61.reg, atheros.reg, cemspecled_func0_1.reg, AdhocModeSelect.reg
DelReg          = atheros.DelReg
CopyFiles       = atheros.CopyFiles
*IfType         = 71        ; IF_TYPE_IEEE80211
*MediaType      = 16        ; NdisMediumNative802_11
*PhysicalMediaType = 9      ; NdisPhysicalMediumNative802_11
Include         = netvwifibus.inf
Needs           = VWiFiBus.CopyFiles

[ATHR_DEV_OS61_H2063.ndi.NTamd64.Services]
AddService = athr, 2, atheros.Service, atheros.EventLog
Include    = netvwifibus.inf
Needs      = VWiFiBus.Services

[ATHR_DEV_OS61_H2063.ndi.NTamd64.HW]
Include = netvwifibus.inf
Needs   = VWiFiBus.PnPFilterRegistration

[ATHR_DEV_OS61_H002A.ndi.NTamd64]
Characteristics = 0x84
BusType         = 5
AddReg          = atheros_os61.reg, atheros11n.reg, cemspecled_func0_1.reg, AdhocModeSelect.reg
DelReg          = atheros.DelReg
CopyFiles       = atheros.CopyFiles
*IfType         = 71        ; IF_TYPE_IEEE80211
*MediaType      = 16        ; NdisMediumNative802_11
*PhysicalMediaType = 9      ; NdisPhysicalMediumNative802_11
Include         = netvwifibus.inf
Needs           = VWiFiBus.CopyFiles

[ATHR_DEV_OS61_H002A.ndi.NTamd64.Services]
AddService = athr, 2, atheros.Service, atheros.EventLog
Include    = netvwifibus.inf
Needs      = VWiFiBus.Services

[ATHR_DEV_OS61_H002A.ndi.NTamd64.HW]
Include = netvwifibus.inf
Needs   = VWiFiBus.PnPFilterRegistration

[ATHR_DEV_OS61_H30A1.ndi.NTamd64]
Characteristics = 0x84
BusType         = 5
AddReg          = atheros_os61.reg, atheros11n.reg, cemspecled_func0_1.reg, AdhocModeSelect.reg, amp_default.reg
DelReg          = atheros.DelReg
CopyFiles       = atheros.CopyFiles
*IfType         = 71            ; IF_TYPE_IEEE80211
*MediaType      = 16            ; NdisMediumNative802_11
*PhysicalMediaType = 9          ; NdisPhysicalMediumNative802_11
Include         = netvwifibus.inf
Needs           = VWiFiBus.CopyFiles

[ATHR_DEV_OS61_H30A1.ndi.NTamd64.Services]
AddService = athr, 2, atheros.Service, atheros.EventLog
Include    = netvwifibus.inf
Needs      = VWiFiBus.Services

[ATHR_DEV_OS61_H30A1.ndi.NTamd64.HW]
Include = netvwifibus.inf
Needs   = VWiFiBus.PnPFilterRegistration

[ATHR_DEV_OS61_H30AB.ndi.NTamd64]
Characteristics = 0x84
BusType         = 5
AddReg          = atheros_os61.reg, atheros11n.reg, cemspecled_func0_1.reg, janusda.reg, throughput.reg, AdhocModeSelect.reg, amp_default.reg
DelReg          = atheros.DelReg
CopyFiles       = atheros.CopyFiles
*IfType         = 71            ; IF_TYPE_IEEE80211
*MediaType      = 16            ; NdisMediumNative802_11
*PhysicalMediaType = 9          ; NdisPhysicalMediumNative802_11
Include         = netvwifibus.inf
Needs           = VWiFiBus.CopyFiles

[ATHR_DEV_OS61_H30AB.ndi.NTamd64.Services]
AddService = athr, 2, atheros.Service, atheros.EventLog
Include    = netvwifibus.inf
Needs      = VWiFiBus.Services

[ATHR_DEV_OS61_H30AB.ndi.NTamd64.HW]
Include = netvwifibus.inf
Needs   = VWiFiBus.PnPFilterRegistration

[ATHR_DEV_OS61_H30A4.ndi.NTamd64]
Characteristics = 0x84
BusType         = 5
AddReg          = atheros_os61.reg, atheros11n.reg, ledcontrol4.reg, AdhocModeSelect.reg
DelReg          = atheros.DelReg
CopyFiles       = atheros.CopyFiles
*IfType         = 71            ; IF_TYPE_IEEE80211
*MediaType      = 16            ; NdisMediumNative802_11
*PhysicalMediaType = 9          ; NdisPhysicalMediumNative802_11
Include         = netvwifibus.inf
Needs           = VWiFiBus.CopyFiles

[ATHR_DEV_OS61_H30A4.ndi.NTamd64.Services]
AddService = athr, 2, atheros.Service, atheros.EventLog
Include    = netvwifibus.inf
Needs      = VWiFiBus.Services

[ATHR_DEV_OS61_H30A4.ndi.NTamd64.HW]
Include = netvwifibus.inf
Needs   = VWiFiBus.PnPFilterRegistration

[ATHR_DEV_OS61_H3197.ndi.NTamd64]
Characteristics = 0x84
BusType         = 5
AddReg          = atheros_os61.reg, atheros11n.reg, cemspecled_func0_1.reg, HPheliusda.reg, AdhocModeSelect.reg
DelReg          = atheros.DelReg
CopyFiles       = atheros.CopyFiles
*IfType         = 71            ; IF_TYPE_IEEE80211
*MediaType      = 16            ; NdisMediumNative802_11
*PhysicalMediaType = 9          ; NdisPhysicalMediumNative802_11
Include         = netvwifibus.inf
Needs           = VWiFiBus.CopyFiles

[ATHR_DEV_OS61_H3197.ndi.NTamd64.Services]
AddService = athr, 2, atheros.Service, atheros.EventLog
Include    = netvwifibus.inf
Needs      = VWiFiBus.Services

[ATHR_DEV_OS61_H3197.ndi.NTamd64.HW]
Include = netvwifibus.inf
Needs   = VWiFiBus.PnPFilterRegistration

[ATHR_DEV_OS61_H3116.ndi.NTamd64]
Characteristics = 0x84
BusType         = 5
AddReg          = atheros_os61.reg, atheros11n.reg, ledcontrol6.reg, AdhocModeSelect.reg
DelReg          = atheros.DelReg
CopyFiles       = atheros.CopyFiles
*IfType         = 71            ; IF_TYPE_IEEE80211
*MediaType      = 16            ; NdisMediumNative802_11
*PhysicalMediaType = 9          ; NdisPhysicalMediumNative802_11
Include         = netvwifibus.inf
Needs           = VWiFiBus.CopyFiles

[ATHR_DEV_OS61_H3116.ndi.NTamd64.Services]
AddService = athr, 2, atheros.Service, atheros.EventLog
Include    = netvwifibus.inf
Needs      = VWiFiBus.Services

[ATHR_DEV_OS61_H3116.ndi.NTamd64.HW]
Include = netvwifibus.inf
Needs   = VWiFiBus.PnPFilterRegistration

[ATHR_DEV_OS61_H3112.ndi.NTamd64]
Characteristics = 0x84
BusType         = 5
AddReg          = atheros_os61.reg, atheros11n.reg, ledcontrol6.reg, AdhocModeSelect.reg
DelReg          = atheros.DelReg
CopyFiles       = atheros.CopyFiles
*IfType         = 71            ; IF_TYPE_IEEE80211
*MediaType      = 16            ; NdisMediumNative802_11
*PhysicalMediaType = 9          ; NdisPhysicalMediumNative802_11
Include         = netvwifibus.inf
Needs           = VWiFiBus.CopyFiles

[ATHR_DEV_OS61_H3112.ndi.NTamd64.Services]
AddService = athr, 2, atheros.Service, atheros.EventLog
Include    = netvwifibus.inf
Needs      = VWiFiBus.Services

[ATHR_DEV_OS61_H3112.ndi.NTamd64.HW]
Include = netvwifibus.inf
Needs   = VWiFiBus.PnPFilterRegistration

[ATHR_DEV_OS61_H3119.ndi.NTamd64]
Characteristics = 0x84
BusType         = 5
AddReg          = atheros_os61.reg, atheros11n.reg, 9485BTcoex.reg, customer2GreenTx.reg, paprdenable.reg, AdhocModeSelect.reg, edmaStopRecvDelay.reg, cemspecled_func0_6.reg, sharegpio.reg, amp_default.reg, InvalidRateIgnore.reg
DelReg          = atheros.DelReg
CopyFiles       = atheros.CopyFiles
*IfType         = 71        ; IF_TYPE_IEEE80211
*MediaType      = 16        ; NdisMediumNative802_11
*PhysicalMediaType = 9      ; NdisPhysicalMediumNative802_11
Include         = netvwifibus.inf, machine.inf
Needs           = VWiFiBus.CopyFiles

[ATHR_DEV_OS61_H3119.ndi.NTamd64.Services]
AddService = athr, 2, atheros.Service, atheros.EventLog
Include    = netvwifibus.inf
Needs      = VWiFiBus.Services

[ATHR_DEV_OS61_H3119.ndi.NTamd64.HW]
Include = netvwifibus.inf
Needs   = PciASPMOptIn, VWiFiBus.PnPFilterRegistration

[ATHR_DEV_OS61_H3118.ndi.NTamd64]
Characteristics = 0x84
BusType         = 5
AddReg          = atheros_os61.reg, atheros11n.reg, customer2GreenTx.reg, paprdenable.reg, AdhocModeSelect.reg, edmaStopRecvDelay.reg, cemspecled_func0_6.reg, sharegpio.reg, amp_default.reg, InvalidRateIgnore.reg, miracast_scc.reg
DelReg          = atheros.DelReg
CopyFiles       = atheros.CopyFiles
*IfType         = 71        ; IF_TYPE_IEEE80211
*MediaType      = 16        ; NdisMediumNative802_11
*PhysicalMediaType = 9      ; NdisPhysicalMediumNative802_11
Include         = netvwifibus.inf, machine.inf
Needs           = VWiFiBus.CopyFiles

[ATHR_DEV_OS61_H3118.ndi.NTamd64.Services]
AddService = athr, 2, atheros.Service, atheros.EventLog
Include    = netvwifibus.inf
Needs      = VWiFiBus.Services

[ATHR_DEV_OS61_H3118.ndi.NTamd64.HW]
Include = netvwifibus.inf
Needs   = PciASPMOptIn, VWiFiBus.PnPFilterRegistration

[ATHR_DEV_OS61_H3335.ndi.NTamd64]
Characteristics = 0x84
BusType         = 5
AddReg          = atheros_os61.reg, atheros11n.reg, smpsDynamic.reg, ledcontrol7.reg, customer2GreenTx.reg, paprdenable.reg, jupiter2ant.reg, AdhocModeSelect.reg, wowenable.reg, roamPolicy.reg, amp_default.reg, InvalidRateIgnore.reg, miracast_scc.reg
DelReg          = atheros.DelReg
CopyFiles       = atheros.CopyFiles
*IfType         = 71        ; IF_TYPE_IEEE80211
*MediaType      = 16        ; NdisMediumNative802_11
*PhysicalMediaType = 9      ; NdisPhysicalMediumNative802_11
Include         = netvwifibus.inf, machine.inf
Needs           = VWiFiBus.CopyFiles

[ATHR_DEV_OS61_H3335.ndi.NTamd64.Services]
AddService = athr, 2, atheros.Service, atheros.EventLog
Include    = netvwifibus.inf
Needs      = VWiFiBus.Services

[ATHR_DEV_OS61_H3335.ndi.NTamd64.HW]
Include = netvwifibus.inf
Needs   = PciASPMOptIn, VWiFiBus.PnPFilterRegistration

[ATHR_DEV_OS61_H9565.ndi.NTamd64]
Characteristics = 0x84
BusType         = 5
AddReg          = atheros_os61.reg, atheros11n.reg, htAdhoc.reg, aphroditeant.reg, aphrodite_coex.reg, ledcontrol8.reg, ConnectionFailure.reg, aphroditeantdiv.reg, amp_default.reg, InvalidRateIgnore.reg, power_management.reg, miracast_scc.reg
DelReg          = atheros.DelReg
CopyFiles       = atheros.CopyFiles
*IfType         = 71        ; IF_TYPE_IEEE80211
*MediaType      = 16        ; NdisMediumNative802_11
*PhysicalMediaType = 9      ; NdisPhysicalMediumNative802_11
Include         = netvwifibus.inf, machine.inf
Needs           = VWiFiBus.CopyFiles

[ATHR_DEV_OS61_H9565.ndi.NTamd64.Services]
AddService = athr, 2, atheros.Service, atheros.EventLog
Include    = netvwifibus.inf
Needs      = VWiFiBus.Services

[ATHR_DEV_OS61_H9565.ndi.NTamd64.HW]
Include = netvwifibus.inf
Needs   = PciASPMOptIn, VWiFiBus.PnPFilterRegistration

[ATHR_DEV_OS61_HNFA335.ndi.NTamd64]
Characteristics = 0x84
BusType         = 5
AddReg          = atheros_os61.reg, atheros11n.reg, htAdhoc.reg, aphroditeant.reg, aphrodite_coex.reg, ledcontrol8acthi.reg, ConnectionFailure.reg, aphroditeantdiv.reg, amp_default.reg, InvalidRateIgnore.reg
DelReg          = atheros.DelReg
CopyFiles       = atheros.CopyFiles
*IfType         = 71        ; IF_TYPE_IEEE80211
*MediaType      = 16        ; NdisMediumNative802_11
*PhysicalMediaType = 9      ; NdisPhysicalMediumNative802_11
Include         = netvwifibus.inf, machine.inf
Needs           = VWiFiBus.CopyFiles

[ATHR_DEV_OS61_HNFA335.ndi.NTamd64.Services]
AddService = athr, 2, atheros.Service, atheros.EventLog
Include    = netvwifibus.inf
Needs      = VWiFiBus.Services

[ATHR_DEV_OS61_HNFA335.ndi.NTamd64.HW]
Include = netvwifibus.inf
Needs   = PciASPMOptIn, VWiFiBus.PnPFilterRegistration

[ATHR_DEV_OS61_178310CF.ndi.NTamd64]
Characteristics = 0x84
BusType         = 5
AddReg          = atheros_os61.reg, atheros11n.reg, 5416.bandselect.reg, customer1ani.reg, adhocchannelselect.reg, customer1roamPolicy.reg, smpsDynamic.reg, jupiter2ant.reg, htAdhocdisable.reg, customer1GreenTx.reg, SleepTimePwrSaveMax2000.reg, swBeaconProcess.reg
DelReg          = atheros.DelReg
CopyFiles       = atheros.CopyFiles
*IfType         = 71        ; IF_TYPE_IEEE80211
*MediaType      = 16        ; NdisMediumNative802_11
*PhysicalMediaType = 9      ; NdisPhysicalMediumNative802_11
Include         = netvwifibus.inf, machine.inf
Needs           = VWiFiBus.CopyFiles

[ATHR_DEV_OS61_178310CF.ndi.NTamd64.Services]
AddService = athr, 2, atheros.Service, atheros.EventLog
Include    = netvwifibus.inf
Needs      = VWiFiBus.Services

[ATHR_DEV_OS61_178310CF.ndi.NTamd64.HW]
Include = netvwifibus.inf
Needs   = PciASPMOptIn, VWiFiBus.PnPFilterRegistration

[ATHR_DEV_OS61_180E10CF.ndi.NTamd64]
Characteristics = 0x84
BusType         = 5
AddReg          = atheros_os61.reg, atheros11n.reg, 5416.bandselect.reg, customer1ani.reg, adhocchannelselect.reg, customer1roamPolicy.reg, smpsDynamic.reg, jupiter2ant.reg, htAdhocdisable.reg, customer1GreenTx.reg, j21swwow.reg, SleepTimePwrSaveMax2000.reg, swBeaconProcess.reg
DelReg          = atheros.DelReg
CopyFiles       = atheros.CopyFiles
*IfType         = 71        ; IF_TYPE_IEEE80211
*MediaType      = 16        ; NdisMediumNative802_11
*PhysicalMediaType = 9      ; NdisPhysicalMediumNative802_11
Include         = netvwifibus.inf, machine.inf
Needs           = VWiFiBus.CopyFiles

[ATHR_DEV_OS61_180E10CF.ndi.NTamd64.Services]
AddService = athr, 2, atheros.Service, atheros.EventLog
Include    = netvwifibus.inf
Needs      = VWiFiBus.Services

[ATHR_DEV_OS61_180E10CF.ndi.NTamd64.HW]
Include = netvwifibus.inf
Needs   = PciASPMOptIn, VWiFiBus.PnPFilterRegistration

[ATHR_DEV_OS61_3117104D.ndi.NTamd64]
Characteristics = 0x84
BusType         = 5
AddReg          = atheros_os61.reg, atheros11n.reg, 5416.bandselect.reg, customer1ani.reg, adhocchannelselect.reg, customer1roamPolicy.reg, smpsDynamic.reg, jupiter2ant.reg, htAdhocdisable.reg, customer1GreenTx.reg, j21swwow.reg, SleepTimePwrSaveMax2000.reg
DelReg          = atheros.DelReg
CopyFiles       = atheros.CopyFiles
*IfType         = 71        ; IF_TYPE_IEEE80211
*MediaType      = 16        ; NdisMediumNative802_11
*PhysicalMediaType = 9      ; NdisPhysicalMediumNative802_11
Include         = netvwifibus.inf, machine.inf
Needs           = VWiFiBus.CopyFiles

[ATHR_DEV_OS61_3117104D.ndi.NTamd64.Services]
AddService = athr, 2, atheros.Service, atheros.EventLog
Include    = netvwifibus.inf
Needs      = VWiFiBus.Services

[ATHR_DEV_OS61_3117104D.ndi.NTamd64.HW]
Include = netvwifibus.inf
Needs   = PciASPMOptIn, VWiFiBus.PnPFilterRegistration
AddReg  = MSI.reg

[ATHR_DEV_OS61_3027185F.ndi.NTamd64]
Characteristics = 0x84
BusType         = 5
AddReg          = atheros_os61.reg, atheros11n.reg, htAdhoc.reg, aphroditeant2.reg, aphrodite_coex2.reg, ledcontrol8.reg, ConnectionFailure.reg, aphroditeantdiv2.reg
DelReg          = atheros.DelReg
CopyFiles       = atheros.CopyFiles
*IfType         = 71        ; IF_TYPE_IEEE80211
*MediaType      = 16        ; NdisMediumNative802_11
*PhysicalMediaType = 9      ; NdisPhysicalMediumNative802_11
Include         = netvwifibus.inf, machine.inf
Needs           = VWiFiBus.CopyFiles

[ATHR_DEV_OS61_3027185F.ndi.NTamd64.Services]
AddService = athr, 2, atheros.Service, atheros.EventLog
Include    = netvwifibus.inf
Needs      = VWiFiBus.Services

[ATHR_DEV_OS61_3027185F.ndi.NTamd64.HW]
Include = netvwifibus.inf
Needs   = PciASPMOptIn, VWiFiBus.PnPFilterRegistration

[ATHR_DEV_OS61_04031B9A.ndi.NTamd64]
Characteristics = 0x84
BusType         = 5
AddReg          = atheros_os61.reg, atheros11n.reg, htAdhoc.reg, triggerlevelkiteonly.reg, c3war.reg, ledcontrol9.reg
DelReg          = atheros.DelReg
CopyFiles       = atheros.CopyFiles
*IfType         = 71            ; IF_TYPE_IEEE80211
*MediaType      = 16            ; NdisMediumNative802_11
*PhysicalMediaType = 9          ; NdisPhysicalMediumNative802_11
Include         = netvwifibus.inf, machine.inf
Needs           = VWiFiBus.CopyFiles

[ATHR_DEV_OS61_04031B9A.ndi.NTamd64.Services]
AddService = athr, 2, atheros.Service, atheros.EventLog
Include    = netvwifibus.inf
Needs      = VWiFiBus.Services

[ATHR_DEV_OS61_04031B9A.ndi.NTamd64.HW]
Include = netvwifibus.inf
Needs   = VWiFiBus.PnPFilterRegistration

;;End of Others Section

[atheros_os61.reg]
HKR, Ndi,                           Service,    0, "athr"
HKR, Ndi\Interfaces,                UpperRange, 0, "ndis5"
HKR, Ndi\Interfaces,                LowerRange, 0, "wlan,ethernet,vwifi"

[atheros11n.reg]
HKR, Ndi\params\*ReceiveBuffers,    ParamDesc,  0, "%ReceiveBuffers%"
HKR, Ndi\params\*ReceiveBuffers,    default,    0, "256"
HKR, Ndi\params\*ReceiveBuffers,    min,        0, "1"
HKR, Ndi\params\*ReceiveBuffers,    max,        0, "00000512"
HKR, Ndi\params\*ReceiveBuffers,    step,       0, "1"
HKR, Ndi\params\*ReceiveBuffers,    Base,       0, "10"
HKR, Ndi\params\*ReceiveBuffers,    type,       0, "int"
HKR, Ndi\params\*TransmitBuffers,   ParamDesc,  0, "%TransmitBuffers%"
HKR, Ndi\params\*TransmitBuffers,   default,    0, "512"
HKR, Ndi\params\*TransmitBuffers,   min,        0, "1"
HKR, Ndi\params\*TransmitBuffers,   max,        0, "00000512"
HKR, Ndi\params\*TransmitBuffers,   step,       0, "1"
HKR, Ndi\params\*TransmitBuffers,   Base,       0, "10"
HKR, Ndi\params\*TransmitBuffers,   type,       0, "int"
HKR, Ndi\params\shortPreamble,      ParamDesc,  0,  %shortPreamble%
HKR, Ndi\params\shortPreamble,      Base,       0,  "10"
HKR, Ndi\params\shortPreamble,      default,    0,  "1"
HKR, Ndi\params\shortPreamble,      type,       0,  "enum"
HKR, Ndi\params\shortPreamble\enum, "1",        0,  %shortPreambleEnable%
HKR, Ndi\params\shortPreamble\enum, "0",        0,  %shortPreambleDisable%
HKR, Ndi\params\scanTimeValid,      ParamDesc,  0,  %scanTimeValid%
HKR, Ndi\params\scanTimeValid,      default,    0,  "60"
HKR, Ndi\params\scanTimeValid,      min,        0,  "20"
HKR, Ndi\params\scanTimeValid,      max,        0,  "120"
HKR, Ndi\params\scanTimeValid,      step,       0,  "5"
HKR, Ndi\params\scanTimeValid,      base,       0,  "10"
HKR, Ndi\params\scanTimeValid,      type,       0,  "int"

;/* Enable these if VLAN or 802.1p is to be enabled */
;HKR, Ndi\Params\*PriorityVLANTag,  ParamDesc,  , %PriorityVLAN%
;HKR, Ndi\Params\*PriorityVLANTag,  default,    , "3"
;HKR, Ndi\Params\*PriorityVLANTag,  type,       , "enum"
;HKR, Ndi\Params\*PriorityVLANTag\enum, 0,      , %PriorityVLANDisabled%
;HKR, Ndi\Params\*PriorityVLANTag\enum, 1,      , %PriorityEnabled%
;HKR, Ndi\Params\*PriorityVLANTag\enum, 2,      , %VLANEnabled%
;HKR, Ndi\Params\*PriorityVLANTag\enum, 3,      , %PriorityVLANEnabled%

[atheros.reg]
HKR, Ndi\params\*ReceiveBuffers,    ParamDesc,  0, "%ReceiveBuffers%"
HKR, Ndi\params\*ReceiveBuffers,    default,    0, "256"
HKR, Ndi\params\*ReceiveBuffers,    min,        0, "1"
HKR, Ndi\params\*ReceiveBuffers,    max,        0, "00000512"
HKR, Ndi\params\*ReceiveBuffers,    step,       0, "1"
HKR, Ndi\params\*ReceiveBuffers,    Base,       0, "10"
HKR, Ndi\params\*ReceiveBuffers,    type,       0, "int"
HKR, Ndi\params\*TransmitBuffers,   ParamDesc,  0, "%TransmitBuffers%"
HKR, Ndi\params\*TransmitBuffers,   default,    0, "256"
HKR, Ndi\params\*TransmitBuffers,   min,        0, "1"
HKR, Ndi\params\*TransmitBuffers,   max,        0, "00000512"
HKR, Ndi\params\*TransmitBuffers,   step,       0, "1"
HKR, Ndi\params\*TransmitBuffers,   Base,       0, "10"
HKR, Ndi\params\*TransmitBuffers,   type,       0, "int"
HKR, Ndi\params\shortPreamble,      ParamDesc,  0,  %shortPreamble%
HKR, Ndi\params\shortPreamble,      Base,       0,  "10"
HKR, Ndi\params\shortPreamble,      default,    0,  "1"
HKR, Ndi\params\shortPreamble,      type,       0,  "enum"
HKR, Ndi\params\shortPreamble\enum, "1",        0,  %shortPreambleEnable%
HKR, Ndi\params\shortPreamble\enum, "0",        0,  %shortPreambleDisable%
HKR, Ndi\params\scanTimeValid,      ParamDesc,  0,  %scanTimeValid%
HKR, Ndi\params\scanTimeValid,      default,    0,  "60"
HKR, Ndi\params\scanTimeValid,      min,        0,  "20"
HKR, Ndi\params\scanTimeValid,      max,        0,  "120"
HKR, Ndi\params\scanTimeValid,      step,       0,  "5"
HKR, Ndi\params\scanTimeValid,      base,       0,  "10"
HKR, Ndi\params\scanTimeValid,      type,       0,  "int"

[atheros.DelReg]
HKR, Interrupt Management
HKR, Ndi\IHVExtensions
HKR, Ndi\params,MapRegisters,0x2000
HKR, Ndi\params,radioEnable,0x2000
HKR, Ndi\params,sleepMode,0x2000
HKR, Ndi\params\*TransmitBuffers
HKR, Ndi\params\ampEnable
HKR, Ndi\params\authTypeUseOnly
HKR, Ndi\params\ignore11dBeacon
HKR, Ndi\params\smpsDynamic
HKR, Ndi\params\tpc
HKR,,*ReceiveBuffers
HKR,,*SelectiveSuspend
HKR,,*SSIdleTimeout
HKR,,*TransmitBuffers
HKR,,11nTXRetry
HKR,,abolt
HKR,,ActivityLEDFunc
HKR,,adhocBand
HKR,,AdhocModeSelect
HKR,,AdjustRSSI
HKR,,aggrLimit
HKR,,aggrProtDuration
HKR,,aggrProtEnable
HKR,,aggrProtMax
HKR,,aggrSubframes
HKR,,aifs
HKR,,ampDbgWdmEnable
HKR,,ampEnable
HKR,,ampFilterName
HKR,,ampGUID
HKR,,ampHtEnable
HKR,,ampIgnoreNonERP
HKR,,ampSelChannel
HKR,,ampThruTest
HKR,,ampTxopLimit
HKR,,analogShiftRegDelay
HKR,,antCtrlComm2gSwitchEnable
HKR,,antDivFastDivBias
HKR,,antDivLowRssiCfg
HKR,,antennaSwitch
HKR,,antennaSwitchSwap
HKR,,AthDebugLevel
HKR,,ATHP2pCertificate
HKR,,authTypeUseOnly
HKR,,AutoCVUpdate
HKR,,AwakeTimePerf
HKR,,AwakeTimePwrSave
HKR,,AwakeTimePwrSaveMax
HKR,,BeaconFilterEnable
HKR,,beaconInterval
HKR,,bkScanEnable
HKR,,bkScanMaxDeferralTime
HKR,,bssAgingPeriod
HKR,,bssType
HKR,,btActiveGpioSelect
HKR,,btActivePolarity
HKR,,btCoexAFHSideBand
HKR,,btCoexAgent
HKR,,btCoexAggrLimit
HKR,,btCoexAntDivEnable
HKR,,btCoexConCurTx
HKR,,btCoexConcurTxCfg
HKR,,btCoexdisablePKDET
HKR,,btCoexDisablePTA
HKR,,btCoexDisablePTACfg
HKR,,btCoexDivDefVal
HKR,,btCoexEnable
HKR,,btCoexEnhanceA2DP
HKR,,btCoexLowACKPwr
HKR,,btCoexMiscCfg
HKR,,btCoexRSSIModeProfile
HKR,,btCoexStompA2DPCfg
HKR,,btCoexStompSCOCfg
HKR,,btCoexStompType
HKR,,btCoexWeight
HKR,,btDutyCycle
HKR,,btModule
HKR,,btPeriod
HKR,,btPriorityGpioSelect
HKR,,btScheme
HKR,,btSingleAnt
HKR,,btWlanIsolation
HKR,,BusConfig
HKR,,c3WarEnable
HKR,,c3WarTimer2
HKR,,c3WarTimerPeriod
HKR,,CalibrationTime
HKR,,capLinkSp
HKR,,cckTrigHigh
HKR,,cckTrigLow
HKR,,cckWeakSigThr
HKR,,ccode
HKR,,ccxDebugLevel
HKR,,ccxEnable
HKR,,CCXUpdateXmitStatus
HKR,,cfpignore
HKR,,CheckForHangInterval
HKR,,clearListOnScan
HKR,,clist
HKR,,cmdRegister
HKR,,CMQ
HKR,,ConnectionLEDFunc
HKR,,crashOnBug
HKR,,cservDebugLevel
HKR,,ctlignore
HKR,,CVTimeOut
HKR,,CVUpdatePER
HKR,,cwmEnable
HKR,,cwmExtBusyThreshold
HKR,,cwmExtOffset
HKR,,cwmExtProtMode
HKR,,cwmExtProtSpacing
HKR,,cwmIgnoreExtCCA
HKR,,cwmin
HKR,,cwmMode
HKR,,D3D0IsrConfig
HKR,,d3forcel1disable.reg
HKR,,d3forcel1disablekite.reg
HKR,,d3forcel1disablekite1.reg
HKR,,debugMode
HKR,,defaultAntCfg
HKR,,defaultApChannel
HKR,,defaultApPhyMode
HKR,,defaultIbssChannel
HKR,,defaultKey
HKR,,delayIndicateComplete
HKR,,delayNWSleep
HKR,,disable2040Coexist
HKR,,disableAdHocAIACCI
HKR,,disableHT20ShortGI
HKR,,DisableLED01
HKR,,disableRFSilent
HKR,,disableStopSoftAPWow
HKR,,disabletidqueue
HKR,,disableTurboG
HKR,,disableWakeOnApLost
HKR,,DmaStopWaitTime
HKR,,EAPOLConfig
HKR,,EapolKey4DelayMs
HKR,,edmaStopRecvDelay
HKR,,enable2GHzHt40Cap
HKR,,enableANI
HKR,,enableAp80211d
HKR,,enableFCC3
HKR,,enableReportNdisHWWowCap
HKR,,EnableSmartGO
HKR,,EncryptionAlg
HKR,,EnhanceCCXFastRoam
HKR,,extapEnable
HKR,,extapUapsdEnable
HKR,,extAttenMarginCfg
HKR,,extendedChanMode
HKR,,extLnaCtlGpio
HKR,,fakeAIFSN4WFA
HKR,,fastChannelChange
HKR,,fastClockEnable
HKR,,FilterOutCCKRateEnable
HKR,,firStepLvl
HKR,,forceBias
HKR,,forceBiasAuto
HKR,,forcePpmEnable
HKR,,forcePpmUpdateTimeout
HKR,,forceSmartAntenna
HKR,,forceSTDMagicOffload
HKR,,FragThreshold
HKR,,fstEnable
HKR,,ftEnable
HKR,,genTimerIsrCheckIntval
HKR,,goprefersingle
HKR,,gpioFunc0ActHi
HKR,,gpioFunc1ActHi
HKR,,gpioFunc2ActHi
HKR,,gpioLedCustom
HKR,,gpioPinFunc0
HKR,,gpioPinFunc1
HKR,,gpioPinFunc2
HKR,,GreenTx
HKR,,halaifs
HKR,,halBeaconFilterInterval
HKR,,halBuffaloApWar
HKR,,halCalReuse
HKR,,halCsdValue
HKR,,halDebugComponents
HKR,,halFullResetWarEnable
HKR,,halIrstEnable
HKR,,halIrstNormalWakeUpTimeout
HKR,,halKeepAwakeStrongRssi
HKR,,halLGRetry
HKR,,halMitiShiftValue
HKR,,halModifyRxGain2G
HKR,,halModifyRxGain5G
HKR,,halNlo
HKR,,halPcieClockReq
HKR,,halPcieDetach
HKR,,halPcieL1SKPEnable
HKR,,halPciePowerReset
HKR,,halPciePowerSaveEnable
HKR,,halPcieRestore
HKR,,halPcieSerDesWrite
HKR,,halPcieWaen
HKR,,halPllPwrSave
HKR,,halRestoreSettingCount
HKR,,halRttCtrl
HKR,,halShortRetry
HKR,,halusbForceWake
HKR,,halUseBTWakeUp
HKR,,halWakeUpCfg
HKR,,halWakeupDelay
HKR,,halWowNFRTC
HKR,,halWowOffload
HKR,,halWowOffloadBtTimeout
HKR,,halWowParameter
HKR,,halWowWDTPeriod
HKR,,hsEnable
HKR,,ht40AdhocEnable
HKR,,htAdhocAggrEnable
HKR,,htAdhocEnable
HKR,,htDupIeEnable
HKR,,htEnable
HKR,,htEnableWepTkip
HKR,,htVendorIeEnable
HKR,,hwMfpSupport
HKR,,HwTxRetries
HKR,,IdleConfiguration
HKR,,ignore11dBeacon
HKR,,ignoreDynamicHalt
HKR,,indicateRxLinkSpeed
HKR,,internalScanFlags
HKR,,internalScanMaxChannels
HKR,,internalScanMaxOffchannelTime
HKR,,internalScanMaxScanTime
HKR,,internalScanMode
HKR,,intrMitigationRxEnable
HKR,,intrMitigationTxEnable
HKR,,InvalidRateIgnore
HKR,,isMagpie
HKR,,K2ScanPartialReset
HKR,,ktStackSize
HKR,,lastScanTS
HKR,,ldpcEnable
HKR,,LinkLEDDefaultOn
HKR,,LinkLEDFunc
HKR,,lnaDivUseBtAntEnable
HKR,,LowerHTTxGain
HKR,,MapRegisters
HKR,,maxBssListIdicateSize
HKR,,maxDwellTimeActive
HKR,,maxDwellTimePassive
HKR,,maxP2PClientBmissCount
HKR,,maxRestTime
HKR,,maxRoamDuration
HKR,,maxRxUrb
HKR,,maxScanInterval
HKR,,maxTxEpaolRetry
HKR,,maxTxMgmtRetry
HKR,,maxTxStreamPkgNum
HKR,,maxTxUrb
HKR,,maxVapPendingTxNBL
HKR,,mccStaTimeSlotVovi1
HKR,,mci_int_defer
HKR,,mciConfig
HKR,,MediumTimeUsed
HKR,,minDwellTimeActive
HKR,,minDwellTimePassive
HKR,,minRestTime
HKR,,mlmeDebugLevel
HKR,,MPCheckForHangEnabled
HKR,,MPDUExchangeTimeVI
HKR,,MPDUExchangeTimeVO
HKR,,MPGlobalDebugComponents
HKR,,MPGlobalDebugLevel
HKR,,MPGlobalDebugPrint
HKR,,MPSendsHaveStalledPeriod
HKR,,MPSendsStalledDoInternalReset
HKR,,MSISupported
HKR,,NetBand
HKR,,NetworkAddress
HKR,,noascan
HKR,,NOAStartAheadus
HKR,,noHtCapInSafeMode
HKR,,noiseImmunityLvl
HKR,,NonAggrMaxTxqDepth
HKR,,numSwRetries
HKR,,ocsEnable
HKR,,OCSPauseLmac
HKR,,ocsScanPauseMs
HKR,,ofdmTrigHigh
HKR,,ofdmTrigLow
HKR,,ofdmWeakSigDet
HKR,,oidDebugLevel
HKR,,OKCRoaming
HKR,,OverrideTxOk
HKR,,overRideTxPower
HKR,,P2pDevEnable
HKR,,p2pGoUapsdEnable
HKR,,p2pUsePassiveChan
HKR,,paprdEnable
HKR,,pausetimeout
HKR,,pciCacheLineSize
HKR,,pciDetectEnable
HKR,,pcieAspm
HKR,,pcieDisableAspmOnRfWake
HKR,,pciForceWake
HKR,,pDeweight
HKR,,periodicScanEnable
HKR,,PMConfig
HKR,,PMFstatus
HKR,,powerDebugLevel
HKR,,prefBssid1
HKR,,prefBssid2
HKR,,prefBssid3
HKR,,prefBssid4
HKR,,PriorityForEAP
HKR,,privacyInvoked
HKR,,prohibitAny
HKR,,PsActivityCheckInterval
HKR,,psntfdelay
HKR,,psPollEnabled
HKR,,QoS
HKR,,radioEnable
HKR,,radioEnableInterval
HKR,,rateCtrlEnable
HKR,,rateCtrlTxFastDrop
HKR,,ReconnectAfterAssocFail
HKR,,RecoveryEnable
HKR,,RefreshScan
HKR,,regCapBits
HKR,,regdmn
HKR,,reserveScanTable
HKR,,resmgrLowPriority
HKR,,rfKillDelayDetect
HKR,,rifsAggrDiv
HKR,,roamDebugLevel
HKR,,roamEnable
HKR,,roamPolicy
HKR,,roamRateA
HKR,,roamRateB
HKR,,roamRateBOnly
HKR,,roamRssiA
HKR,,roamRssiB
HKR,,roamRssiBOnly
HKR,,rrmEnable
HKR,,rssiAdjust
HKR,,rssiThrHigh
HKR,,rssiThrLow
HKR,,rtsProtectionEnable
HKR,,RTSThreshold
HKR,,rxAggrEnable
HKR,,rxChainDetect
HKR,,rxChainDetectDeltaA
HKR,,rxChainDetectDeltaG
HKR,,rxChainDetectRef
HKR,,rxChainDetectThreshA
HKR,,rxChainDetectThreshG
HKR,,rxChainMask
HKR,,rxChainMaskLegacy
HKR,,rxDebugLevel
HKR,,rxRifsEnable
HKR,,rxRifsSkipThresh
HKR,,rxRifsTimeout
HKR,,saFastDivDisable
HKR,,saFixedAltLna
HKR,,saFixedMainLna
HKR,,saFixedSwitchComR
HKR,,saFixedSwitchComT
HKR,,scanDataIdleTime
HKR,,scanParamsConfigEnable
HKR,,scanTimePreSleep
HKR,,scanTimeValid
HKR,,scanType
HKR,,serializeRegMode
HKR,,sharedGpioFunc0
HKR,,shMemAllocRetry
HKR,,shortPreamble
HKR,,showAntDivDbgInfo
HKR,,showDynamicTxRate
HKR,,singleWriteKC
HKR,,sleepMode
HKR,,SleepTimePerf
HKR,,sleepTimePostScan
HKR,,SleepTimePwrSave
HKR,,SleepTimePwrSaveMax
HKR,,slowAntDivEnable
HKR,,slowAntDivMinDwellTime
HKR,,slowAntDivSettleTime
HKR,,slowAntDivThreshold
HKR,,SmartNetEnable
HKR,,smbiosAuthenticationEnable
HKR,,smbiosAuthenticationPattern
HKR,,smbiosEnable
HKR,,SmeEnable
HKR,,smpsDataThreshold
HKR,,smpsDynamic
HKR,,smpsRssiThreshold
HKR,,softApResetDelayMs
HKR,,softLEDEnable
HKR,,spectralDropPacket
HKR,,spectralEnable
HKR,,spectralFFTPeriod
HKR,,spectralSSCount
HKR,,spectralSSPeriod
HKR,,spurImmunityLvl
HKR,,ssid
HKR,,ssid2
HKR,,ssid3
HKR,,stbcEnable
HKR,,surpriseRemovalOk
HKR,,swapDefaultLED
HKR,,swBeaconProcess
HKR,,SWCVTimeOut
HKR,,SwTxRetryScale
HKR,,ThirdPortEnable
HKR,,TLEnable
HKR,,tpc
HKR,,translateNullSsid
HKR,,transmitRateMax
HKR,,TransmitRateSet
HKR,,TransmitRetrySet
HKR,,TSF2Enable
HKR,,txAggrEnable
HKR,,txAmsduEnable
HKR,,TxBFCtl
HKR,,txChainMask
HKR,,txChainMaskLegacy
HKR,,txCoalescingEnable
HKR,,txDebugLevel
HKR,,txRifsEnable
HKR,,txStreamL1AggNumThr
HKR,,txStreamL1PkgNumThr
HKR,,txTrigLevelMax
HKR,,uapsdEnabledBE
HKR,,uapsdEnabledBK
HKR,,uapsdEnabledVI
HKR,,uapsdEnabledVO
HKR,,usbEnhanceInstantConnect
HKR,,usbForceWake
HKR,,usbInstantDelayMs
HKR,,usbSSuspendEnable
HKR,,usbStaWhqlEnable
HKR,,usbWmiRetry
HKR,,userCoverageClass
HKR,,VistaApEnable
HKR,,voviEnableBitMap 
HKR,,wakeOnTsfChanged
HKR,,wapiEnable
HKR,,watchdogPollingInterval
HKR,,wb225SwGreenTxThres1
HKR,,wb225SwGreenTxThres2
HKR,,wfdAllowExternalScan
HKR,,WFDCapability
HKR,,WfdChanUpdate
HKR,,WfdForceSetOpChan
HKR,,WfdGoPrefer2G
HKR,,WfdListenChan
HKR,,WfdOnChanTime
HKR,,WfdOpChan
HKR,,WfdPreferChanTimeout
HKR,,WfdRegClass
HKR,,WiFiLEDEnable
HKR,,wlanActiveGpioSelect
HKR,,wmeEnabled
HKR,,wmmacEnable
HKR,,wmmPSTest
HKR,,wModeSelect
HKR,,wowEnable
HKR,,WowEnablePME
HKR,,wpsBtnSupport
HKR,,wpsButtonGpio
HKR,,wsis5
HKR,,xpblevel5


[expresscardaspmoff.reg]
HKR, ,                                  pciDetectEnable,                0x00002,  "2"
HKR, ,                                  halPciePowerSaveEnable,         0x00002,  "1"
HKR, ,                                  pcieAspm,                       0x00002,  "0"

[rfKillDelayDetect.reg]
HKR, ,                                  rfKillDelayDetect,              0x00002,  "1"

[d3hot.reg] 
HKR, ,                                  halPciePowerReset,              0x00002,  "0"
HKR, ,                                  halPcieRestore,                 0x00002,  "1"

[enableswretry] 
HKR, ,                                  numSwRetries,                   0x00002,  "4"

[interruptpolling.reg]
HKR, ,                                  isrPollInterval,                0x00002,  "100"

[pcibusconfig.reg]
HKR, ,                                  BusConfig,                      0x00002,  "0"
HKR, ,                                  serializeRegMode,               0x00002,  "2"

[serializing.reg]
HKR, ,                                  serializeRegMode,               0x00002,  "1"

[bandselect.reg]
HKR, Ndi\params\NetBand,                ParamDesc,                      0,        %WirelessMode%
HKR, Ndi\params\NetBand,                Base,                           0,        "10"
HKR, Ndi\params\NetBand,                default,                        0,        "1647"
HKR, Ndi\params\NetBand,                type,                           0,        "enum"
HKR, Ndi\params\NetBand\enum,           "1647",                         0,        %Auto%
HKR, Ndi\params\NetBand\enum,           "1603",                         0,        %5GOnly%
HKR, Ndi\params\NetBand\enum,           "44",                           0,        %2GOnly%

[roamthreshA.reg]
HKR, Ndi\params\roamRssiA,              ParamDesc,                      0,        %roamRssiA%
HKR, Ndi\params\roamRssiA,              default,                        0,        "15"
HKR, Ndi\params\roamRssiA,              min,                            0,        "1"
HKR, Ndi\params\roamRssiA,              max,                            0,        "95"
HKR, Ndi\params\roamRssiA,              step,                           0,        "1"
HKR, Ndi\params\roamRssiA,              base,                           0,        "10"
HKR, Ndi\params\roamRssiA,              type,                           0,        "int"

[ignore11d.reg]
HKR,NDI\params\ignore11dBeacon,         ParamDesc,,                               %11DModeSwitch%
HKR,NDI\params\ignore11dBeacon,         type,,                                    "enum"
HKR,NDI\params\ignore11dBeacon,         Default,,                                 "1"
HKR,NDI\params\ignore11dBeacon\enum,    0,,                                       %Enable%
HKR,NDI\params\ignore11dBeacon\enum,    1,,                                       %Disable%

;[radioswitch.reg]
;HKR, Ndi\params\radioEnable,            ParamDesc,                      0,        %radioEnable%
;HKR, Ndi\params\radioEnable,            Base,                           0,        "10"
;HKR, Ndi\params\radioEnable,            default,                        0,        "1"
;HKR, Ndi\params\radioEnable,            type,                           0,        "enum"
;HKR, Ndi\params\radioEnable\enum,       "1",                            0,        %radioEnableOn%
;HKR, Ndi\params\radioEnable\enum,       "0",                            0,        %radioEnableOff%

[overridetxok.reg]
HKR, ,                                  OverrideTxOk,                   0x00002,  "1"

[adhocchannelselect.reg]
HKR, Ndi\params\defaultIbssChannel,     ParamDesc,                      0,        %adhocchannel%
HKR, Ndi\params\defaultIbssChannel,     default,                        0,        "10"
HKR, Ndi\params\defaultIbssChannel,     min,                            0,        "1"
HKR, Ndi\params\defaultIbssChannel,     max,                            0,        "11"
HKR, Ndi\params\defaultIbssChannel,     step,                           0,        "1"
HKR, Ndi\params\defaultIbssChannel,     base,                           0,        "10"
HKR, Ndi\params\defaultIbssChannel,     type,                           0,        "int"

[5416.bgnxb.reg]
HKR, ,                                  NetBand,                        0x00002,  "26636"
HKR, ,                                  wmodeselect,                    0x00002,  "26636"

[5416.bandselect.reg]
HKR, Ndi\params\NetBand,                ParamDesc,                      0,  %WirelessMode%
HKR, Ndi\params\NetBand,                Base,                           0,  "10"
HKR, Ndi\params\NetBand,                default,                        0,  "130671"
HKR, Ndi\params\NetBand,                type,                           0,  "enum"
HKR, Ndi\params\NetBand\enum,           "130671",                       0,  %Auto%
HKR, Ndi\params\NetBand\enum,           "104003",                       0,  %5GOnly%
HKR, Ndi\params\NetBand\enum,           "26668",                        0,  %2GOnly%

[wirelessmodeselectCompex.reg]
HKR, Ndi\params\NetBand,                ParamDesc,                      0,  %WirelessMode%
HKR, Ndi\params\NetBand,                Base,                           0,  "10"
HKR, Ndi\params\NetBand,                default,                        0,  "130671"
HKR, Ndi\params\NetBand,                type,                           0,  "enum"
HKR, Ndi\params\NetBand\enum,           "1",                            0,  %11AOnly%
HKR, Ndi\params\NetBand\enum,           "104003",                       0,  %11ANOnly%
HKR, Ndi\params\NetBand\enum,           "12",                           0,  %11BGOnly%
HKR, Ndi\params\NetBand\enum,           "26668",                        0,  %11BGNOnly%
HKR, Ndi\params\NetBand\enum,           "130671",                       0,  %11ABGN%

[wirelessmodeselectkite.reg]
HKR, Ndi\params\NetBand,                ParamDesc,                      0,  %WirelessMode%
HKR, Ndi\params\NetBand,                Base,                           0,  "10"
HKR, Ndi\params\NetBand,                default,                        0,  "26636"
HKR, Ndi\params\NetBand,                type,                           0,  "enum"
HKR, Ndi\params\NetBand\enum,           "26636",                        0,  %WirelessModeAuto%
HKR, Ndi\params\NetBand\enum,           "12",                           0,  %WirelessMode11bgOnly%

[acer.bandselect.reg]
HKR, Ndi\params\NetBand,                ParamDesc,                      0,  %WirelessMode%
HKR, Ndi\params\NetBand,                Base,                           0,  "10"
HKR, Ndi\params\NetBand,                default,                        0,  "130671"
HKR, Ndi\params\NetBand,                type,                           0,  "enum"
HKR, Ndi\params\NetBand\enum,           "130671",                       0,  "802.11a/b/g/n"
HKR, Ndi\params\NetBand\enum,           "26668",                        0,  "802.11b/g/n"
HKR, Ndi\params\NetBand\enum,           "26664",                        0,  "802.11g/n"
HKR, Ndi\params\NetBand\enum,           "104003",                       0,  "802.11a/n"

[wirelessmode.all.reg]
HKR, Ndi\params\NetBand,                ParamDesc,                      0,  %WirelessMode%
HKR, Ndi\params\NetBand,                Base,                           0,  "10"
HKR, Ndi\params\NetBand,                default,                        0,  "130671"
HKR, Ndi\params\NetBand,                type,                           0,  "enum"
HKR, Ndi\params\NetBand\enum,           "4",                            0,  "1. b only"
HKR, Ndi\params\NetBand\enum,           "40",                           0,  "2. g only"
HKR, Ndi\params\NetBand\enum,           "44",                           0,  "3. b/g"
HKR, Ndi\params\NetBand\enum,           "26664",                        0,  "4. g/n"
HKR, Ndi\params\NetBand\enum,           "26668",                        0,  "5. b/g/n"
HKR, Ndi\params\NetBand\enum,           "1",                            0,  "6. a only"
HKR, Ndi\params\NetBand\enum,           "104003",                       0,  "7. a/n"
HKR, Ndi\params\NetBand\enum,           "130671",                       0,  "8. a/b/g/n"
HKR, Ndi\params\NetBand\enum,           "130665",                       0,  "9. a/g/n"

[wirelessmode.2g.reg]
HKR, Ndi\params\NetBand,                ParamDesc,                      0,  %WirelessMode%
HKR, Ndi\params\NetBand,                Base,                           0,  "10"
HKR, Ndi\params\NetBand,                default,                        0,  "26668"
HKR, Ndi\params\NetBand,                type,                           0,  "enum"
HKR, Ndi\params\NetBand\enum,           "4",                       		0,  "1. b only"
HKR, Ndi\params\NetBand\enum,           "40",                       	0,  "2. g only"
HKR, Ndi\params\NetBand\enum,           "44",                       	0,  "3. b/g"
HKR, Ndi\params\NetBand\enum,           "26664",                       	0,  "4. g/n"
HKR, Ndi\params\NetBand\enum,           "26668",                       	0,  "5. b/g/n"

[acer.preferredband.reg]
HKR, Ndi\params\PreferredBand,          ParamDesc,                      0,  %PreferredBand%
HKR, Ndi\params\PreferredBand,          Base,                           0,  "10"
HKR, Ndi\params\PreferredBand,          default,                        0,  "0"
HKR, Ndi\params\PreferredBand,          type,                           0,  "enum"
HKR, Ndi\params\PreferredBand\enum,     "0",                            0,  "1. No Preference"
HKR, Ndi\params\PreferredBand\enum,     "1",                            0,  "2. Prefer 2.4GHz Band"
HKR, Ndi\params\PreferredBand\enum,     "2",                            0,  "3. Prefer 5.2GHz Band"

[5416.antennacontrols.reg] 
HKR, ,                                  rxChainMask,                    0x00002,  "7"
;HKR, ,                                  txChainMaskLegacy,              0x00002,  "5"
HKR, ,                                  rxChainMaskLegacy,              0x00002,  "7"
HKR, ,                                  rxChainDetect,                  0x00002,  "1"
HKR, ,                                  rxChainDetectRef,               0x00002,  "0"
HKR, ,                                  rxChainDetectThreshA,           0x00002,  "0"
HKR, ,                                  rxChainDetectThreshG,           0x00002,  "0"
HKR, ,                                  rxChainDetectDeltaA,            0x00002,  "20"
HKR, ,                                  rxChainDetectDeltaG,            0x00002,  "20"

[9485BTcoex.reg]
HKR, ,                                  wlanActiveGpioSelect,           0x00002,  "5"
HKR, ,                                  btActiveGpioSelect,             0x00002,  "4"
HKR, ,                                  btPriorityGpioSelect,           0x00002,  "8"
HKR, ,                                  btCoexEnable,                   0x00002,  "4"
HKR, ,                                  btCoexAgent,                    0x00002,  "1"
HKR, ,                                  btCoexDisablePTA,               0x00002,  "2621441"
HKR, ,                                  btWlanIsolation,                0x00002,  "25"
HKR, ,                                  btCoexAntDivEnable,             0x00002,  "0"

[9485BTcoexPTA.reg]
HKR, ,                                  wlanActiveGpioSelect,           0x00002,  "5"
HKR, ,                                  btActiveGpioSelect,             0x00002,  "4"
HKR, ,                                  btPriorityGpioSelect,           0x00002,  "8"
HKR, ,                                  btCoexEnable,                   0x00002,  "4"
HKR, ,                                  btCoexAgent,                    0x00002,  "1"
HKR, ,                                  btCoexDisablePTA,               0x00002,  "3932161"
HKR, ,                                  btWlanIsolation,                0x00002,  "25"
HKR, ,                                  btCoexAntDivEnable,             0x00002,  "0"

[9485BTCoexAgent0.reg]
HKR, ,                                  wlanActiveGpioSelect,           0x00002,  "5"
HKR, ,                                  btActiveGpioSelect,             0x00002,  "4"
HKR, ,                                  btPriorityGpioSelect,           0x00002,  "8"
HKR, ,                                  btCoexEnable,                   0x00002,  "4"
HKR, ,                                  btCoexAgent,                    0x00002,  "0"
HKR, ,                                  btCoexDisablePTA,               0x00002,  "2621441"
HKR, ,                                  btWlanIsolation,                0x00002,  "25"
HKR, ,                                  btCoexAntDivEnable,             0x00002,  "0"

[9485BTcoexDivEn.reg]
HKR, ,                                  wlanActiveGpioSelect,           0x00002,  "5"
HKR, ,                                  btActiveGpioSelect,             0x00002,  "4"
HKR, ,                                  btPriorityGpioSelect,           0x00002,  "8"
HKR, ,                                  btCoexEnable,                   0x00002,  "4"
HKR, ,                                  btCoexAgent,                    0x00002,  "1"
HKR, ,                                  btCoexDisablePTA,               0x00002,  "3932161"
HKR, ,                                  btWlanIsolation,                0x00002,  "25"
HKR, ,                                  btCoexAntDivEnable,             0x00002,  "3"
HKR, ,                                  antDivLowRssiCfg,               0x00002,  "20"
HKR, ,                                  antDivFastDivBias,              0x00002,  "3"
HKR, ,                                  btCoexDivDefVal,                0x00002,  "1"

[9485BTcoexDivEn_1.reg]
HKR, ,                                  wlanActiveGpioSelect,           0x00002,  "5"
HKR, ,                                  btActiveGpioSelect,             0x00002,  "4"
HKR, ,                                  btPriorityGpioSelect,           0x00002,  "8"
HKR, ,                                  btCoexEnable,                   0x00002,  "4"
HKR, ,                                  btCoexAgent,                    0x00002,  "1"
HKR, ,                                  btCoexDisablePTA,               0x00002,  "2621441"
HKR, ,                                  btWlanIsolation,                0x00002,  "25"
HKR, ,                                  btCoexAntDivEnable,             0x00002,  "3"
HKR, ,                                  antDivLowRssiCfg,               0x00002,  "20"
HKR, ,                                  antDivFastDivBias,              0x00002,  "3"
HKR, ,                                  btCoexDivDefVal,                0x00002,  "1"

[pushbutton.reg]
HKR, ,                                  wpsButtonGpio,                  0x00002,  "9"

[smpsDynamic.reg]
HKR, Ndi\params\smpsDynamic,            ParamDesc,  0,  %smpsDynamic%
HKR, Ndi\params\smpsDynamic,            Base,       0,  "10"
HKR, Ndi\params\smpsDynamic,            default,    0,  "0"
HKR, Ndi\params\smpsDynamic,            type,       0,  "enum"
HKR, Ndi\params\smpsDynamic\enum,       "1",        0,  %Enable%
HKR, Ndi\params\smpsDynamic\enum,       "0",        0,  %Disable%

[amp.reg]
HKR, ,                                  ampEnable,                      0x00002,  "1"
HKR, Ndi\params\ampEnable,              ParamDesc,                      0,        %bt30%
HKR, Ndi\params\ampEnable,              default,                        0,        "1"
HKR, Ndi\params\ampEnable,              type,                           0,        "enum"
HKR, Ndi\params\ampEnable\enum,         "1",                            0,        %bt30enable%
HKR, Ndi\params\ampEnable\enum,         "0",                            0,        %bt30disable%

[bt30_high_speed.reg]
HKR, ,                                  ampEnable,                      0x00002,  "0"

[ampTFilter.reg]
HKR, ,                                  ampFilterName,                  0x00002,  "ATHAMPFLx"

[ampBFilter.reg]
HKR, ,                                  ampFilterName,                  0x00002,  "BTWAMPFL"

[ampFilter.reg]
HKR, ,                                  ampFilterName,                  0x00002,  "ATHAMPFL"

[ampGUID.reg]
HKR, ,                                  ampGUID,                        0x00002,  "1"

[amp_default.reg]
HKR, ,                                  ampEnable,                      0x00002,  "0"
HKR, Ndi\params\ampEnable,              ParamDesc,                      0,        %bt30%
HKR, Ndi\params\ampEnable,              default,                        0,        "0"
HKR, Ndi\params\ampEnable,              type,                           0,        "enum"
HKR, Ndi\params\ampEnable\enum,         "1",                            0,        %bt30enable%
HKR, Ndi\params\ampEnable\enum,         "0",                            0,        %bt30disable%

[ctlPowerTableChangeEnable.reg]
HKR, ,                                  ctlPowerTableChangeEnable,      0x00002,  "1"

[customer0.reg]
HKR, ,                                  ssid,                           0x00002,  "randomssidtoshutoffautoconnectib"
HKR, ,                                  scanTimePreSleep,               0x00002,  "60" 
HKR, ,                                  capLinkSp,                      0x00002,  "1" 
HKR, ,                                  pcieAspm,                       0x00002,  "2" 
HKR, ,                                  halPciePowerSaveEnable,         0x00002,  "1" 
HKR, Ndi\params\scanTimeValid,          ParamDesc,                      0,        %scanTime%
HKR, Ndi\params\scanTimeValid,          default,                        0,        "60"
HKR, Ndi\params\scanTimeValid,          min,                            0,        "20"
HKR, Ndi\params\scanTimeValid,          max,                            0,        "120"
HKR, Ndi\params\scanTimeValid,          step,                           0,        "5"
HKR, Ndi\params\scanTimeValid,          base,                           0,        "10"
HKR, Ndi\params\scanTimeValid,          type,                           0,        "int"

[customer0_HB95.reg]
HKR, ,                                  ssid,                           0x00002,  "randomssidtoshutoffautoconnectib"
HKR, ,                                  scanTimePreSleep,               0x00002,  "60" 
HKR, Ndi\params\scanTimeValid,          ParamDesc,                      0,        %scanTime%
HKR, Ndi\params\scanTimeValid,          default,                        0,        "60"
HKR, Ndi\params\scanTimeValid,          min,                            0,        "20"
HKR, Ndi\params\scanTimeValid,          max,                            0,        "120"
HKR, Ndi\params\scanTimeValid,          step,                           0,        "5"
HKR, Ndi\params\scanTimeValid,          base,                           0,        "10"
HKR, Ndi\params\scanTimeValid,          type,                           0,        "int"

[customer0_HB93.reg]
HKR, ,                                  ssid,                           0x00002,  "randomssidtoshutoffautoconnectib"
HKR, ,                                  scanTimePreSleep,               0x00002,  "60" 
HKR, ,                                  pcieAspm,                       0x00002,  "2" 
HKR, ,                                  halPciePowerSaveEnable,         0x00002,  "1" 
HKR, Ndi\params\scanTimeValid,          ParamDesc,                      0,        %scanTime%
HKR, Ndi\params\scanTimeValid,          default,                        0,        "60"
HKR, Ndi\params\scanTimeValid,          min,                            0,        "20"
HKR, Ndi\params\scanTimeValid,          max,                            0,        "120"
HKR, Ndi\params\scanTimeValid,          step,                           0,        "5"
HKR, Ndi\params\scanTimeValid,          base,                           0,        "10"
HKR, Ndi\params\scanTimeValid,          type,                           0,        "int"

[customerop.reg]
HKR, ,                                  gpioPinFunc1,                   0x00002,  "1"

[customer0LED.reg]
HKR, ,                                  gpioPinFunc1,                   0x00002,  "0"

[customer0LED1.reg]
HKR, ,                                  gpioPinFunc1,                   0x00002,  "1"
HKR, ,                                  overrideACstatus,               0x00002,  "1"
HKR, ,                                  halPcieClockReq,                0x00002,  "0"

[customer0LED2.reg]
HKR, ,                                  gpioPinFunc1,                   0x00002,  "3"
HKR, ,                                  overrideACstatus,               0x00002,  "1"
HKR, ,                                  halPcieClockReq,                0x00002,  "0"

[customer0_11n.reg]
;PCIe Related
HKR, ,                                  radioEnableInterval,            0x00002,  "5"
HKR, ,                                  pcieAspm,                       0x00002,  "2"
HKR, ,                                  halPciePowerSaveEnable,         0x00002,  "1"
HKR, ,                                  overrideACstatus,               0x00002,  "1"
HKR, ,                                  forceWake,                      0x00002,  "0"
HKR, ,                                  antennaSwitchSwap,              0x00002,  "1"
;LED Related
HKR, ,                                  gpioPinFunc1,                   0x00002,  "1"
;General Customer0
HKR, ,                                  ssid,                           0x00002,  "randomssidtoshutoffautoconnectib"
HKR,NDI\params\ignore11dBeacon,ParamDesc,,      %11DModeSwitch%
HKR,NDI\params\ignore11dBeacon,type,,           "enum"
HKR,NDI\params\ignore11dBeacon,Default,,        "1"
HKR,NDI\params\ignore11dBeacon\enum,0,,         %Enable%
HKR,NDI\params\ignore11dBeacon\enum,1,,         %Disable%

HKR, Ndi\params\roamRssiA,              ParamDesc,                      0,  %roamRssiA%
HKR, Ndi\params\roamRssiA,              default,                        0,  "15"
HKR, Ndi\params\roamRssiA,              min,                            0,  "1"
HKR, Ndi\params\roamRssiA,              max,                            0,  "95"
HKR, Ndi\params\roamRssiA,              step,                           0,  "1"
HKR, Ndi\params\roamRssiA,              base,                           0,  "10"
HKR, Ndi\params\roamRssiA,              type,                           0,  "int"

HKR, Ndi\params\scanTimeValid,          ParamDesc,                      0,  %scanTime%
HKR, Ndi\params\scanTimeValid,          default,                        0,  "60"
HKR, Ndi\params\scanTimeValid,          min,                            0,  "20"
HKR, Ndi\params\scanTimeValid,          max,                            0,  "120"
HKR, Ndi\params\scanTimeValid,          step,                           0,  "5"
HKR, Ndi\params\scanTimeValid,          base,                           0,  "10"
HKR, Ndi\params\scanTimeValid,          type,                           0,  "int"

[customer1ani.reg]
HKR, Ndi\params\rssiThrHigh,            ParamDesc,                      0,        %rssiThrHigh%
HKR, Ndi\params\rssiThrHigh,            Base,                           0,        "10"
HKR, Ndi\params\rssiThrHigh,            default,                        0,        "40"
HKR, Ndi\params\rssiThrHigh,            type,                           0,        "enum"
HKR, Ndi\params\rssiThrHigh\enum,       "40",                           0,        %rssiThrHighNormal%
HKR, Ndi\params\rssiThrHigh\enum,       "32",                           0,        %rssiThrHighMin%

[customer1roamPolicy.reg]
HKR, Ndi\params\roamPolicy,             ParamDesc,                      0,        %roamPolicy%
HKR, Ndi\params\roamPolicy,             Base,                           0,        "10"
HKR, Ndi\params\roamPolicy,             default,                        0,        "3"
HKR, Ndi\params\roamPolicy,             type,                           0,        "enum"
HKR, Ndi\params\roamPolicy\enum,        "1",                            0,        %roamPolicyVeryLow%
HKR, Ndi\params\roamPolicy\enum,        "2",                            0,        %roamPolicyLow%
HKR, Ndi\params\roamPolicy\enum,        "3",                            0,        %roamPolicyNormal%
HKR, Ndi\params\roamPolicy\enum,        "4",                            0,        %roamPolicyHigh%
HKR, Ndi\params\roamPolicy\enum,        "5",                            0,        %roamPolicyVeryHigh%

[customer1GreenTx.reg]
HKR, Ndi\params\GreenTx,                ParamDesc,                      0,        %GreenTx%
HKR, Ndi\params\GreenTx,                Base,                           0,        "10"
HKR, Ndi\params\GreenTx,                default,                        0,        "0"
HKR, Ndi\params\GreenTx,                type,                           0,        "enum"
HKR, Ndi\params\GreenTx\enum,           "0",                            0,        %GreenTxEnableOff%
HKR, Ndi\params\GreenTx\enum,           "1",                            0,        %GreenTxEnableOn%

[customer2GreenTx.reg]
HKR, ,                                  GreenTx,                            0x00002,  "15"

[customer_power_Toshiba.reg]
HKR, ,                                  SleepTimePwrSave,               0x00002,  "1000"
HKR, ,                                  SleepTimePerf,                  0x00002,  "1000"
HKR, ,                                  PsActivityCheckInterval,		0x00002,  "4"
HKR, ,                                  AwakeTimePwrSaveMax,            0x00002,  "35"
HKR, ,                                  AwakeTimePwrSave,               0x00002,  "35"
HKR, ,                                  periodicScanEnable,             0x00002,  "0"
HKR, ,                                  swBeaconProcess,                0x00002,  "0"

[power_management.reg]
HKR, ,                                  PsActivityCheckInterval,		0x00002,  "4"
HKR, ,                                  AwakeTimePwrSaveMax,            0x00002,  "35"
HKR, ,                                  AwakeTimePwrSave,               0x00002,  "35"
HKR, ,                                  bkScanEnable,               	0x00002,  "0"
HKR, ,                                  swBeaconProcess,				0x00002,  "0"

[customer2.reg]
HKR,,                                   linkLEDFunc,                    0,        "53"
HKR,,                                   activityLEDFunc,                0,        "51"
HKR,,                                   connectionLEDFunc,              0,        "55"

[customer2.11n.reg]
HKR, ,                                  gpioPinFunc0,                   0x00002,  "1"

[customer2merlin.reg]
HKR, ,                                  gpioPinFunc0,                   0x00002,  "1"
HKR, ,                                  gpioFunc0ActHi,                 0x00002,  "1"

[customer3.reg]
HKR, ,                                  scanTimePreSleep,               0x00002,  "60"
HKR, ,                                  SleepTimePerf,                  0x00002,  "500"
HKR, ,                                  LinkLEDFunc,                    0x00002,  "19"
HKR, ,                                  ActivityLEDFunc,                0x00002,  "21"

[customer3a.reg]
HKR, ,                                  scanTimePreSleep,               0x00002,  "60"
HKR, ,                                  SleepTimePerf,                  0x00002,  "500"
HKR, ,                                  gpioPinFunc1,                   0x00002,  "3"
HKR, ,                                  gpioLedCustom,                  0x00002,  "4"
HKR, ,                                  gpioFunc1ActHi,                 0x00002,  "0"

;[customer3b.reg]
;HKR, ,                                  gpioPinFunc1,                  0x00002,  "3"
;HKR, ,                                  overrideACstatus,              0x00002,  "1"
;HKR, ,                                  halPcieClockReq,               0x00002,  "0"
;HKR, ,                                  gpioLedCustom,                 0x00002,  "4"
;HKR, ,                                  gpioFunc1ActHi,                0x00002,  "0"

[customer3c.reg]
HKR, ,                                  scanTimePreSleep,               0x00002,  "60"
HKR, ,                                  SleepTimePerf,                  0x00002,  "500"
HKR, ,                                  gpioPinFunc0,                   0x00002,  "1"
HKR, ,                                  gpioLedCustom,                  0x00002,  "3"

[customer3d.reg]
HKR, ,                                  scanTimePreSleep,               0x00002,  "60"
HKR, ,                                  SleepTimePerf,                  0x00002,  "500"
HKR, ,                                  gpioPinFunc1,                   0x00002,  "3"
HKR, ,                                  gpioLedCustom,                  0x00002,  "0"
HKR, ,                                  gpioFunc1ActHi,                 0x00002,  "0"

[customer3e.reg]
HKR, ,                                  scanTimePreSleep,               0x00002,  "60"
HKR, ,                                  SleepTimePerf,                  0x00002,  "500"
HKR, ,                                  gpioPinFunc0,                   0x00002,  "3"
HKR, ,                                  gpioLedCustom,                  0x00002,  "3"

[customer3f.reg]
HKR, ,                                  scanTimePreSleep,               0x00002,  "60"
HKR, ,                                  SleepTimePerf,                  0x00002,  "500"
HKR, ,                                  gpioPinFunc0,                   0x00002,  "8"
HKR, ,                                  gpioLedCustom,                  0x00002,  "3"

[customer3g.reg]
HKR, ,                                  scanTimePreSleep,               0x00002,  "60"
HKR, ,                                  SleepTimePerf,                  0x00002,  "500"
HKR, ,                                  gpioPinFunc0,                   0x00002,  "6"
HKR, ,                                  gpioLedCustom,                  0x00002,  "3"

;add by alan liu for liteon PCIE 1.1
[customer3gpcie11.reg]
HKR, ,                                  scanTimePreSleep,               0x00002,  "60"
HKR, ,                                  SleepTimePerf,                  0x00002,  "500"
HKR, ,                                  gpioPinFunc0,                   0x00002,  "6"
HKR, ,                                  gpioPinFunc1,                   0x00002,  "6"
HKR, ,                                  gpioPinFunc2,                   0x00002,  "6"
HKR, ,                                  gpioLedCustom,                  0x00002,  "4"
;-----------------------------------------------------------------------------------------------------

[customer3h.reg]
HKR, ,                                  scanTimePreSleep,               0x00002,  "60"
HKR, ,                                  SleepTimePerf,                  0x00002,  "500"
HKR, ,                                  gpioPinFunc0,                   0x00002,  "4"
HKR, ,                                  gpioLedCustom,                  0x00002,  "3"

[customer3_legacybgwmode.reg]
HKR, Ndi\params\wModeSelect,            ParamDesc,                      0,        %wModeSelect%
HKR, Ndi\params\wModeSelect,            Base,                           0,        "10"
HKR, Ndi\params\wModeSelect,            default,                        0,        "12"
HKR, Ndi\params\wModeSelect,            type,                           0,        "enum"
HKR, Ndi\params\wModeSelect\enum,       "4",                            0,        %wModeLegacy11bonly%
HKR, Ndi\params\wModeSelect\enum,       "12",                           0,        %wModeLegacy11bg%

[customer4.reg]
HKR, ,                                  gpioPinFunc0,                   0x00002,  "1"
HKR, ,                                  translateNullSsid,              0x00002,  "1"
HKR, ,                                  AwakeTimePerf,                  0x00002,  "200"

[customer4a.reg]
HKR, ,                                  gpioPinFunc0,                   0x00002,  "1"
HKR, ,                                  gpioFunc0ActHi,                 0x00002,  "0"
HKR, ,                                  halPcieClockReq,                0x00002,  "0"
HKR, ,                                  translateNullSsid,              0x00002,  "1"
HKR, ,                                  AwakeTimePerf,                  0x00002,  "200"

[customer4as.reg]
HKR, ,                                  gpioPinFunc0,                   0x00002,  "8"
HKR, ,                                  gpioFunc0ActHi,                 0x00002,  "0"
HKR, ,                                  halPcieClockReq,                0x00002,  "0"
HKR, ,                                  translateNullSsid,              0x00002,  "1"
HKR, ,                                  AwakeTimePerf,                  0x00002,  "200"

[customer4adhoc.reg]
HKR, ,                                  defaultIbssChannel,             0x00002,  "11"

[customer4b.reg]
HKR, ,                                  gpioPinFunc0,                   0x00002,  "3"
HKR, ,                                  gpioFunc0ActHi,                 0x00002,  "0"
HKR, ,                                  halPcieClockReq,                0x00002,  "0"
HKR, ,                                  translateNullSsid,              0x00002,  "1"
HKR, ,                                  AwakeTimePerf,                  0x00002,  "200"

[customer4c.reg]
HKR, ,                                  translateNullSsid,              0x00002,  "1"
HKR, ,                                  AwakeTimePerf,                  0x00002,  "200"

[customer4a_ASPM.reg]
HKR, ,                                  pcieAspm,                       0x00002,  "0"

[customer5Led.reg]
HKR, ,                                  softLEDEnable,                  0x00002,  "1"
HKR, ,                                  swapDefaultLED,                 0x00002,  "1"

[customer5.11nLED.reg]
HKR, ,                                  gpioLedCustom,                  0x00002,  "1"
HKR, ,                                  gpioPinFunc0,                   0x00002,  "1"
HKR, ,                                  gpioPinFunc1,                   0x00002,  "2"
HKR, ,                                  gpioFunc0ActHi,                 0x00002,  "1"
HKR, ,                                  gpioFunc1ActHi,                 0x00002,  "0"

[customer5.PCIe11nLed.reg]
HKR, ,                                  gpioLedCustom,                  0x00002,  "1"
HKR, ,                                  gpioPinFunc1,                   0x00002,  "1"

[customer5.3x3.reg]
HKR, ,                                  txChainMask,                    0x00002,  "7"
HKR, ,                                  rxChainMask,                    0x00002,  "7"

[customer7Led.reg]
HKR, ,                                  gpioLedCustom,                  0x00002,  "2"
HKR, ,                                  gpioPinFunc0,                   0x00002,  "1"
HKR, ,                                  gpioPinFunc1,                   0x00002,  "2"
HKR, ,                                  gpioFunc0ActHi,                 0x00002,  "1"
HKR, ,                                  gpioFunc1ActHi,                 0x00002,  "1"

[customer9Led.reg]
HKR, ,                                  gpioPinFunc1,                   0x00002,  "1"

[Customer15a.led.reg]
HKR, ,                                  gpioPinFunc0,                   0x00002,  "1"
HKR, ,                                  gpioLedCustom,                  0x00002,  "3"

[Customer15b.led.reg]
HKR, ,                                  gpioPinFunc0,                   0x00002,  "3"
HKR, ,                                  gpioLedCustom,                  0x00002,  "3"

[gpioled.reg]
HKR,,                                   linkLEDFunc,                    0,        "49"
HKR,,                                   activityLEDFunc,                0,        "51"
HKR,,                                   connectionLEDFunc,              0,        "55"

[ratecap.reg]
HKR, ,                                  txCoalescingEnable,             0x00002,  "1"

[customer11n.reg]
HKR, Ndi\params\*ReceiveBuffers,        ParamDesc,                      0,        "%ReceiveBuffers%"
HKR, Ndi\params\*ReceiveBuffers,        default,                        0,        "256"
HKR, Ndi\params\*ReceiveBuffers,        min,                            0,        "1"
HKR, Ndi\params\*ReceiveBuffers,        max,                            0,        "00000512"
HKR, Ndi\params\*ReceiveBuffers,        step,                           0,        "1"
HKR, Ndi\params\*ReceiveBuffers,        Base,                           0,        "10"
HKR, Ndi\params\*ReceiveBuffers,        type,                           0,        "int"
HKR, Ndi\params\*TransmitBuffers,       ParamDesc,                      0,        "%TransmitBuffers%"
HKR, Ndi\params\*TransmitBuffers,       default,                        0,        "512"
HKR, Ndi\params\*TransmitBuffers,       min,                            0,        "1"
HKR, Ndi\params\*TransmitBuffers,       max,                            0,        "00000512"
HKR, Ndi\params\*TransmitBuffers,       step,                           0,        "1"
HKR, Ndi\params\*TransmitBuffers,       Base,                           0,        "10"
HKR, Ndi\params\*TransmitBuffers,       type,                           0,        "int"
HKR, Ndi\params\shortPreamble,          ParamDesc,                      0,        %shortPreamble%
HKR, Ndi\params\shortPreamble,          Base,                           0,        "10"
HKR, Ndi\params\shortPreamble,          default,                        0,        "1"
HKR, Ndi\params\shortPreamble,          type,                           0,        "enum"
HKR, Ndi\params\shortPreamble\enum,     "1",                            0,        %shortPreambleEnable%
HKR, Ndi\params\shortPreamble\enum,     "0",                            0,        %shortPreambleDisable%
HKR, Ndi\params\scanTimeValid,          ParamDesc,                      0,        %scanTimeValid%
HKR, Ndi\params\scanTimeValid,          default,                        0,        "60"
HKR, Ndi\params\scanTimeValid,          min,                            0,        "20"
HKR, Ndi\params\scanTimeValid,          max,                            0,        "120"
HKR, Ndi\params\scanTimeValid,          step,                           0,        "5"
HKR, Ndi\params\scanTimeValid,          base,                           0,        "10"
HKR, Ndi\params\scanTimeValid,          type,                           0,        "int"

[customer11.reg]
HKR, Ndi\params\*ReceiveBuffers,    ParamDesc,  0, "%ReceiveBuffers%"
HKR, Ndi\params\*ReceiveBuffers,    default,    0, "256"
HKR, Ndi\params\*ReceiveBuffers,    min,        0, "1"
HKR, Ndi\params\*ReceiveBuffers,    max,        0, "00000512"
HKR, Ndi\params\*ReceiveBuffers,    step,       0, "1"
HKR, Ndi\params\*ReceiveBuffers,    Base,       0, "10"
HKR, Ndi\params\*ReceiveBuffers,    type,       0, "int"
HKR, Ndi\params\*TransmitBuffers,   ParamDesc,  0, "%TransmitBuffers%"
HKR, Ndi\params\*TransmitBuffers,   default,    0, "256"
HKR, Ndi\params\*TransmitBuffers,   min,        0, "1"
HKR, Ndi\params\*TransmitBuffers,   max,        0, "00000512"
HKR, Ndi\params\*TransmitBuffers,   step,       0, "1"
HKR, Ndi\params\*TransmitBuffers,   Base,       0, "10"
HKR, Ndi\params\*TransmitBuffers,   type,       0, "int"
HKR, Ndi\params\shortPreamble,      ParamDesc,  0,  %shortPreamble%
HKR, Ndi\params\shortPreamble,      Base,       0,  "10"
HKR, Ndi\params\shortPreamble,      default,    0,  "1"
HKR, Ndi\params\shortPreamble,      type,       0,  "enum"
HKR, Ndi\params\shortPreamble\enum, "1",        0,  %shortPreambleEnable%
HKR, Ndi\params\shortPreamble\enum, "0",        0,  %shortPreambleDisable%
HKR, Ndi\params\scanTimeValid,      ParamDesc,  0,  %scanTimeValid%
HKR, Ndi\params\scanTimeValid,      default,    0,  "60"
HKR, Ndi\params\scanTimeValid,      min,        0,  "20"
HKR, Ndi\params\scanTimeValid,      max,        0,  "120"
HKR, Ndi\params\scanTimeValid,      step,       0,  "5"
HKR, Ndi\params\scanTimeValid,      base,       0,  "10"
HKR, Ndi\params\scanTimeValid,      type,       0,  "int"

[customer11custom.reg]
HKR, Ndi\params\bkScanEnable,           ParamDesc,                      0,        %bkScanEnable%
HKR, Ndi\params\bkScanEnable,           Base,                           0,        "10"
HKR, Ndi\params\bkScanEnable,           default,                        0,        "1"
HKR, Ndi\params\bkScanEnable,           type,                           0,        "enum"
HKR, Ndi\params\bkScanEnable\enum,      "1",                            0,        %bkScanEnableOn%
HKR, Ndi\params\bkScanEnable\enum,      "0",                            0,        %bkScanEnableOff%

HKR, Ndi\params\radioEnable,            ParamDesc,                      0,        %radioEnable%
HKR, Ndi\params\radioEnable,            Base,                           0,        "10"
HKR, Ndi\params\radioEnable,            default,                        0,        "1"
HKR, Ndi\params\radioEnable,            type,                           0,        "enum"
HKR, Ndi\params\radioEnable\enum,       "1",                            0,        %radioEnableOn%
HKR, Ndi\params\radioEnable\enum,       "0",                            0,        %radioEnableOff%

HKR, Ndi\params\roamRssiA,              ParamDesc,                      0,        %roamRssi11A%
HKR, Ndi\params\roamRssiA,              default,                        0,        "15"
HKR, Ndi\params\roamRssiA,              min,                            0,        "1"
HKR, Ndi\params\roamRssiA,              max,                            0,        "95"
HKR, Ndi\params\roamRssiA,              step,                           0,        "1"
HKR, Ndi\params\roamRssiA,              base,                           0,        "10"
HKR, Ndi\params\roamRssiA,              type,                           0,        "int"

HKR, Ndi\params\roamRssiBOnly,          ParamDesc,                      0,        %roamRssi11BOnly%
HKR, Ndi\params\roamRssiBOnly,          default,                        0,        "8"
HKR, Ndi\params\roamRssiBOnly,          min,                            0,        "0"
HKR, Ndi\params\roamRssiBOnly,          max,                            0,        "95"
HKR, Ndi\params\roamRssiBOnly,          step,                           0,        "1"
HKR, Ndi\params\roamRssiBOnly,          base,                           0,        "10"
HKR, Ndi\params\roamRssiBOnly,          type,                           0,        "int"

HKR, Ndi\params\roamRssiB,              ParamDesc,                      0,        %roamRssi11B%
HKR, Ndi\params\roamRssiB,              default,                        0,        "24"
HKR, Ndi\params\roamRssiB,              min,                            0,        "0"
HKR, Ndi\params\roamRssiB,              max,                            0,        "95"
HKR, Ndi\params\roamRssiB,              step,                           0,        "1"
HKR, Ndi\params\roamRssiB,              base,                           0,        "10"
HKR, Ndi\params\roamRssiB,              type,                           0,        "int"

HKR, Ndi\params\roamRateA,              ParamDesc,                      0,        %roamRateA%
HKR, Ndi\params\roamRateA,              Base,                           0,        "10"
HKR, Ndi\params\roamRateA,              default,                        0,        "24000"
HKR, Ndi\params\roamRateA,              type,                           0,        "enum"
HKR, Ndi\params\roamRateA\enum,         "6000",                         0,        %roamRateA6M%
HKR, Ndi\params\roamRateA\enum,         "9000",                         0,        %roamRateA9M%
HKR, Ndi\params\roamRateA\enum,         "12000",                        0,        %roamRateA12M%
HKR, Ndi\params\roamRateA\enum,         "18000",                        0,        %roamRateA18M%
HKR, Ndi\params\roamRateA\enum,         "24000",                        0,        %roamRateA24M%
HKR, Ndi\params\roamRateA\enum,         "36000",                        0,        %roamRateA36M%
HKR, Ndi\params\roamRateA\enum,         "48000",                        0,        %roamRateA48M%
HKR, Ndi\params\roamRateA\enum,         "54000",                        0,        %roamRateA54M%

HKR, Ndi\params\roamRateBOnly,          ParamDesc,                      0,        %roamRateBOnly%
HKR, Ndi\params\roamRateBOnly,          Base,                           0,        "10"
HKR, Ndi\params\roamRateBOnly,          default,                        0,        "5000"
HKR, Ndi\params\roamRateBOnly,          type,                           0,        "enum"
HKR, Ndi\params\roamRateBOnly\enum,     "1000",                         0,        %roamRateBOnly1M%
HKR, Ndi\params\roamRateBOnly\enum,     "2000",                         0,        %roamRateBOnly2M%
HKR, Ndi\params\roamRateBOnly\enum,     "5000",                         0,        %roamRateBOnly5M%
HKR, Ndi\params\roamRateBOnly\enum,     "11000",                        0,        %roamRateBOnly11M%

HKR, Ndi\params\roamRateB,              ParamDesc,                      0,        %roamRateB%
HKR, Ndi\params\roamRateB,              Base,                           0,        "10"
HKR, Ndi\params\roamRateB,              default,                        0,        "9000"
HKR, Ndi\params\roamRateB,              type,                           0,        "enum"
HKR, Ndi\params\roamRateB\enum,         "1000",                         0,        %roamRateB1M%
HKR, Ndi\params\roamRateB\enum,         "2000",                         0,        %roamRateB2M%
HKR, Ndi\params\roamRateB\enum,         "5000",                         0,        %roamRateB5M%
HKR, Ndi\params\roamRateB\enum,         "6000",                         0,        %roamRateB6M%
HKR, Ndi\params\roamRateB\enum,         "9000",                         0,        %roamRateB9M%
HKR, Ndi\params\roamRateB\enum,         "11000",                        0,        %roamRateB11M%

HKR, Ndi\params\pcieAspm,               ParamDesc,                      0,        %pcieAspm%
HKR, Ndi\params\pcieAspm,               Base,                           0,        "10"
HKR, Ndi\params\pcieAspm,               default,                        0,        "0"
HKR, Ndi\params\pcieAspm,               type,                           0,        "enum"
HKR, Ndi\params\pcieAspm\enum,          "0",                            0,        %pcieAspmOff%
HKR, Ndi\params\pcieAspm\enum,          "1",                            0,        %pcieAspmL0sOn%
HKR, Ndi\params\pcieAspm\enum,          "2",                            0,        %pcieAspmL1On%
HKR, Ndi\params\pcieAspm\enum,          "3",                            0,        %pcieAspmL0sandL1On%

[customer11_11n40wmode.reg]
HKR, Ndi\params\wModeSelect,            ParamDesc,                      0,        %wModeSelect%
HKR, Ndi\params\wModeSelect,            Base,                           0,        "10"
HKR, Ndi\params\wModeSelect,            default,                        0,        "129055"
HKR, Ndi\params\wModeSelect,            type,                           0,        "enum"
HKR, Ndi\params\wModeSelect\enum,       "26628",                        0,        %wModeSelect11bonly%
HKR, Ndi\params\wModeSelect\enum,       "102403",                       0,        %wModeSelect11na%
HKR, Ndi\params\wModeSelect\enum,       "26652",                        0,        %wModeSelect11nbg%
HKR, Ndi\params\wModeSelect\enum,       "129055",                       0,        %wModeSelect11abgn%

[customer11_11nwmode.reg]
HKR, Ndi\params\wModeSelect,            ParamDesc,                      0,        %wModeSelect%
HKR, Ndi\params\wModeSelect,            Base,                           0,        "10"
HKR, Ndi\params\wModeSelect,            default,                        0,        "6175"
HKR, Ndi\params\wModeSelect,            type,                           0,        "enum"
HKR, Ndi\params\wModeSelect\enum,       "2052",                         0,        %wModeSelect11bonly%
HKR, Ndi\params\wModeSelect\enum,       "4099",                         0,        %wModeSelect11na%
HKR, Ndi\params\wModeSelect\enum,       "2076",                         0,        %wModeSelect11nbg%
HKR, Ndi\params\wModeSelect\enum,       "6175",                         0,        %wModeSelect11abgn%

[customer11_legacywmode.reg]
HKR, Ndi\params\wModeSelect,            ParamDesc,                      0,        %wModeSelect%
HKR, Ndi\params\wModeSelect,            Base,                           0,        "10"
HKR, Ndi\params\wModeSelect,            default,                        0,        "31"
HKR, Ndi\params\wModeSelect,            type,                           0,        "enum"
HKR, Ndi\params\wModeSelect\enum,       "4",                            0,        %wModeLegacy11bonly%
HKR, Ndi\params\wModeSelect\enum,       "3",                            0,        %wModeLegacy11a%
HKR, Ndi\params\wModeSelect\enum,       "28",                           0,        %wModeLegacy11bg%
HKR, Ndi\params\wModeSelect\enum,       "31",                           0,        %wModeLegacy11abg%

[customer11Ant.reg]
HKR, Ndi\params\antennaSwitch,          ParamDesc,                      0,        %antennaSwitch%
HKR, Ndi\params\antennaSwitch,          Base,                           0,        "10"
HKR, Ndi\params\antennaSwitch,          default,                        0,        "2"
HKR, Ndi\params\antennaSwitch,          type,                           0,        "enum"
HKR, Ndi\params\antennaSwitch\enum,     "0",                            0,        %antennaSwitchA%
HKR, Ndi\params\antennaSwitch\enum,     "1",                            0,        %antennaSwitchB%
HKR, Ndi\params\antennaSwitch\enum,     "2",                            0,        %antennaSwitchAuto%

[customer_GigaByte.reg]
HKR, ,                          txChainMask,          0x00002,  "5"

[customer_GigaByteLed0.reg]
HKR, ,                                  LinkLedFunc,                    0, "19"
HKR, ,                                  ActivityLedFunc,        0, "21" 

[customer_GigaByteLed1.reg]
HKR, ,                                  LinkLedFunc,                    0, "03"
HKR, ,                                  ActivityLedFunc,                0, "05"

[customer_GigaByteLed2.reg]
HKR, ,                                  LinkLedFunc,                    0, "07"
HKR, ,                                  ActivityLedFunc,                0, "05"

[customer_Samsung.reg]
HKR, Ndi\params\sleepMode,                ParamDesc,                      0,  %PowerSaveMode%
HKR, Ndi\params\sleepMode,                Base,                           0,  "10"
HKR, Ndi\params\sleepMode,                default,                        0,  "2"
HKR, Ndi\params\sleepMode,                type,                           0,  "enum"
HKR, Ndi\params\sleepMode\enum,           "0",                            0,  %Off%
HKR, Ndi\params\sleepMode\enum,           "1",                            0,  %Maximum%
HKR, Ndi\params\sleepMode\enum,           "2",                            0,  %Normal%
HKR, ,                                  pcieAspm,                       0x00002,  "2" 
HKR, ,                                  halPciePowerSaveEnable,         0x00002,  "1" 

[ignore11denable.reg]
HKR, ,                                  ignore11dBeacon,                0x00002,  "1" 

[xb72.via.reg]
HKLM, SYSTEM\CurrentControlSet\Services\pci\Parameters,168c0024,0x00000001, 00,00,00,20,00,00,00,00

[rssiAdjust.reg]
HKR, ,                                  rssiAdjust,                     0x00002,  "7"

[cmdRegister.reg]
HKR, ,                                  cmdRegister,                    0x00002,  "838"

[htAdhocdisable.reg]
HKR, ,                                  htAdhocEnable,                  0x00002,  "0"

[htAdhoc.reg]
HKR, NDI\params\htAdhocEnable,ParamDesc,,       %AdHoc11n%
HKR, NDI\params\htAdhocEnable,type,,            "enum"
HKR, NDI\params\htAdhocEnable,Default,,         "0"
HKR, NDI\params\htAdhocEnable\enum,0,,          %Disable%
HKR, NDI\params\htAdhocEnable\enum,1,,          %Enable%

[AdhocModeSelect.reg]
HKR, NDI\params\AdhocModeSelect,ParamDesc,,             %AdhocMode%
HKR, NDI\params\AdhocModeSelect,type,,                  "enum"
HKR, NDI\params\AdhocModeSelect,Default,,               "2"
HKR, NDI\params\AdhocModeSelect\enum,0,,                %wModeSelect11g%
HKR, NDI\params\AdhocModeSelect\enum,1,,                %wModeSelect11n%
HKR, NDI\params\AdhocModeSelect\enum,2,,                %wModeSelect11b%

[edmaStopRecvDelay.reg]
HKR, ,                                  edmaStopRecvDelay,              0x10001,  3

[htWepTkipOpt.reg]
HKR, Ndi\params\htEnableWepTkip,ParamDesc,  0,  %WepTkip11n%
HKR, NDI\params\htEnableWepTkip,type,,          "enum"
HKR, NDI\params\htEnableWepTkip,Default,,       "1"
HKR, NDI\params\htEnableWepTkip\enum,0,,        %Disable%
HKR, NDI\params\htEnableWepTkip\enum,1,,        %Enable%

[htEnableWepTkip.reg]
HKR, ,                                  htEnableWepTkip,                  0x00002,  "1"

[cemspecled_func1_1.reg]
HKR, ,                                  gpioPinFunc1,                   0x00002,  "1"
HKR, ,                                  gpioLedCustom,                  0x00002,  "4"

[cemspecled_func1_3.reg]
HKR, ,                                  gpioPinFunc1,                   0x00002,  "3"
HKR, ,                                  gpioLedCustom,                  0x00002,  "4"

[cemspecled_func1_6.reg]
HKR, ,                                  gpioPinFunc1,                   0x00002,  "6"
HKR, ,                                  gpioLedCustom,                  0x00002,  "4"

[cemspecled_func1_8.reg]
HKR, ,                                  gpioPinFunc1,                   0x00002,  "8"
HKR, ,                                  gpioLedCustom,                  0x00002,  "4"

[cemspecled_func2_1.reg]
HKR, ,                                  gpioPinFunc0,                   0x00002,  "1"
HKR, ,                                  gpioLedCustom,                  0x00002,  "3"

[cemspecled_func2_8.reg]
HKR, ,                                  gpioPinFunc0,                   0x00002,  "8"
HKR, ,                                  gpioLedCustom,                  0x00002,  "3"

[cemspecled_func2_6.reg]
HKR, ,                                  gpioPinFunc0,                   0x00002,  "6"
HKR, ,                                  gpioLedCustom,                  0x00002,  "3"

[cemspecled_func0_1.reg]
HKR, ,                                  gpioPinFunc0,                   0x00002,  "1"
HKR, ,                                  gpioFunc0ActHi,                 0x00002,  "0"
HKR, ,                                  sharedGpioFunc0,                0x00002,  "1"

[cemspecled_func0_6.reg]
HKR, ,                                  gpioPinFunc0,                   0x00002,  "6"
HKR, ,                                  gpioFunc0ActHi,                 0x00002,  "0"

[cemspecled_func0_6_Hi.reg]
HKR, ,                                  gpioPinFunc0,                   0x00002,  "6"
HKR, ,                                  gpioFunc0ActHi,                 0x00002,  "1"

[cemspecled_func2_10.reg]
HKR, ,                                  gpioPinFunc0,                   0x00002,  "10"
HKR, ,                                  gpioLedCustom,                  0x00002,  "3"

[cemspecled_func1_10.reg]
HKR, ,                                  gpioPinFunc1,                   0x00002,  "10"
HKR, ,                                  gpioLedCustom,                  0x00002,  "4"

[d3forcel1disable.reg]
HKR, ,                                  halPcieWaen,                    0x00002,  "4212539"

[d3forcel1disable1.reg]
HKR, ,                                  halPcieWaen,                         0x00002,  "4212539"
HKR, ,                                  halPcieDetach,                    0x00002,  "1"

[maxpowersave.reg]
HKR, ,                                  sleepTimePwrSave,               0x00002,  "1000"
HKR, ,                                  SleepTimePerf,                  0x00002,  "1000"

[maxpowersave2.reg]
HKR, ,                                  sleepTimePwrSave,               0x00002,  "1000"
HKR, ,                                  SleepTimePerf,                  0x00002,  "1000"
HKR, ,                                  AwakeTimePwrSaveMax,            0x00002,  "150"

[customer_IODATA.reg]
HKR, ,                                  LinkLedFunc,                    0, "49"
HKR, ,                                  ActivityLedFunc,                0, "51"

[janusda.reg]
HKR, ,                                  btCoexEnable,                   0x00002,  "4"
HKR, ,                                  btCoexAgent,                    0x00002,  "1"
HKR, ,                                  btCoexDisablePTA,               0x00002,  "2621441"
HKR, ,                                  btWlanIsolation,                0x00002,  "25"
HKR, ,                                  btCoexAntDivEnable,             0x00002,  "0"

[janusda_coexPTA_40_21.reg]
HKR, ,                                  btCoexEnable,                   0x00002,  "4"
HKR, ,                                  btCoexAgent,                    0x00002,  "1"
HKR, ,                                  btCoexDisablePTA,               0x00002,  "2621441"
HKR, ,                                  btWlanIsolation,                0x00002,  "21"

[janusda_CoexAgent0.reg]
HKR, ,                                  btCoexEnable,                   0x00002,  "4"
HKR, ,                                  btCoexAgent,                    0x00002,  "0"
HKR, ,                                  btCoexDisablePTA,               0x00002,  "2621441"
HKR, ,                                  btWlanIsolation,                0x00002,  "25"
HKR, ,                                  btCoexAntDivEnable,             0x00002,  "0"

[roamPolicy.reg]
HKR, Ndi\params\roamPolicy,             ParamDesc,                      0,        %roamPolicy%
HKR, Ndi\params\roamPolicy,             Base,                           0,        "10"
HKR, Ndi\params\roamPolicy,             default,                        0,        "3"
HKR, Ndi\params\roamPolicy,             type,                           0,        "enum"
HKR, Ndi\params\roamPolicy\enum,        "1",                            0,        %roamPolicyVeryLow%
HKR, Ndi\params\roamPolicy\enum,        "2",                            0,        %roamPolicyLow%
HKR, Ndi\params\roamPolicy\enum,        "3",                            0,        %roamPolicyNormal%
HKR, Ndi\params\roamPolicy\enum,        "4",                            0,        %roamPolicyHigh%
HKR, Ndi\params\roamPolicy\enum,        "5",                            0,        %roamPolicyVeryHigh%

[roamPolicy2.reg]
HKR, Ndi\params\roamPolicy,             ParamDesc,                      0,        %roamPolicy%
HKR, Ndi\params\roamPolicy,             Base,                           0,        "10"
HKR, Ndi\params\roamPolicy,             default,                        0,        "3"
HKR, Ndi\params\roamPolicy,             type,                           0,        "enum"
HKR, Ndi\params\roamPolicy\enum,        "1",                            0,        %roamPolicyVeryLow2%
HKR, Ndi\params\roamPolicy\enum,        "2",                            0,        %roamPolicyLow2%
HKR, Ndi\params\roamPolicy\enum,        "3",                            0,        %roamPolicyNormal2%
HKR, Ndi\params\roamPolicy\enum,        "4",                            0,        %roamPolicyHigh2%
HKR, Ndi\params\roamPolicy\enum,        "5",                            0,        %roamPolicyVeryHigh2%

[hb97ChainMask.reg]
HKR, ,                                  txChainMaskLegacy,              0x00002,  "3"
HKR, ,                                  rxChainMaskLegacy,              0x00002,  "3"

[heliusda.reg]
HKR, ,                                  btCoexEnable,                   0x00002,  "4"
HKR, ,                                  btCoexAgent,                    0x00002,  "1"
HKR, ,                                  btModule,                       0x00002,  "2"
HKR, ,                                  txCoalescingEnable,             0x00002,  "1"
HKR, ,                                  txChainMaskLegacy,              0x00002,  "2"
HKR, ,                                  rxChainMaskLegacy,              0x00002,  "2"
HKR, ,                                  btCoexEnhanceA2DP,              0x00002,  "70"

[WB197da.reg]
HKR, ,                                  btCoexEnable,                   0x00002,  "4"
HKR, ,                                  btCoexAgent,                    0x00002,  "1"
HKR, ,                                  btModule,                       0x00002,  "2"
HKR, ,                                  txCoalescingEnable,             0x00002,  "1"
HKR, ,                                  txChainMaskLegacy,              0x00002,  "3"
HKR, ,                                  rxChainMaskLegacy,              0x00002,  "3"
HKR, ,                                  btCoexEnhanceA2DP,              0x00002,  "70"

[btcoexa2dp99.reg]
HKR, ,                                  btCoexEnhanceA2DP,              0x00002,  "99"

[jupiter2ant.reg]
HKR, ,                                  btCoexEnable,                   0x00002,  "5"
HKR, ,                                  btCoexAgent,                    0x00002,  "1"
HKR, ,                                  halPllPwrSave,                  0x00002,  "7"
HKR, ,                                  txChainMaskLegacy,              0x00002,  "2"
HKR, ,                                  rxChainMaskLegacy,              0x00002,  "3"

[jupiter2ant2.reg]
HKR, ,                                  btCoexEnable,                   0x00002,  "5"
HKR, ,                                  btCoexAgent,                    0x00002,  "1"
HKR, ,                                  halPllPwrSave,                  0x00002,  "7"
HKR, ,                                  txChainMaskLegacy,              0x00002,  "3"
HKR, ,                                  rxChainMaskLegacy,              0x00002,  "3"

[aphroditeant.reg]
HKR, ,                                  btCoexEnable,                   0x00002,  "5"
HKR, ,                                  btCoexAgent,                    0x00002,  "1"
HKR, ,                                  halPllPwrSave,                  0x00002,  "7"
HKR, ,                                  mciConfig,                      0x00000,  "16819393"
HKR, ,                                  btCoexLowACKPwr,                0x00000,  "1835777"
HKR, ,                                  btCoexdisablePKDET,             0x00000,  "949"

[aphroditeant2.reg]
HKR, ,                                  btCoexEnable,                   0x00002,  "5"
HKR, ,                                  btCoexAgent,                    0x00002,  "1"
HKR, ,                                  halPllPwrSave,                  0x00002,  "7"
HKR, ,                                  mciConfig,                      0x00000,  "33596642"
HKR, ,                                  btCoexLowACKPwr,                0x00000,  "2622209"

[aphrodite_coex.reg]
HKR, ,                                  btCoexStompA2DPCfg,             0x00000,  "24323329"
HKR, ,                                  btCoexStompSCOCfg,              0x00000,  "25502465"
HKR, ,                                  btCoexMiscCfg,                  0x00000,  "5"

[aphrodite_coex_ts.reg]
HKR, ,                                  btCoexStompA2DPCfg,             0x00000,  "24323329"
HKR, ,                                  btCoexStompSCOCfg,              0x00000,  "25502465"
HKR, ,                                  btCoexMiscCfg,                  0x00000,  "7"

[aphrodite_coex2.reg]
HKR, ,                                  btCoexStompA2DPCfg,             0x00000,  "24323329"
HKR, ,                                  btCoexStompSCOCfg,              0x00000,  "19211009"
HKR, ,                                  btCoexMiscCfg,                  0x00000,  "1"

[aphrodite_coex2_a2dp.reg]
HKR, ,                                  btCoexStompA2DPCfg,             0x00000,  "24323331"
HKR, ,                                  btCoexStompSCOCfg,              0x00000,  "19211009"
HKR, ,                                  btCoexMiscCfg,                  0x00000,  "1"

[aphroditeantdiv.reg]
HKR, ,                                  btCoexAntDivEnable,             0x00002,  "3"
HKR, ,                                  lnaDivUseBtAntEnable,           0x00002,  "1"

[aphroditeantdiv2.reg]
HKR, ,                                  btCoexAntDivEnable,             0x00002,  "3"
HKR, ,                                  btCoexDivDefVal,                0x00002,  "1"
HKR, ,                                  lnaDivUseBtAntEnable,           0x00002,  "1"

[aphrodite_coexPTA_40_20.reg]
HKR, ,                                  btCoexDisablePTA,               0x00000,  "2621441"
HKR, ,                                  btWlanIsolation,                0x00000,  "20"

[aphrodite_coexPTA_34_25.reg]
HKR, ,                                  btCoexDisablePTA,               0x00000,  "2228225"
HKR, ,                                  btCoexDisablePTACfg,            0x00000,  "1"
HKR, ,                                  btWlanIsolation,                0x00000,  "25"

[eTputA2dpHid.reg]
HKR, ,                                  btCoexMiscCfg,                  0x00000,  "16"

[halBtcTSWar.reg]
HKR, ,                                  halBtcTSWar,             		0x00002,  "1"

[merlinshiftdelay.reg]
HKR, ,                                  analogShiftRegDelay,            0x00002,  "10"

[tpshiftdelay.reg]
HKR, ,                                  analogShiftRegDelay,            0x00002,  "30"

[minpower.reg]
HKR, ,                                  legacyMinTxPowerLimit,          0x00002,  "10"

[wowenable.reg]
HKR, ,                                  wowEnable,                      0x00002,  "1"
HKR, ,                                  CMQ,                            0x00002,  "0"

[j21swwow.reg]
HKR, ,                                  halWowOffload,                  0x00010001,  0x00e3ec01
HKR, ,                                  halWowOffloadBtTimeout,         0x00010001,  0x00000030
HKR, ,                                  halWakeupDelay,                 0x00010001,  0x0000003C
HKR, ,                                  halNlo,                         0x00010001,  0x00000001
HKR, ,                                  enableReportNdisHWWowCap,       0x00010001,  0x00000001
HKR, ,                                  WowEnablePME,                   0x00010001,  0x00000000
HKR, ,                                  wowEnable,                      0x00002,     "1"

[A11swwow.reg]
HKR, ,                                  halWowOffload,                  0x00010001,  0x00c3ec01
HKR, ,                                  halWowOffloadBtTimeout,         0x00010001,  0x00000030
HKR, ,                                  halWakeupDelay,                 0x00010001,  0x0000003C
HKR, ,                                  halNlo,                         0x00010001,  0x00000001
HKR, ,                                  WowEnablePME,                   0x00010001,  0x00000000
HKR, ,                                  halWowParameter,                0x00010001,  0x80000000
HKR, ,                                  halWowWDTPeriod,                0x00010001,  0x00000002
HKR, ,                                  wowEnable,                      0x00002,     "1"

[S5wow.reg]
HKR, ,                                  wsis5,                          0x00002,  "1"
HKR, ,                                  wowEnable,                      0x00002,  "1"

[DisWakeOnAPLost.reg]
HKR, ,                                  disableWakeOnApLost,            0x00002,  "1"

[RestoreSettingCount.reg]
HKR, ,                                  halRestoreSettingCount,         0x00002,  "150"

[triggerlevelkiteonly.reg]
HKR, ,                                  txTrigLevelMax ,                0x00002,  "32"
HKR, ,                                  fakeAIFSN4WFA ,                 0x00002,  "1"

[c3war.reg]
HKR, ,                                  c3WarTimerPeriod,               0x00002,  "130"

[indicaterxlinkspeed.reg]
HKR, ,                                  indicateRxLinkSpeed ,           0x00002,  "1"

[fullhwresethb93.reg]
HKR, ,                                  halFullResetWarEnable ,         0x00002,  "0"

[sharegpio.reg]
HKR, ,                                  sharedGpioFunc0 ,               0x00002,  "1"

[rxLatencyWar.reg]
HKR, ,                                  rxLatencyWar ,                  0x00002,  "1"

[power.reg]
HKR, ,                                  pcieAspm,                       0x00002,  "2"
HKR, ,                                  halpciePowerSaveEnable,         0x00002,  "1"
HKR, ,                                  overrideACstatus,               0x00002,  "1"
HKR, ,                                  scanTimePreSleep,               0x00002,  "5"

[ledcontrol.reg]
HKR, ,                                  gpioPinFunc0,                   0x00002,  "3"
HKR, ,                                  gpioFunc0ActHi,                 0x00002,  "0"

[ledcontrol2.reg]
HKR, ,                                  gpioPinFunc0,                   0x00002,  "1"
HKR, ,                                  gpioFunc0ActHi,                 0x00002,  "0"

[ledcontrol3.reg]
HKR, ,                                  gpioPinFunc0,                   0x00002,  "1"
HKR, ,                                  gpioFunc0ActHi,                 0x00002,  "0"
HKR, ,                                  gpioLedCustom,                  0x00002,  "3"

[kitec3.reg]
HKR, ,                                  c3WarTimerPeriod,               0x00002,  "130"
HKR, ,                                  txTrigLevelMax ,                0x00002,  "32"

[regdmn.reg]
HKR, ,                                  regdmn,                         0x00010001,  0x65

[djanusda.reg]
HKR, ,                                  btCoexEnable,                   0x00002,  "4"
HKR, ,                                  btCoexAgent,                    0x00002,  "1"
HKR, ,                                  netband,                        0x00002,  "2060"
HKR, ,                                  btCoexDisablePTA,               0x00002,  "2621441"
HKR, ,                                  btWlanIsolation,                0x00002,  "25"
HKR, ,                                  btCoexAntDivEnable,             0x00002,  "0"

[djanusda2.reg]
HKR, ,                                  btCoexEnable,                   0x00002,  "4"
HKR, ,                                  btCoexAgent,                    0x00002,  "1"
HKR, ,                                  netband,                        0x00002,  "2060"
HKR, ,                                  btCoexRSSIModeProfile,          0x00002,  "17115137"
HKR, ,                                  btCoexDisablePTA,               0x00002,  "2621441"
HKR, ,                                  btWlanIsolation,                0x00002,  "25"
HKR, ,                                  btCoexAntDivEnable,             0x00002,  "0"

[fastclockdisable.reg]
HKR, ,                                  fastClockEnable,                0x00002,  "0"

[paprdenable.reg]
HKR, ,                                  paprdEnable,                    0x00002,  "1"

[MSI.reg]
HKR, "Interrupt Management", 0x00000010
HKR, "Interrupt Management\MessageSignaledInterruptProperties", 0x00000010
HKR, "Interrupt Management\MessageSignaledInterruptProperties", MSISupported, 0x00010001, 1
HKR, "Interrupt Management\MessageSignaledInterruptProperties", MessageNumberLimit, 0x00010001, 4

[9485LnaDivUseBtAntEnable.reg]
HKR, ,                                  lnaDivUseBtAntEnable,           0x00002,  "1"

[antCtrlComm2gSwitchEnable.reg]
HKR, ,                                  antCtrlComm2gSwitchEnable,      0x00010001,  0x000BBB88

[CUS198_xLnaGpioCfg.reg]
HKR, ,                                  extLnaCtlGpio,                  0x00010001,  0x00000200
HKR, ,                                  extAttenMarginCfg,              0x00002,  "1"

[rateCtrlTxFastDrop.reg]
HKR, ,                                  rateCtrlTxFastDrop,             0x00002,  "1"

[led_func0_4.reg]
HKR, ,                                  gpioPinFunc0,                   0x00002,  "4"
HKR, ,                                  gpioFunc0ActHi,                 0x00002,  "0"

[led_func0_10.reg]
HKR, ,                                  gpioPinFunc0,                   0x00002,  "10"
HKR, ,                                  gpioFunc0ActHi,                 0x00002,  "0"
HKR, ,                                  gpioLedCustom,                  0x00002,  "10"
HKR, ,                                  sharedGpioFunc0 ,               0x00002,  "1"
HKR, ,                                  gpioPinFunc1,                   0x00002,  "10"
HKR, ,                                  gpioPinFunc2,                   0x00002,  "10"

[ledcontrol4.reg]
HKR, ,                                  gpioPinFunc0,                   0x00002,  "8"
HKR, ,                                  gpioFunc0ActHi,                 0x00002,  "0"
HKR, ,                                  sharedGpioFunc0,                0x00002,  "1"

[ledcontrol6.reg]
HKR, ,                                  gpioPinFunc0,                   0x00002,  "10"
HKR, ,                                  gpioFunc0ActHi,                 0x00002,  "0"
HKR, ,                                  sharedGpioFunc0,                0x00002,  "1"

[ledcontrol7.reg]
HKR, ,                                  gpioPinFunc0,                   0x00002,  "4"
HKR, ,                                  gpioFunc0ActHi,                 0x00002,  "0"
HKR, ,                                  sharedGpioFunc0,                0x00002,  "1"

[ledcontrol8.reg]
HKR, ,                                  gpioPinFunc0,                   0x00002,  "4"
HKR, ,                                  gpioFunc0ActHi,                 0x00002,  "0"
HKR, ,                                  sharedGpioFunc0,                0x00002,  "1"

[ledcontrol8acthi.reg]
HKR, ,                                  gpioPinFunc0,                   0x00002,  "4"
HKR, ,                                  gpioFunc0ActHi,                 0x00002,  "1"
HKR, ,                                  sharedGpioFunc0,                0x00002,  "1"

[ledcontrol9_blink.reg]
HKR, ,                                  gpioPinFunc0,                   0x00002,  "4"
HKR, ,                                  gpioPinFunc1,                   0x00002,  "4"
HKR, ,                                  gpioFunc0ActHi,                 0x00002,  "0"
HKR, ,                                  sharedGpioFunc0,                0x00002,  "1"
HKR, ,                                  gpioLedCustom,                  0x00002,  "3"

[throughput.reg]
HKR, ,                                  ampTxopLimit,                   0x00002,  "16"
HKR, ,                                  ampIgnoreNonERP,                0x00002,  "1"

[HPheliusda.reg]
HKR, ,                                  btCoexEnable,                   0x00002,  "4"
HKR, ,                                  btCoexAgent,                    0x00002,  "1"
HKR, ,                                  btModule,                       0x00002,  "2"
HKR, ,                                  txCoalescingEnable,             0x00002,  "1"

[AdjustRSSI.reg]
HKR, ,                                  AdjustRSSI,                     0x00002,  "1"

[halShortRetry.reg]
HKR, ,                                  halShortRetry,                  0x00002,  "11"

[IdleConfiguration.reg]
HKR, ,                                  IdleConfiguration,              0x00002,  "0"

[delayNWSleep.reg]
HKR, ,                                  delayNWSleep,                   0x00002,  "1"

[ConnectionFailure.reg]
HKR, ,                                  delayNWSleep,                   0x00002,  "1"
HKR, ,                                  swBeaconProcess,                0x00002,  "1"

[ocsEnable.reg]
HKR, ,                                  ocsEnable,                      0x00002,  "1"

[cemspecled_func0_4.reg]
HKR, ,                                  gpioPinFunc0,                   0x00002,  "4"
HKR, ,                                  gpioLedCustom,                  0x00002,  "3"

[TxPowerSelect.reg]
HKR, Ndi\params\overRideTxPower,        ParamDesc,                      0,  %TxPower%
HKR, Ndi\params\overRideTxPower,        Base,                           0,  "10"
HKR, Ndi\params\overRideTxPower,        default,                        0,  "0"
HKR, Ndi\params\overRideTxPower,        type,                           0,  "enum"
HKR, Ndi\params\overRideTxPower\enum,   "10",                           0,  %TxPowerLowest%
HKR, Ndi\params\overRideTxPower\enum,   "15",                           0,  %TxPowerMediumLow%
HKR, Ndi\params\overRideTxPower\enum,   "20",                           0,  %TxPowerMedium%
HKR, Ndi\params\overRideTxPower\enum,   "25",                           0,  %TxPowerMediumHigh%
HKR, Ndi\params\overRideTxPower\enum,   "0",                            0,  %TxPowerHighest%

[SleepTimePwrSaveMax1000.reg]
HKR, ,                                  SleepTimePwrSaveMax,            0x00002,  "1000"

[SleepTimePwrSaveMax2000.reg]
HKR, ,                                  SleepTimePwrSaveMax,            0x00002,  "2000"

[FilterOutCCK.reg]
HKR, ,                                  FilterOutCCKRateEnable,         0x00002,  "1"

[AphroditeMitiShift.reg]
HKR, ,                                  halMitiShiftValue,             0x10001, 0x00050003

[ledcontrol9.reg]
HKR, ,                                  gpioPinFunc0,                   0x00002,  "1"
HKR, ,                                  gpioPinFunc1,                   0x00002,  "1"
HKR, ,                                  gpioLedCustom,                  0x00002,  "4"

[customer_power.reg]
HKR, ,                                  SleepTimePwrSave,               0x00002,  "1000"
HKR, ,                                  SleepTimePerf,                  0x00002,  "1000"
HKR, ,                                  AwakeTimePwrSaveMax,            0x00002,  "150"
HKR, ,                                  AwakeTimePwrSave,               0x00002,  "150"
HKR, ,                                  periodicScanEnable,             0x00002,  "0"
HKR, ,                                  swBeaconProcess,                0x00002,  "0"

[InvalidRateIgnore.reg]
HKR, ,                                  InvalidRateIgnore,              0x00002,  "1"

[miracast_off.reg]
HKR, ,                                                                  *MiracastSupported,                             0x10001,        0x0

[miracast_scc.reg]
HKR, ,                                  ocsEnable,                		0x00002,  "0"
HKR, ,                                  GoPreferSingle,                	0x00002,  "1"
[miracast_usepass_chl.reg]
HKR, ,                                  p2pUsePassiveChan,                0x00002,   "1"

[cfpignore.reg]
HKR, ,                                  cfpignore,                      0x00002,  "1"

[MAEnable.reg]
HKR, ,                                  smbiosAuthenticationEnable,                      0x00002,  "1"

[forceMaxPowerSave.reg]
HKR, ,                                  maxPowerSave,                   0x00002,  "1"

[WB222SB.reg]
HKR, ,                                  NetBand,                        0x00002,  "26668"

[heavyClipFuncEnable.reg]
HKR, ,                                  heavyClipFuncEnable,            0x00002,  "1"

[paprdDisablePartialTime.reg]
HKR, ,                                  paprdDisablePartialTime,            0x00002,  "1"

[MCCStaTputAdjust.reg] ; EV [141623]
HKR, ,                                  mccStaTimeSlotVovi1,            0x00002,  "35"
HKR, ,                                  pausetimeout,                   0x00002,  "20"

[swBeaconProcess.reg]
HKR, Ndi\params\swBeaconProcess,      ParamDesc,  0,  %swBeaconProcess%
HKR, Ndi\params\swBeaconProcess,      Base,       0,  "10"
HKR, Ndi\params\swBeaconProcess,      default,    0,  "0"
HKR, Ndi\params\swBeaconProcess,      type,       0,  "enum"
HKR, Ndi\params\swBeaconProcess\enum, "1",        0,  %swBeaconProcessEnable%
HKR, Ndi\params\swBeaconProcess\enum, "0",        0,  %swBeaconProcessDisable%

[acerCtlPowerChangeEnable.reg]
HKR, ,                                  acerCtlPowerChangeEnable,            0x00002,  "1"

;;End of Customized Section

[atheros.Service]
DisplayName     = %ATHR.Service.DispName%
ServiceType     = 1         ;SERVICE_KERNEL_DRIVER
StartType       = 3         ;SERVICE_DEMAND_START
ErrorControl    = 1         ;SERVICE_ERROR_NORMAL
ServiceBinary   = %12%\athw10x.sys
LoadOrderGroup  = NDIS

[atheros.EventLog]
AddReg = atheros.AddEventLog.reg

[atheros.AddEventLog.reg]
HKR, , EventMessageFile, 0x00020000, "%%SystemRoot%%\System32\netevent.dll"
HKR, , TypesSupported,   0x00010001, 7


[atheros.CopyFiles]
athw10x.sys,,,2

[SourceDisksNames]
1 = %DiskDescription%,athw10x.sys,,

[SourceDisksFiles]
athw10x.sys = 1,,

[DestinationDirs]
atheros.CopyFiles            = 12
DefaultDestDir               = 11

[Strings]
Msft                         = "Microsoft"
Atheros                      = "Qualcomm Atheros Communications Inc."
Gigabyte                     = "Gigabyte Technology Corp."
ATHR.Service.DispName        = "Qualcomm Atheros Extensible Wireless LAN device driver"
DiskDescription              = "Qualcomm Atheros Sample Driver Disk 1"
TransmitBuffers              = "Transmit Buffers"
ReceiveBuffers               = "Receive Buffers"
scanTimeValid                = "Scan Valid Interval"
shortPreamble                = "802.11b Preamble"
shortPreambleEnable          = "Long and Short"
shortPreambleDisable         = "Long only"
rssiThrHigh                  = "RSSI Threshold"
rssiThrHighNormal            = "Normal"
rssiThrHighMin               = "Min"
;radioEnable                 = "Radio On/Off"
;radioEnableOn               = "On"
;radioEnableOff              = "Off"
scanTime                     = "Roam Time (sec)"
roamRssiA                    = "Roam Time Threshold (db)"
WirelessMode                 = "Wireless Mode Selection"
WirelessMode11bgOnly         = "802.11b/g"
WirelessModeAuto             = "Auto"
PreferredBand                = "Preferred Band"
adhocchannel                 = "Adhoc channel Selection"
bkScanEnable                 = "BackgroundScan On/Off"
bkScanEnableOn               = "On"
bkScanEnableOff              = "Off"
radioEnable                  = "Radio On/Off"
radioEnableOn                = "On"
radioEnableOff               = "Off"
bt30                         = "802.11 Bluetooth High Speed"
bt30enable                   = "Enable"
bt30disable                  = "Disable"
roamRssi11A                  = "roamRssiA"
roamRssi11B                  = "roamRssiB"
roamRssi11BOnly              = "roamRssiBOnly"
roamRateA                    = "roamRateA"
roamRateA6M                  = " 6Mbps"
roamRateA9M                  = " 9Mbps"
roamRateA12M                 = "12Mbps"
roamRateA18M                 = "18Mbps"
roamRateA24M                 = "24Mbps"
roamRateA36M                 = "36Mbps"
roamRateA48M                 = "48Mbps"
roamRateA54M                 = "54Mbps"
roamRateBOnly                = "roamRateBOnly"
roamRateBOnly1M              = " 1Mbps"
roamRateBOnly2M              = " 2Mbps"
roamRateBOnly5M              = " 5Mbps"
roamRateBOnly11M             = "11Mbps"
roamRateB                    = "roamRateB"
roamRateB1M                  = " 1Mbps"
roamRateB2M                  = " 2Mbps"
roamRateB5M                  = " 5Mbps"
roamRateB6M                  = " 6Mbps"
roamRateB9M                  = " 9Mbps"
roamRateB11M                 = "11Mbps"
pcieAspm                     = "pcieAspm"
pcieAspmOff                  = "L0s Off, L1 Off"
pcieAspmL0sOn                = "L0s On,  L1 Off"
pcieAspmL1On                 = "L0s Off, L1 On"
pcieAspmL0sandL1On           = "L0s On,  L1 On"
wModeSelect                  = "Wireless Mode"
wModeSelect11bonly           = "11b only"
wModeSelect11b               = "11b"
wModeSelect11g               = "11g"
wModeSelect11n               = "11n"
wModeSelect11nbg             = "11n(2.4GHz) and g and b"
wModeSelect11na              = "11n(5GHz) and a"
wModeSelect11abgn            = "11abgn"
wModeLegacy11a               = "11a only"
wModeLegacy11bonly           = "11b only"
wModeLegacy11bg              = "11g and 11b"
wModeLegacy11abg             = "11abg"
antennaSwitch                = "AntennaSwitch"
antennaSwitchAuto            = "Auto"
antennaSwitchA               = "Antenna A"
antennaSwitchB               = "Antenna B"
Auto                         = "Auto"
5GOnly                       = "5Ghz Only"
2GOnly                       = "2Ghz Only"
11AOnly                      = "802.11a (5GHz)"
11ANOnly                     = "802.11a/n (5GHz)"
11BGOnly                         = "802.11b/g (2.4GHz)"
11BGNOnly                        = "802.11b/g/n (2.4GHz)"
11ABGN                       = "802.11a/b/g/n (2.4GHz/5GHz)"
11DModeSwitch                = "11d Mode Switch"
Enable                       = "Enable"
Disable                      = "Disable"
WepTkip11n                   = "WepTKIP 11n"
PowerSaveMode                = "Power Save Mode"
Off                          = "Off"
Maximum                      = "Maximum"
Normal                       = "Normal"
802_11d                      = "802.11d"
smpsDynamic                  = "Dynamic MIMO Power Save"
AdHoc11n                     = "AdHoc 11n"
AdhocMode                    = "AdHoc Mode"
roamPolicy                   = "Roaming Policy"
roamPolicyVeryHigh           = "Very High"
roamPolicyHigh               = "High"
roamPolicyNormal             = "Normal"
roamPolicyLow                = "Low"
roamPolicyVeryLow            = "Very Low"
roamPolicyVeryHigh2          = "5.Very High"
roamPolicyHigh2              = "4.High"
roamPolicyNormal2            = "3.Normal"
roamPolicyLow2               = "2.Low"
roamPolicyVeryLow2           = "1.Very Low"
GreenTx                      = "Green Tx"
GreenTxEnableOn              = "On"
GreenTxEnableOff             = "Off"
TxPower                      = "Transmit Power"
TxPowerLowest                = "1.Lowest"
TxPowerMediumLow             = "2.Medium-Low"
TxPowerMedium                = "3.Medium"
TxPowerMediumHigh            = "4.Medium-High"
TxPowerHighest               = "5.Highest"
swBeaconProcess              = "SW Beacon Process"
swBeaconProcessEnable        = "Enable"
swBeaconProcessDisable       = "Disable"
ATHR.DeviceDesc.0013         = "Qualcomm Atheros Wireless Network Adapter"
ATHR.DeviceDesc.001A         = "Qualcomm Atheros AR5005G Wireless Network Adapter"
ATHR.DeviceDesc.001B         = "Qualcomm Atheros AR5006X Wireless Network Adapter"
ATHR.DeviceDesc.1030         = "Qualcomm Atheros AR5002G Wireless Network Adapter"
ATHR.DeviceDesc.2030         = "Qualcomm Atheros AR5002G Wireless Network Adapter"
ATHR.DeviceDesc.1031         = "Qualcomm Atheros AR5002X Wireless Network Adapter"
ATHR.DeviceDesc.2031         = "Qualcomm Atheros AR5002X Wireless Network Adapter"
ATHR.DeviceDesc.1041         = "Qualcomm Atheros AR5004G Wireless Network Adapter"
ATHR.DeviceDesc.2041         = "Qualcomm Atheros AR5004G Wireless Network Adapter"
ATHR.DeviceDesc.1042         = "Qualcomm Atheros AR5004X Wireless Network Adapter"
ATHR.DeviceDesc.2042         = "Qualcomm Atheros AR5004X Wireless Network Adapter"
ATHR.DeviceDesc.1051         = "Qualcomm Atheros AR5005GS Wireless Network Adapter"
ATHR.DeviceDesc.2051         = "Qualcomm Atheros AR5005GS Wireless Network Adapter"
ATHR.DeviceDesc.1053         = "Qualcomm Atheros AR5005GS Wireless Network Adapter"
ATHR.DeviceDesc.2053         = "Qualcomm Atheros AR5005GS Wireless Network Adapter"
ATHR.DeviceDesc.1061         = "Qualcomm Atheros AR5006GS Wireless Network Adapter"
ATHR.DeviceDesc.2061         = "Qualcomm Atheros AR5006GS Wireless Network Adapter"
ATHR.DeviceDesc.1062         = "Qualcomm Atheros AR5006XS Wireless Network Adapter"
ATHR.DeviceDesc.2062         = "Qualcomm Atheros AR5006XS Wireless Network Adapter"
ATHR.DeviceDesc.1065         = "Qualcomm Atheros AR5006G Wireless Network Adapter"
ATHR.DeviceDesc.2065         = "Qualcomm Atheros AR5006G Wireless Network Adapter"
ATHR.DeviceDesc.3061         = "Qualcomm Atheros AR5006EGS Wireless Network Adapter"
ATHR.DeviceDesc.3062         = "Qualcomm Atheros AR5006EXS Wireless Network Adapter"
ATHR.DeviceDesc.3063         = "Qualcomm Atheros AR5006EX Wireless Network Adapter"
ATHR.DeviceDesc.3065         = "Qualcomm Atheros AR5006EG Wireless Network Adapter"
ATHR.DeviceDesc.2055         = "Qualcomm Atheros AR5007G Wireless Network Adapter"
ATHR.DeviceDesc.3067         = "Qualcomm Atheros AR5007EG Wireless Network Adapter"
ATHR.DeviceDesc.1071         = "Qualcomm Atheros AR5008 Wireless Network Adapter"
ATHR.DeviceDesc.3072         = "Qualcomm Atheros AR5008X Wireless Network Adapter"
ATHR.DeviceDesc.3091         = "Qualcomm Atheros AR928X Wireless Network Adapter"
ATHR.DeviceDesc.2091         = "Qualcomm Atheros AR922X Wireless Network Adapter"
ATHR.DeviceDesc.30A1         = "Qualcomm Atheros AR9285 Wireless Network Adapter"
ATHR.DeviceDesc.30ABLT       = "Qualcomm Atheros AR9002WB-1NG Wireless Network Adapter"
ATHR.DeviceDesc.30AB         = "Qualcomm Atheros AR9002WB-1NG Wireless Network Adapter #1"
ATHR.DeviceDesc.30AD         = "Qualcomm Atheros AR9002WB-1NG Wireless Network Adapter #2"
ATHR.DeviceDesc.2A371A3B     = "Qualcomm Atheros AR9002WB Wireless Network Adapter"
ATHR.DeviceDesc.30AE         = "Qualcomm Atheros AR5008WB-EG Wireless Network Adapter #1"
ATHR.DeviceDesc.30AF         = "Qualcomm Atheros AR5008WB-EG Wireless Network Adapter #2"
ATHR.DeviceDesc.30A7         = "Qualcomm Atheros AR2427 Wireless Network Adapter"
ATHR.DeviceDesc.10CF         = "IEEE 802.11a/g Wireless LAN Adapter (A)"
ATHR.DeviceDesc.1737_g       = "Linksys Wireless-G Notebook Adapter"
ATHR.DeviceDesc.1737_bg      = "Linksys Wireless A+G Notebook Adapter"
ATHR.DeviceDesc.1737_abg     = "Linksys Wireless A+G PCI Adapter"
ATHR.DeviceDesc.0044         = "Linksys Dual-Band Wireless A+G PCI Adapter"
ATHR.DeviceDesc.1013         = "11b/g Wireless LAN Mini PCI Adapter"
ATHR.DeviceDesc.2013         = "11a/b/g Wireless LAN Mini PCI Adapter II" 
ATHR.DeviceDesc.3013         = "11b/g Wireless LAN Mini PCI Express Adapter"
ATHR.DeviceDesc.4013         = "11a/b/g Wireless LAN Mini PCI Express Adapter"
ATHR.DeviceDesc.5013         = "11b/g Wireless LAN Mini PCI Express Adapter II"
ATHR.DeviceDesc.6013         = "11b/g Wireless LAN Mini PCI Express Adapter III"
ATHR.DeviceDesc.0032168c     = "11b/g/n Wireless LAN Mini-PCI Express Adapter"
ATHR.DeviceDesc.0033168c     = "11a/b/g/n Wireless LAN Mini-PCI Express Adapter"
ATHR.DeviceDesc.90001385     = "NETGEAR WN711 RangeMax Wireless-N Expresscard Adapter"
ATHR.DeviceDesc.4B001385     = "NETGEAR 108 Mbps Wireless PC Card WG511T"
ATHR.DeviceDesc.5D001385     = "NETGEAR RangeMax(TM) Wireless PC Card WPN511"
ATHR.DeviceDesc.4D001385     = "NETGEAR 108 Mbps Wireless PCI Adapter WG311T"
ATHR.DeviceDesc.4F001385     = "NETGEAR Double 108 Mbps Wireless PC Card WG511U"
ATHR.DeviceDesc.04061468     = "LAN-Express AS IEEE 802.11g miniPCI Adapter"
ATHR.DeviceDesc.04071468     = "LAN-Express AS IEEE 802.11a/g miniPCI Adapter"
ATHR.DeviceDesc.04231468     = "LAN-Express AS IEEE 802.11g PCI-E Adapter"
ATHR.DeviceDesc.F6D3000      = "Belkin Wireless A/G Desktop Network Card"
ATHR.DeviceDesc.80111799     = "Belkin N1 Wireless Notebook Card"
ATHR.DeviceDesc.G650         = "D-Link AirPlus DWL-G650 Wireless Cardbus Adapter(rev.C)"
ATHR.DeviceDesc.G520X        = "D-Link AirPlus Xtreme G DWL-G520 Adapter"
ATHR.DeviceDesc.G520         = "D-Link AirPlus DWL-G520 Wireless PCI Adapter(rev.B)"
ATHR.DeviceDesc.AG520        = "D-Link AirXpert DWL-AG520 Wireless PCI Adapter"
ATHR.DeviceDesc.AG530        = "D-Link AirPremier DWL-AG530 Wireless PCI Adapter"
ATHR.DeviceDesc.G630         = "D-Link AirPlus G DWL-G630 Wireless Cardbus Adapter(rev.D)"
ATHR.DeviceDesc.G510         = "D-Link AirPlus G DWL-G510 Wireless PCI Adapter(rev.B)"
ATHR.DeviceDesc.AG650        = "D-Link AirXpert DWL-AG650 Wireless Cardbus Adapter"
ATHR.DeviceDesc.AG660        = "D-Link AirPremier DWL-AG660 Wireless Cardbus Adapter"
ATHR.DeviceDesc.G680         = "D-Link AirPremier DWL-G680 Wireless Cardbus Adapter"
ATHR.DeviceDesc.G550         = "D-Link AirPremier DWL-G550 Wireless PCI Adapter"
ATHR.DeviceDesc.AG660B       = "D-Link AirPremier AG DWL-AG660 Wireless Cardbus Adapter"
ATHR.DeviceDesc.AG530B       = "D-Link AirPremier AG DWL-AG530 Wireless PCI Adapter"
ATHR.DeviceDesc.G650P        = "D-Link AirPlus G DWL-G650+A Wireless Cardbus Adapter"
ATHR.DeviceDesc.G520P        = "D-Link AirPlus G DWL-G520+A Wireless PCI Adapter"
ATHR.DeviceDesc.WDA1320      = "D-Link WDA-1320 Desktop Adapter"
ATHR.DeviceDesc.WDA2320      = "D-Link WDA-2320 Desktop Adapter"
ATHR.DeviceDesc.DWA520       = "D-Link Wireless 108G DWA-520 Desktop Adapter"
ATHR.DeviceDesc.DWA620       = "D-Link Wireless 108G DWA-620 Notebook Adapter"
ATHR.DeviceDesc.CWNA2330     = "D-Link WNA-2330 Notebook Adapter"
ATHR.DeviceDesc.CWNA1330     = "D-Link WNA-1330 Notebook Adapter"
ATHR.DeviceDesc.CG650        = "D-Link AirPlus Xtreme G DWL-G650 Adapter"
ATHR.DeviceDesc.CG630        = "D-Link AirPlus G DWL-G630 Wireless Cardbus Adapter"
ATHR.DeviceDesc.DWA642       = "D-Link DWA-642 RangeBooster N Notebook Adapter"
ATHR.DeviceDesc.DWA645       = "D-Link DWA-645 RangeBooster N650 Notebook Adapter"
ATHR.DeviceDesc.DWA542       = "D-Link DWA-542 RangeBooster N Desktop Adapter"
ATHR.DeviceDesc.DWA547       = "D-Link DWA-547 RangeBooster N650 Desktop Adapter"
ATHR.DeviceDesc.DWA652       = "D-Link DWA-652 XtremeN Notebook Adapter"
ATHR.DeviceDesc.DWA552       = "D-Link DWA-552 XtremeN Desktop Adapter"
ATHR.DeviceDesc.DWA643       = "D-Link DWA-643 Xtreme N ExpressCard Notebook Adapter"
ATHR.DeviceDesc.DWA556       = "D-Link DWA-556 Xtreme N PCIe Desktop Adapter"
ATHR.DeviceDesc.3070         = "Gigaset PC Card 108"
ATHR.DeviceDesc.3071         = "Speedport Gigaset 54 Mbit"
ATHR.DeviceDesc.800118CB     = "Gigaset PC Card 300"
ATIWC.DeviceDesc.ATICB       = "Allied Telesyn AT-WCC201g Wireless Card Bus Adapter"
ATIWC.DeviceDesc.ATIPC       = "Allied Telesyn AT-WCP201g Wireless PCI Adapter"
ATHR.DeviceDesc.2A5F103C     = "Foxconn 802.11 a/b/g/n Wireless System Adaptor"
ATHR.DeviceDesc.500011AD     = "HP 802.11a/b/g Wireless Network Adapter"
ATHR.DeviceDesc.500111AD     = "HP 802.11b/g Wireless Network Adapter"
ATHR.DeviceDesc.1000168c     = "Qualcomm Atheros 802.11 a/b/g/n Dualband Wireless Network Module"
GIGA.DeviceDesc.E914         = "Gigabyte GN-WI03N (mini) PCI WLAN Card"
GIGA.DeviceDesc.E915         = "Gigabyte GN-WP02N PCI Express WLAN Card"
GIGA.DeviceDesc.E916         = "Gigabyte GN-WI06N (mini) PCI Express WLAN Card"
GIGA.DeviceDesc.E815         = "Gigabyte GN-WM02N Express WLAN Card"
GIGA.DeviceDesc.E801         = "Gigabyte GN-WLMA102 Cardbus WLAN Card"
GIGA.DeviceDesc.E811         = "Gigabyte GN-WMAG Cardbus WLAN Card"
GIGA.DeviceDesc.E814         = "Gigabyte GN-WM01GT Cardbus WLAN Card"
GIGA.DeviceDesc.0013         = "Gigabyte GN-WIAH (mini) PCI WLAN Card"
GIGA.DeviceDesc.E901         = "Gigabyte GN-WI01HT (mini) PCI WLAN Card"
GIGA.DeviceDesc.E911         = "Gigabyte GN-WIAG/GN-WPEAG (mini) PCI WLAN Card"
GIGA.DeviceDesc.E912         = "Gigabyte GN-WP01GT (mini) PCI WLAN Card"
GIGA.DeviceDesc.E913         = "Gigabyte GN-WI01GT (mini) PCI-E WLAN Card"
GIGA.DeviceDesc.E917         = "Gigabyte GN-WI07HT (mini) PCI-E WLAN Card"
GIGA.DeviceDesc.E918         = "Gigabyte GN-WS50G (mini) PCI-E WLAN Card"
GIGA.DeviceDesc.E9191458     = "Gigabyte GN-WS53HN Wireless LAN Mini PCI Express Adapter"
ATHR.DeviceDesc.7141144F     = "Qualcomm Atheros AR9281 Wireless Network Adapter"
ATHR.DeviceDesc.7136144F     = "Qualcomm Atheros AR9280 Wireless Network Adapter"
ATHR.DeviceDesc.E006105B     = "Qualcomm Atheros AR5B91 Wireless Network Adapter"
ATHR.DeviceDesc.655211AD     = "Qualcomm Atheros AR5B92 Wireless Network Adapter"
ATHR.DeviceDesc.CM9          = "WNC CM9 Wireless LAN mini-PCI Network Adapter"
ATHR.DeviceDesc.1ACE         = "TP-LINK Wireless N Adapter"
ATHR.DeviceDesc.00341B0A     = "Qualcomm Atheros AR9281 802.11b/g/n WLAN HMC Network"
ATHR.DeviceDesc.2063         = "Qualcomm Atheros AR5006 802.11a/b/g WiFi Adapter"
ATHR.DeviceDesc.3096         = "Qualcomm Atheros AR5009 802.11a/g/n WiFi Adapter"
ATHR.DeviceDesc.5E001385     = "NETGEAR WPN311 RangeMax(TM) Wireless PCI Adapter"
ATHR.DeviceDesc.0036         = "11b/g/n Wireless LAN Mini-PCI Express Adapter II"
ATHR.DeviceDesc.0037         = "11b/g/n Wireless LAN Mini-PCI Express Adapter III"
ATHR.DeviceDesc.309917AA     = "11a/b/g/n Wireless LAN Adapter"
ATHR.DeviceDesc.7163144F     = "Qualcomm Atheros AR9283 Wireless Network Adapter"
ATHR.DeviceDesc.E01F105B     = "Qualcomm Atheros AR5B93 Wireless Network Adapter"
ATHR.DeviceDesc.663111AD     = "Qualcomm Atheros AR5B95 Wireless Network Adapter"
ATHR.DeviceDesc.660311AD     = "Qualcomm Atheros AR5B97 Wireless Network Adapter"
ATHR.DeviceDesc.661711AD     = "Qualcomm Atheros AR5B125 Wireless Network Adapter"
ATHR.DeviceDesc.E04A105B     = "Qualcomm Atheros AR5B116 Wireless Network Adapter"
ATHR.DeviceDesc.661811AD     = "Qualcomm Atheros AR5BWB225 Wireless Network Adapter"
ATHR.DeviceDesc.E051105B     = "Qualcomm Atheros AR5BMD225 Wireless Network Adapter"
ATHR.DeviceDesc.311711AD     = "Qualcomm Atheros AR5BWB222 Wireless Network Adapter"
ATHR.DeviceDesc.E059105B     = "Qualcomm Atheros AR5BMD222 Wireless Network Adapter"
ATHR.DeviceDesc.E086105B     = "Qualcomm Atheros AR5BNFA222 Wireless Network Adapter"
ATHR.DeviceDesc.30A4         = "Qualcomm Atheros AR9287 Wireless Network Adapter"
ATHR.DeviceDesc.2099         = "Qualcomm Atheros AR9227 Wireless Network Adapter"
ATHR.DeviceDesc.D05B10FC     = "I-O DATA WHG-AGDN/CB Wireless LAN Adapter"
ATHR.DeviceDesc.30B0         = "Qualcomm Atheros AR9002WB-2NG Wireless Network Adapter"
ATHR.DeviceDesc.ospsim       = "Qualcomm Atheros Osprey Simulation Wireless Network Adapter"
ATHR.DeviceDesc.ospemu       = "Qualcomm Atheros Osprey Emulation Wireless Network Adapter"
ATHR.DeviceDesc.osprey       = "Qualcomm Atheros Osprey Wireless Network Adapter"
ATHR.DeviceDesc.938x         = "Qualcomm Atheros AR938x Wireless Network Adapter"
ATHR.DeviceDesc.9485         = "Qualcomm Atheros AR9485 Wireless Network Adapter"
ATHR.DeviceDesc.1111         = "Qualcomm Atheros AR1111 Wireless Network Adapter"
ATHR.DeviceDesc.9580         = "Qualcomm Atheros AR9580 Wireless Network Adapter"
ATHR.DeviceDesc.3119         = "Qualcomm Atheros AR9485WB-EG Wireless Network Adapter"
ATHR.DeviceDesc.D3067        = "Qualcomm Atheros AR5007 802.11b/g WiFi Adapter"
ATHR.DeviceDesc.D30A1        = "Qualcomm Atheros AR9285 802.11b/g/n WiFi Adapter"
ATHR.DeviceDesc.D30AB        = "Qualcomm Atheros AR9285 802.11b/g/n WiFi Adapter"
ATHR.DeviceDesc.0300T        = "TP-LINK 300Mbps Wireless N Adapter"
ATHR.DeviceDesc.0301T        = "TP-LINK 150Mbps Wireless N Adapter"
ATHR.DeviceDesc.3B001106     = "VIA 802.11b/g/n PCIe Wireless Network Adapter"
ATHR.DeviceDesc.00231931     = "Option GTM67x PCIe WiFi Adapter"
ATHR.DeviceDesc.11951A3B     = "Qualcomm Atheros AR1111 Wireless Network Adapter"
ATHR.DeviceDesc.21001A3B     = "Qualcomm Atheros AR1111 WB-EG Wireless Network Adapter"
ATHR.DeviceDesc.H3067        = "Qualcomm Atheros AR5007 802.11b/g WiFi Adapter"
ATHR.DeviceDesc.H2063        = "Qualcomm Atheros AR5006 802.11a/b/g WiFi Adapter"
ATHR.DeviceDesc.H3096        = "Qualcomm Atheros AR5009 802.11a/g/n WiFi Adapter"
ATHR.DeviceDesc.H30A1        = "Qualcomm Atheros AR9285 802.11b/g/n WiFi Adapter"
ATHR.DeviceDesc.H30AB        = "Qualcomm Atheros AR9285 802.11b/g/n WiFi Adapter"
ATHR.DeviceDesc.H30A4        = "Qualcomm Atheros AR9287 802.11b/g/n WiFi Adapter"
ATHR.DeviceDesc.H3197        = "Qualcomm Atheros AR9287 802.11b/g/n WiFi Adapter"
ATHR.DeviceDesc.H3116        = "Qualcomm Atheros AR9382 802.11a/g/n WiFi Adapter"
ATHR.DeviceDesc.H3112        = "Qualcomm Atheros AR9380 802.11a/g/n WiFi Adapter"
ATHR.DeviceDesc.H3119        = "Qualcomm Atheros AR9485 802.11b/g/n WiFi Adapter"
ATHR.DeviceDesc.H3118        = "Qualcomm Atheros AR9485 802.11b/g/n WiFi Adapter"
ATHR.DeviceDesc.946x         = "Qualcomm Atheros AR946x Wireless Network Adapter"
ATHR.DeviceDesc.H3335        = "Qualcomm Atheros AR9462 802.11a/b/g/n WiFi Adapter"
ATHR.DeviceDesc.956x         = "Qualcomm Atheros AR956x Wireless Network Adapter"
ATHR.DeviceDesc.H9565        = "Qualcomm Atheros QCA9565 802.11b/g/n WiFi Adapter"
ATHR.DeviceDesc.E031105B     = "Qualcomm Atheros AR5B195 Wireless Network Adapter"
ATHR.DeviceDesc.E068105B     = "Qualcomm Atheros AR956x Wireless Network Adapter"
ATHR.DeviceDesc.302617AA     = "Qualcomm Atheros AR956x Wireless Network Adapter"
ATHR.DeviceDesc.DWA566       = "D-Link DWA-566 Wireless N 300 Dual Band PCIe Desktop Adapter"
ATHR.DeviceDesc.TEW726       = "TRENDnet N600 Wireless Dual Band PCIe Adapter"
ATHR.DeviceDesc.k1102        = "Killer Wireless-N 1102 Network Adapter"
ATHR.DeviceDesc.k1103        = "Killer Wireless-N 1103 Network Adapter"
ATHR.DeviceDesc.k1202        = "Killer Wireless-N 1202 Network Adapter"


;/* Enable these if VLAN or 802.1p is to be enabled */
;PriorityVLAN                = "Priority & VLAN"
;PriorityVLANDisabled        = "Priority & VLAN Disabled"
;PriorityEnabled             = "Priority Enabled"
;VLANEnabled                 = "VLAN Enabled"
;PriorityVLANEnabled         = "Priority & VLAN Enabled"
